DCbus Source
Performs a DCbus voltage source
Library
GMCLIB
Description
Performs a voltage behind a Graetz bridge rectifier stabilized with a capacity. The capacity discharging happens according to:
For constant DCbus current consumption the voltage has a well known course:
Parameters and dialog box
The block dialog box appears as follows:
Umax - DCbus amplitude [V]
f_DCbus - DCbus frequency [Hz]
Cout - output capacity [F]
Inputs and outputs
Inputs:
I in - total current consumtion from DCbus [A] (can be obtained: )
Outputs:
U out - DCbus output voltage [V]