<?xml version="1.0" ?>
<nidocument>
<nicomment>
<nifamily displayname="Spectral Measurement Toolset" familyname="Spectral Measurement Toolset"/>
</nicomment>
<nierror code="-20501">
Spectral Measurements: The specified zoom factor must be greater than 0.
</nierror>
<nierror code="-20502">
Spectral Measurements: The specified FFT size must be greater than 0.
</nierror>
<nierror code="-20503">
Spectral Measurements: The input data overflows the internal buffer.
</nierror>
<nierror code="-20504">
Spectral Measurements: The specified sampling frequency must be greater than 0.
</nierror>
<nierror code="-20505">
Spectral Measurements: Either the number of FFT bins or the resolution bandwidth must be specified.
</nierror>
<nierror code="-20506">
Spectral Measurements: The input spectrum data is of an incorrect type.
</nierror>
<nierror code="-20507">
Spectral Measurements: Incorrect averaging type specified.
</nierror>
<nierror code="-20508">
Invalid SMT session handle.
</nierror>
<nierror code="-20509">
Error Loading DLL (DLL not in path?)
</nierror>
<nierror code="-20510">
Function not found in DLL (invalid DLL version?)
</nierror>
<nierror code="-20511">
Could not create required mutex.
</nierror>
<nierror code="-20512">
Spectral Measurements: Either RBW, time, or span must be specified.
</nierror>
<nierror code="-20513">
Spectral Measurements: The specified band does not match the spectra. The band specification chosen might be outside the band  chosen using spectrum settings.
</nierror>
<nierror code="-20514">
Spectral Measurements: This hardware cannot be configured using this VI. Refer to the SMT examples for this hardware.
</nierror>
<nierror code="-20515">
Spectral Measurements: RBW or Spectral Lines value not supported.
</nierror>
<nierror code="-20516">
Spectral Measurements: Input parameter out of range.
</nierror>
<nierror code="-20517">
Spectral Measurements: Spectral Measurement Toolkit does not support this hardware.
</nierror>
<nierror code="-20518">
If pulse shaping filter type is not set to None, the filter parameter cannot be less than 0.1 or higher than 0.9.
</nierror>
<nierror code="-20519">
Spectral Measurements: Value of dt should be more than 1ps and less than 1Ts.
</nierror>
<nierror code="-20520">
Spectral Measurements: value of span should lie between 1pHz and 1THz .
</nierror>
<nierror code="-20521">
Resolution bandwidth (RBW) should be less than span.
</nierror>
<nierror code="20501">
Spectral Measurements: The specified VI is not supported by this version of the SMT.
</nierror>
</nidocument>
