<?XML Version="1.0">
<nidocument>
<nicomment>
<nifamily familyname="Time Frequency Analysis Toolkit" displayname="Time Frequency Analysis Toolkit">
</nifamily>
</nicomment>
<nierror code="-42619">
Time Frequency Analysis Toolkit:  The parameters of the transform info input or the expansion info input are invalid for further computation.
</nierror>
<nierror code="-42618">
Time Frequency Analysis Toolkit:  The row size of the kernel must be a power of 2 and greater than 0. The column size of the kernel must be 2^(ceil(log2(Ls-1))), where Ls is the length of the input signal.
</nierror>
<nierror code="-42615">
Time Frequency Analysis Toolkit:  The number of terms input must be greater than 0.
</nierror>
<nierror code="-42614">
Time Frequency Analysis Toolkit:  The oversampling rate, N/dM, must be greater than or equal to 1.
</nierror>
<nierror code="-42606">
Time Frequency Analysis Toolkit:  This file operation does not support the LabVIEW Real-Time Module.
</nierror>
<nierror code="-42605">
Time Frequency Analysis Toolkit:  The size of the color table must equal 256.
</nierror>
<nierror code="-42601">
Time Frequency Analysis Toolkit:  The input signal is empty, or the signal length is less than the window length.
</nierror>
<nierror code="42602">
Time Frequency Analysis Toolkit:  The sampling rate must be greater than 0.
</nierror>
<nierror code="42603">
Time Frequency Analysis Toolkit:  The frequency bins must be a power of 2 and greater than 0.
</nierror>
<nierror code="42611">
Time Frequency Analysis Toolkit:  The time steps must be greater than 0. 
</nierror>
<nierror code="42613">
Time Frequency Analysis Toolkit:  The order must be greater than or equal to 0.
</nierror>
<nierror code="42614">
Time Frequency Analysis Toolkit:  The oversampling rate, N/dM, must be greater than or equal to 1.
</nierror>
<nierror code="42616">
Time Frequency Analysis Toolkit:  The size of the window must be greater than 0.
</nierror>
<nierror code="42617">
Time Frequency Analysis Toolkit:  The variance of the Gaussian window must be greater than 0.
</nierror>
<nierror code="42618">
Time Frequency Analysis Toolkit:  The Gaussian window length must be a power of 2 and greater than or equal to 8.
</nierror>
<nierror code="42619">
Time Frequency Analysis Toolkit:  The alpha must be greater than or equal to 0.
</nierror>
</nidocument>