Par Statistics
Total Non-vccgnd Signals=498
Total Non-vccgnd Design Pins=926
Total Non-vccgnd Conns=926
Total Non-vccgnd Timing Constrained Conns=868
Phase 1 CPU=9.7 sec
Phase 2 CPU=11.5 sec
Phase 3 CPU=12.2 sec
Phase 4 CPU=14.8 sec
Phase 5 CPU=15.3 sec
Phase 6 CPU=15.3 sec
Phase 7 CPU=15.3 sec
Phase 8 CPU=15.3 sec
Phase 9 CPU=15.4 sec
Phase 10 CPU=15.4 sec
AvgWirelenPerPin Fanout 1=1.0
AvgWirelenPerPin Fanout 2=2.0
AvgWirelenPerPin Fanout 3=4.0
AvgWirelenPerPin Fanout 4=3.0
AvgWirelenPerPin Fanout 10=3.3
AvgWirelenPerPin Fanout 50=3.5
AvgWirelenPerPin Fanout 100=0.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0232