# Processing Summary
# Terasa_GPS_Tuhá

##
Project Information

Project name: | Terasa_GPS_Tuhá
Date created: | 04/12/2017 15:28:12
Time zone: | 0h 00'
Coordinate system name: | CZ_JT13
Application software: | LEICA Geo Office 8.2
Start date and time: | 06/30/2016 07:25:28
End date and time: | 06/30/2016 12:04:53
Manually occupied points: | 9
Processing kernel: | PSI-Pro 3.0
Processed: | 04/12/2017 15:39:52

##
Processing Parameters

Parameters | Selected
--- | ---
Cut-off angle: | 15°
Ephemeris type: | Broadcast
Solution type: | Automatic
GNSS type: | Automatic
Frequency: | Automatic
Fix ambiguities up to: | 80 km
Min. duration for float solution (static): | 5' 00"
Sampling rate: | Use all
Tropospheric model: | Hopfield
Ionospheric model: | Automatic
Use stochastic modelling: | Yes
Min. distance: | 8 km
Ionospheric activity: | Automatic

##
Baseline Overview

Virtual Rinex - R2 | Reference: Virtual Rinex | Rover: R2
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599069.1760 m
| Northing: | 1164502.4303 m | 1159480.7757 m
| Ortho. Hgt: | 235.3634 m | 275.6038 m
Solution type: | Float
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | No

Virtual Rinex - JV | Reference: Virtual Rinex | Rover: JV
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599123.7786 m
| Northing: | 1164502.4303 m | 1159446.2143 m
| Ortho. Hgt: | 235.3634 m | 277.3624 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes

Virtual Rinex - JZ | Reference: Virtual Rinex | Rover: JZ
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599131.6203 m
| Northing: | 1164502.4303 m | 1159450.8058 m
| Ortho. Hgt: | 235.3634 m | 277.3651 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes

Virtual Rinex - 2 | Reference: Virtual Rinex | Rover: 2
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599134.8806 m
| Northing: | 1164502.4303 m | 1159444.0917 m
| Ortho. Hgt: | 235.3634 m | 277.5957 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes

Virtual Rinex - 5 | Reference: Virtual Rinex | Rover: 5
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599128.0314 m
| Northing: | 1164502.4303 m | 1159440.1030 m
| Ortho. Hgt: | 235.3634 m | 277.5877 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes

Virtual Rinex - 6 | Reference: Virtual Rinex | Rover: 6
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599145.9139 m
| Northing: | 1164502.4303 m | 1159431.5419 m
| Ortho. Hgt: | 235.3634 m | 277.6023 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes

Virtual Rinex - 7 | Reference: Virtual Rinex | Rover: 7
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599148.0039 m
| Northing: | 1164502.4303 m | 1159427.9885 m
| Ortho. Hgt: | 235.3634 m | 277.6201 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes

Virtual Rinex - 9 | Reference: Virtual Rinex | Rover: 9
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599147.9870 m
| Northing: | 1164502.4303 m | 1159419.4487 m
| Ortho. Hgt: | 235.3634 m | 277.3357 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes

Virtual Rinex - 10 | Reference: Virtual Rinex | Rover: 10
--- | --- | ---
Coordinates: |  |
| Easting: | 599178.8430 m | 599142.9064 m
| Northing: | 1164502.4303 m | 1159416.5105 m
| Ortho. Hgt: | 235.3634 m | 277.3406 m
Solution type: | Phase: all fix
GNSS type: | GPS / GLONASS
Frequency: | L1/E1 and L2
Ambiguity: | Yes