temperature = 23 °C

log number -> info
486cmRTS
1 ->	wider start, W32TM stopped after RPi, data GOOD
2 ->	wider start, W32TM stopped after RPi, droput at beginning, big jump in results, at least one wrong GPIO state detected, data BAD
3 ->	wider start, W32TM stopped after RPi, big jump in results, at least one wrong GPIO state detected, data BAD
4 ->	wider start, W32TM stopped after RPi, data GOOD
5 ->	wider start, W32TM stopped after RPi, several big jumps in results, at least one wrong GPIO state detected, data BAD
6 ->	narrower start, W32TM stopped after RPi, big jump in results at the end, otherwise OK
7 ->	narrower start, W32TM stopped after RPi, data GOOD
8 ->	narrower start, big jump in results after first point, at least one wrong GPIO state detected, data BAD
9 ->	narrower start, TSC7 data overwritten, other data GOOD
10 ->	wider start, data GOOD
486cmRTS static
1 ->	prism not moving, done right after station setup
266cmRTS
1 ->	wider start, data GOOD
2 ->	wider start, small droput at beginning - 1 pass missed, otherwise OK
3 ->	wider start, small droput at beginning - 1 pass missed, otherwise OK
4 ->	wider start, data GOOD
5 ->	wider start, small droput at beginning - 1 pass missed, otherwise OK
6 ->	narrower start, data GOOD
7 ->	narrower start, big jump in results, data BAD
8 ->	narrower start, data GOOD
9 ->	narrower start, data GOOD
