log number -> info
1 ->	first measurement, original settings
2 ->	second measurement, original settings
3 ->	third measurement, original settings
4 ->	without parallel logging in windows in TSC7 controller, probably original settings
5 ->	had a significant sync dropout during the measurement, probably original settings
6 ->	had perfect sync (probably) the whole time during the experiment, probably original settings
7 ->	W32TM state request rate in windows in TSC7 controller set to 4 seconds
8 ->	W32TM state request rate in windows in TSC7 controller set to 4 seconds, had perfect sync (probably) the whole time during the experiment
9 ->	W32TM state request rate in windows in TSC7 controller set to 4 seconds, some dropouts at the end of measurement
10 ->	W32TM state request not used windows in TSC7 controller during measurement
11 ->	W32TM state request not used windows in TSC7 controller during measurement
12 ->	W32TM state request not used windows in TSC7 controller during measurement
13 ->	no printing to console in Raspberry Pi program during measurement
14 ->	Microsoft provided PTP configuration settings used, a large amount of dropouts during measurement
15 ->	starting measurement from widest possible angle, probably 4 second W32TM state request
16 ->	starting measurement from widest possible angle, probably 4 second W32TM state request
17 ->	starting measurement from widest possible angle, probably 4 second W32TM state request
18 ->	starting measurement from widest possible angle, probably 4 second W32TM state request
19 ->	starting measurement from widest possible angle, probably 4 second W32TM state request
20 ->	starting measurement from widest possible angle, probably 4 second W32TM state request
21 ->	RTS position changed to be closer to pendulum, probably 4 second W32TM state request
22 ->	RTS position changed to be closer to pendulum, probably 4 second W32TM state request
23 ->	RTS position changed to be closer to pendulum, probably 4 second W32TM state request
24 ->	RTS position changed to be closer to pendulum, probably 4 second W32TM state request
25 ->	RTS position changed to be closer to pendulum, probably 4 second W32TM state request
