# Static Call Graph for image .\Targets\Nucleo_F411_ext_8MHz\project.axf

#<CALLGRAPH># ARM Linker, 5050106: Last Updated: Sat Mar 14 00:31:10 2015

### Maximum Stack Usage = 68 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ TM_DISCO_LedInit ⇒ TM_GPIO_Init ⇒ GPIO_Init

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - FPU_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RCC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - Reset_Handler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SPI5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f411xe.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM3_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM4_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - TIM5_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART1_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART2_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - USART6_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f411xe.o(.text) referenced from startup_stm32f411xe.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f411xe.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f411xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  RCC_DeInit (Thumb, 68 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_DELAY_Init

  RCC_GetFlagStatus (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 44 bytes, Stack size 12 bytes, stm32f4xx_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> TM_DELAY_Init

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAIConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 134 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockACLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockBCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLI2SClkDivConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLSAIClkDivConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LTDCCLKDivConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_TIMCLKPresConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEModeConfig (Thumb, 68 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 216 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 120 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> TM_GPIO_DeInit
  - >> TM_GPIO_InitAlternate
  - >> TM_GPIO_Init

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Called By]

  - >> TM_GPIO_InitAlternate

  TimingDelay_Decrement (Thumb, 26 bytes, Stack size 8 bytes, tm_stm32f4_delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TimingDelay_Decrement
  [Called By]
  - >> SysTick_Handler

  TM_DELAY_Init (Thumb, 82 bytes, Stack size 8 bytes, tm_stm32f4_delay.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TM_DELAY_Init ⇒ RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_WaitForHSEStartUp
  - >> RCC_HSEConfig
  [Called By]
  - >> main

  TM_DELAY_EnableDelayTimer (Thumb, 22 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_DELAY_DisableDelayTimer (Thumb, 14 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_DISCO_LedInit (Thumb, 24 bytes, Stack size 16 bytes, tm_stm32f4_disco.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = TM_DISCO_LedInit ⇒ TM_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> TM_GPIO_Init
  [Called By]
  - >> main

  TM_DISCO_ButtonInit (Thumb, 24 bytes, Stack size 16 bytes, tm_stm32f4_disco.o(.text), UNUSED)
  [Calls]

  - >> TM_GPIO_Init

  TM_DISCO_ButtonOnPressed (Thumb, 32 bytes, Stack size 0 bytes, tm_stm32f4_disco.o(.text), UNUSED)

  TM_DISCO_ButtonOnReleased (Thumb, 32 bytes, Stack size 0 bytes, tm_stm32f4_disco.o(.text), UNUSED)

  TM_GPIO_Init (Thumb, 52 bytes, Stack size 32 bytes, tm_stm32f4_gpio.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = TM_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> TM_GPIO_INT_EnableClock
  - >> GPIO_Init
  [Called By]
  - >> TM_DISCO_ButtonInit
  - >> TM_DISCO_LedInit

  TM_GPIO_InitAlternate (Thumb, 96 bytes, Stack size 40 bytes, tm_stm32f4_gpio.o(.text), UNUSED)
  [Calls]

  - >> TM_GPIO_INT_EnableClock
  - >> GPIO_PinAFConfig
  - >> GPIO_Init

  TM_GPIO_DeInit (Thumb, 22 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Init

  TM_GPIO_SetPinAsInput (Thumb, 40 bytes, Stack size 16 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPinAsOutput (Thumb, 46 bytes, Stack size 20 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_GetPortSource (Thumb, 86 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_GetPinSource (Thumb, 18 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_INT_DisableClock (Thumb, 158 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  main (Thumb, 46 bytes, Stack size 0 bytes, main.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = main ⇒ TM_DISCO_LedInit ⇒ TM_GPIO_Init ⇒ GPIO_Init
  [Calls]
  - >> Delayms
  - >> TM_DISCO_LedInit
  - >> TM_DELAY_Init
  - >> SystemInit
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f411xe.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ TimingDelay_Decrement
  [Calls]
  - >> TimingDelay_Decrement
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(RESET)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SystemInit
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - startup_stm32f411xe.o(.text)

  SystemCoreClockUpdate (Thumb, 102 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  TM_GPIO_INT_EnableClock (Thumb, 158 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text))
  [Called By]

  - >> TM_GPIO_InitAlternate
  - >> TM_GPIO_Init

  Delayms (Thumb, 20 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Delayms
  [Called By]
  - >> main

  SetSysClock (Thumb, 100 bytes, Stack size 0 bytes, system_stm32f4xx.o(.text))
  [Called By]

  - >> SystemInit

  ### Undefined Global Symbols