# Static Call Graph for image .\Targets\STM32F429_Discovery\project.axf

#<CALLGRAPH># ARM Linker, 5050106: Last Updated: Fri May 15 14:44:54 2015

### Maximum Stack Usage = 188 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ TM_ILI9341_Init ⇒ TM_SPI_Init ⇒ TM_SPIx_Init ⇒ TM_SPI1_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2D_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_Alarm_IRQHandler from tm_stm32f4_rtc.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_WKUP_IRQHandler from tm_stm32f4_rtc.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - Reset_Handler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f429_439xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f429_439xx.o(.text)
  - _sputc from printf6.o(i._sputc) referenced from printf6.o(i.__0sprintf$6)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_Init (Thumb, 106 bytes, Stack size 16 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> TM_RTC_DisableAlarm
  - >> TM_RTC_Interrupts

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 34 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 40 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  RCC_DeInit (Thumb, 82 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> TM_DELAY_Init

  RCC_GetFlagStatus (Thumb, 60 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_GetFlagStatus
  [Called By]
  - >> RCC_WaitForHSEStartUp
  - >> TM_RTC_Config

  RCC_WaitForHSEStartUp (Thumb, 56 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus
  [Called By]
  - >> TM_DELAY_Init

  RCC_AdjustHSICalibrationValue (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_RTC_Config

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_RTC_Config

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAIConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 222 bytes, Stack size 20 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> TM_SPI_GetPrescalerFromMaxFrequency

  RCC_RTCCLKConfig (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_RTC_Config

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_RTC_Config

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockACLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockBCLKConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLI2SClkDivConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLSAIClkDivConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LTDCCLKDivConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_TIMCLKPresConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 82 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> Read_Digital_Inputs
  - >> InitLedky

  RCC_AHB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_RTC_Init

  RCC_APB2PeriphClockCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> PWR_DeInit
  - >> SPI_I2S_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> SPI_I2S_DeInit

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEModeConfig (Thumb, 40 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 268 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd
  [Called By]
  - >> InitLedky

  GPIO_Init (Thumb, 144 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> Read_Digital_Inputs
  - >> InitLedky

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> Read_Digital_Inputs

  GPIO_ReadInputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> InitLedky
  - >> TM_ILI9341_Init
  - >> TM_ILI9341_InitLCD
  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text))
  [Called By]

  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 70 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  SPI_I2S_DeInit (Thumb, 152 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  SPI_Init (Thumb, 60 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SPI_Init
  [Called By]
  - >> TM_SPIx_Init

  I2S_Init (Thumb, 396 bytes, Stack size 36 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_StructInit (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text))
  [Called By]

  - >> TM_SPIx_Init

  I2S_StructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_DataSizeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_BiDirectionalLineConfig (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_NSSInternalSoftwareConfig (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_SSOutputCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TIModeCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  I2S_FullDuplexConfig (Thumb, 80 bytes, Stack size 12 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_CalculateCRC (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_TransmitCRC (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRC (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_GetCRCPolynomial (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_DMACmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ITConfig (Thumb, 68 bytes, Stack size 12 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_GetITStatus (Thumb, 52 bytes, Stack size 20 bytes, stm32f4xx_spi.o(.text), UNUSED)

  SPI_I2S_ClearITPendingBit (Thumb, 20 bytes, Stack size 8 bytes, stm32f4xx_spi.o(.text), UNUSED)

  RTC_WaitForSynchro (Thumb, 92 bytes, Stack size 8 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_WaitForSynchro
  [Called By]
  - >> RTC_SynchroShiftConfig
  - >> RTC_SetDate
  - >> RTC_SetTime
  - >> RTC_DeInit
  - >> TM_RTC_Init
  - >> TM_RTC_Config

  RTC_EnterInitMode (Thumb, 84 bytes, Stack size 8 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_EnterInitMode
  [Called By]
  - >> RTC_CoarseCalibCmd
  - >> RTC_CoarseCalibConfig
  - >> RTC_SetDate
  - >> RTC_SetTime
  - >> RTC_RefClockCmd
  - >> RTC_Init
  - >> RTC_DeInit

  RTC_DeInit (Thumb, 204 bytes, Stack size 16 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_EnterInitMode
  - >> RTC_WaitForSynchro

  RTC_ExitInitMode (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text))
  [Called By]

  - >> RTC_CoarseCalibCmd
  - >> RTC_CoarseCalibConfig
  - >> RTC_SetDate
  - >> RTC_SetTime
  - >> RTC_RefClockCmd
  - >> RTC_Init

  RTC_Init (Thumb, 94 bytes, Stack size 12 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RTC_Init ⇒ RTC_EnterInitMode
  [Calls]
  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode
  [Called By]
  - >> TM_RTC_SetDateTime

  RTC_StructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_WriteProtectionCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_RefClockCmd (Thumb, 76 bytes, Stack size 12 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode

  RTC_BypassShadowCmd (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_SetTime (Thumb, 200 bytes, Stack size 24 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = RTC_SetTime ⇒ RTC_EnterInitMode
  [Calls]
  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode
  - >> RTC_WaitForSynchro
  - >> RTC_Bcd2ToByte
  - >> RTC_ByteToBcd2
  [Called By]
  - >> TM_RTC_SetDateTime

  RTC_TimeStructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_GetTime (Thumb, 74 bytes, Stack size 16 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_GetTime
  [Calls]
  - >> RTC_Bcd2ToByte
  [Called By]
  - >> TM_RTC_GetDateTime

  RTC_GetSubSecond (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_SetDate (Thumb, 190 bytes, Stack size 24 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = RTC_SetDate ⇒ RTC_EnterInitMode
  [Calls]
  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode
  - >> RTC_WaitForSynchro
  - >> RTC_Bcd2ToByte
  - >> RTC_ByteToBcd2
  [Called By]
  - >> TM_RTC_SetDateTime

  RTC_DateStructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_GetDate (Thumb, 70 bytes, Stack size 16 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_GetDate
  [Calls]
  - >> RTC_Bcd2ToByte
  [Called By]
  - >> TM_RTC_GetDateTime

  RTC_SetAlarm (Thumb, 230 bytes, Stack size 24 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_Bcd2ToByte
  - >> RTC_ByteToBcd2
  [Called By]
  - >> TM_RTC_SetAlarm

  RTC_AlarmStructInit (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_GetAlarm (Thumb, 114 bytes, Stack size 24 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_Bcd2ToByte

  RTC_AlarmCmd (Thumb, 112 bytes, Stack size 16 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Called By]

  - >> TM_RTC_SetAlarm
  - >> TM_RTC_DisableAlarm

  RTC_AlarmSubSecondConfig (Thumb, 46 bytes, Stack size 12 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_GetAlarmSubSecond (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_WakeUpClockConfig (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text))
  [Called By]

  - >> TM_RTC_Interrupts

  RTC_SetWakeUpCounter (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text))
  [Called By]

  - >> TM_RTC_Interrupts

  RTC_GetWakeUpCounter (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_WakeUpCmd (Thumb, 116 bytes, Stack size 12 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RTC_WakeUpCmd
  [Called By]
  - >> TM_RTC_Interrupts

  RTC_DayLightSavingConfig (Thumb, 50 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_GetStoreOperation (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_OutputConfig (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_CoarseCalibConfig (Thumb, 52 bytes, Stack size 16 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode

  RTC_CoarseCalibCmd (Thumb, 76 bytes, Stack size 12 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_ExitInitMode
  - >> RTC_EnterInitMode

  RTC_CalibOutputCmd (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_CalibOutputConfig (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_SmoothCalibConfig (Thumb, 90 bytes, Stack size 16 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TimeStampCmd (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_GetTimeStamp (Thumb, 144 bytes, Stack size 24 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_Bcd2ToByte

  RTC_GetTimeStampSubSecond (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TamperTriggerConfig (Thumb, 38 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TamperCmd (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TamperFilterConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TamperSamplingFreqConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TamperPinsPrechargeDuration (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TimeStampOnTamperDetectionCmd (Thumb, 38 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TamperPullUpCmd (Thumb, 38 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_WriteBackupRegister (Thumb, 26 bytes, Stack size 8 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_WriteBackupRegister
  [Called By]
  - >> TM_RTC_Config
  - >> TM_RTC_SetDateTime

  RTC_ReadBackupRegister (Thumb, 28 bytes, Stack size 8 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_ReadBackupRegister
  [Called By]
  - >> TM_RTC_Init

  RTC_TamperPinSelection (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_TimeStampPinSelection (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_OutputTypeConfig (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_SynchroShiftConfig (Thumb, 130 bytes, Stack size 20 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_WaitForSynchro

  RTC_ITConfig (Thumb, 94 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text))
  [Called By]

  - >> TM_RTC_SetAlarm
  - >> TM_RTC_DisableAlarm
  - >> TM_RTC_Interrupts

  RTC_GetFlagStatus (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_rtc.o(.text), UNUSED)

  RTC_ClearFlag (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text), UNUSED)
  [Called By]

  - >> TM_RTC_SetAlarm
  - >> TM_RTC_DisableAlarm

  RTC_GetITStatus (Thumb, 60 bytes, Stack size 12 bytes, stm32f4xx_rtc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RTC_GetITStatus
  [Called By]
  - >> RTC_Alarm_IRQHandler
  - >> RTC_WKUP_IRQHandler

  RTC_ClearITPendingBit (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text))
  [Called By]

  - >> RTC_Alarm_IRQHandler
  - >> RTC_WKUP_IRQHandler
  - >> TM_RTC_Init

  EXTI_DeInit (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_Init (Thumb, 142 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text))
  [Called By]

  - >> TM_RTC_DisableAlarm
  - >> TM_RTC_Interrupts

  EXTI_StructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GenerateSWInterrupt (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetFlagStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetITStatus (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text))
  [Called By]

  - >> TM_RTC_DisableAlarm
  - >> TM_RTC_Interrupts
  - >> TM_RTC_Init

  PWR_DeInit (Thumb, 22 bytes, Stack size 8 bytes, stm32f4xx_pwr.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd

  PWR_BackupAccessCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text))
  [Called By]

  - >> TM_RTC_Init

  PWR_PVDLevelConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_PVDCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_WakeUpPinCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_BackupRegulatorCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_MainRegulatorModeConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_OverDriveCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_OverDriveSWCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_UnderDriveCmd (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_MainRegulatorUnderDriveCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_LowRegulatorUnderDriveCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_FlashPowerDownCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_EnterSTOPMode (Thumb, 58 bytes, Stack size 8 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_EnterUnderDriveSTOPMode (Thumb, 58 bytes, Stack size 8 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_EnterSTANDBYMode (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_GetFlagStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  PWR_ClearFlag (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_pwr.o(.text), UNUSED)

  TimingDelay_Decrement (Thumb, 34 bytes, Stack size 8 bytes, tm_stm32f4_delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TimingDelay_Decrement
  [Called By]
  - >> SysTick_Handler

  TM_DELAY_Init (Thumb, 136 bytes, Stack size 16 bytes, tm_stm32f4_delay.o(.text), UNUSED)
  [Calls]

  - >> RCC_WaitForHSEStartUp
  - >> RCC_HSEConfig

  TM_DELAY_EnableDelayTimer (Thumb, 28 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_DELAY_DisableDelayTimer (Thumb, 18 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_SPI6_INT_InitPins (Thumb, 40 bytes, Stack size 16 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = TM_SPI6_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_InitAlternate
  [Called By]
  - >> TM_SPIx_Init

  TM_SPI5_INT_InitPins (Thumb, 84 bytes, Stack size 16 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = TM_SPI5_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_InitAlternate
  [Called By]
  - >> TM_SPIx_Init

  TM_SPI4_INT_InitPins (Thumb, 64 bytes, Stack size 16 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = TM_SPI4_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_InitAlternate
  [Called By]
  - >> TM_SPIx_Init

  TM_SPI3_INT_InitPins (Thumb, 64 bytes, Stack size 16 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = TM_SPI3_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_InitAlternate
  [Called By]
  - >> TM_SPIx_Init

  TM_SPI2_INT_InitPins (Thumb, 110 bytes, Stack size 16 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = TM_SPI2_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_InitAlternate
  [Called By]
  - >> TM_SPIx_Init

  TM_SPI1_INT_InitPins (Thumb, 62 bytes, Stack size 16 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = TM_SPI1_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_InitAlternate
  [Called By]
  - >> TM_SPIx_Init

  TM_SPI_Init (Thumb, 176 bytes, Stack size 24 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = TM_SPI_Init ⇒ TM_SPIx_Init ⇒ TM_SPI1_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_SPIx_Init
  [Called By]
  - >> TM_ILI9341_Init

  TM_SPI_InitWithMode (Thumb, 240 bytes, Stack size 24 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Calls]

  - >> TM_SPIx_Init

  TM_SPI_InitFull (Thumb, 140 bytes, Stack size 40 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Calls]

  - >> TM_SPIx_Init

  TM_SPI_GetPrescalerFromMaxFrequency (Thumb, 88 bytes, Stack size 40 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetClocksFreq

  TM_SPI_Send (Thumb, 46 bytes, Stack size 0 bytes, tm_stm32f4_spi.o(.text))
  [Called By]

  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData
  - >> TM_SPI_SendMulti

  TM_SPI_SendMulti (Thumb, 34 bytes, Stack size 20 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Calls]

  - >> TM_SPI_Send

  TM_SPI_WriteMulti (Thumb, 34 bytes, Stack size 8 bytes, tm_stm32f4_spi.o(.text), UNUSED)

  TM_SPI_ReadMulti (Thumb, 36 bytes, Stack size 12 bytes, tm_stm32f4_spi.o(.text), UNUSED)

  TM_SPI_Send16 (Thumb, 20 bytes, Stack size 0 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Called By]

  - >> TM_SPI_ReadMulti16
  - >> TM_SPI_WriteMulti16
  - >> TM_SPI_SendMulti16

  TM_SPI_SendMulti16 (Thumb, 38 bytes, Stack size 20 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Calls]

  - >> TM_SPI_Send16

  TM_SPI_WriteMulti16 (Thumb, 32 bytes, Stack size 16 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Calls]

  - >> TM_SPI_Send16

  TM_SPI_ReadMulti16 (Thumb, 36 bytes, Stack size 20 bytes, tm_stm32f4_spi.o(.text), UNUSED)
  [Calls]

  - >> TM_SPI_Send16

  TM_GPIO_INT_Init (Thumb, 166 bytes, Stack size 24 bytes, tm_stm32f4_gpio.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = TM_GPIO_INT_Init
  [Called By]
  - >> TM_GPIO_Init
  - >> TM_GPIO_InitAlternate

  TM_GPIO_INT_EnableClock (Thumb, 200 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text))
  [Called By]

  - >> TM_GPIO_Init
  - >> TM_GPIO_InitAlternate

  TM_GPIO_Init (Thumb, 48 bytes, Stack size 36 bytes, tm_stm32f4_gpio.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = TM_GPIO_Init ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_INT_EnableClock
  - >> TM_GPIO_INT_Init
  [Called By]
  - >> TM_ILI9341_Init

  TM_GPIO_InitAlternate (Thumb, 108 bytes, Stack size 44 bytes, tm_stm32f4_gpio.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_INT_EnableClock
  - >> TM_GPIO_INT_Init
  [Called By]
  - >> TM_SPI1_INT_InitPins
  - >> TM_SPI2_INT_InitPins
  - >> TM_SPI3_INT_InitPins
  - >> TM_SPI4_INT_InitPins
  - >> TM_SPI5_INT_InitPins
  - >> TM_SPI6_INT_InitPins

  TM_GPIO_DeInit (Thumb, 38 bytes, Stack size 12 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPinAsInput (Thumb, 38 bytes, Stack size 12 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPinAsOutput (Thumb, 46 bytes, Stack size 12 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPinAsAnalog (Thumb, 38 bytes, Stack size 12 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_GetPortSource (Thumb, 94 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_GetPinSource (Thumb, 18 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_INT_DisableClock (Thumb, 200 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_ILI9341_SendData (Thumb, 40 bytes, Stack size 8 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TM_ILI9341_SendData
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> TM_SPI_Send
  [Called By]
  - >> TM_ILI9341_Rotate
  - >> TM_ILI9341_DrawPixel
  - >> TM_ILI9341_InitLCD
  - >> TM_ILI9341_Fill
  - >> TM_ILI9341_SetCursorPosition

  TM_ILI9341_SendCommand (Thumb, 40 bytes, Stack size 8 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TM_ILI9341_SendCommand
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_SetBits
  - >> TM_SPI_Send
  [Called By]
  - >> TM_ILI9341_Rotate
  - >> TM_ILI9341_DrawPixel
  - >> TM_ILI9341_DisplayOff
  - >> TM_ILI9341_DisplayOn
  - >> TM_ILI9341_InitLCD
  - >> TM_ILI9341_Fill
  - >> TM_ILI9341_SetCursorPosition

  TM_ILI9341_SetCursorPosition (Thumb, 76 bytes, Stack size 24 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TM_ILI9341_SetCursorPosition ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData
  [Called By]
  - >> TM_ILI9341_DrawPixel
  - >> TM_ILI9341_Fill

  TM_ILI9341_Fill (Thumb, 68 bytes, Stack size 24 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = TM_ILI9341_Fill ⇒ TM_ILI9341_SetCursorPosition ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> TM_ILI9341_SetCursorPosition
  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData
  [Called By]
  - >> main
  - >> TM_ILI9341_Init

  TM_ILI9341_Delay (Thumb, 18 bytes, Stack size 8 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TM_ILI9341_Delay
  [Called By]
  - >> TM_ILI9341_InitLCD

  TM_ILI9341_InitLCD (Thumb, 590 bytes, Stack size 8 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TM_ILI9341_InitLCD ⇒ TM_ILI9341_Delay
  [Calls]
  - >> GPIO_SetBits
  - >> TM_ILI9341_Delay
  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData
  [Called By]
  - >> TM_ILI9341_Init

  TM_ILI9341_Init (Thumb, 118 bytes, Stack size 16 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = TM_ILI9341_Init ⇒ TM_SPI_Init ⇒ TM_SPIx_Init ⇒ TM_SPI1_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> GPIO_SetBits
  - >> TM_ILI9341_InitLCD
  - >> TM_ILI9341_Fill
  - >> TM_GPIO_Init
  - >> TM_SPI_Init
  [Called By]
  - >> main

  TM_ILI9341_DisplayOn (Thumb, 10 bytes, Stack size 8 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)
  [Calls]

  - >> TM_ILI9341_SendCommand

  TM_ILI9341_DisplayOff (Thumb, 10 bytes, Stack size 8 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)
  [Calls]

  - >> TM_ILI9341_SendCommand

  TM_ILI9341_DrawPixel (Thumb, 74 bytes, Stack size 16 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = TM_ILI9341_DrawPixel ⇒ TM_ILI9341_SetCursorPosition ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> TM_ILI9341_SetCursorPosition
  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData
  [Called By]
  - >> TM_ILI9341_DrawFilledCircle
  - >> TM_ILI9341_DrawCircle
  - >> TM_ILI9341_DrawLine
  - >> TM_ILI9341_Putc

  TM_ILI9341_Rotate (Thumb, 96 bytes, Stack size 8 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TM_ILI9341_Rotate ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> TM_ILI9341_SendCommand
  - >> TM_ILI9341_SendData
  [Called By]
  - >> main

  TM_ILI9341_Putc (Thumb, 178 bytes, Stack size 40 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = TM_ILI9341_Putc ⇒ TM_ILI9341_DrawPixel ⇒ TM_ILI9341_SetCursorPosition ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> TM_ILI9341_DrawPixel
  [Called By]
  - >> TM_ILI9341_Puts

  TM_ILI9341_Puts (Thumb, 118 bytes, Stack size 40 bytes, tm_stm32f4_ili9341.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = TM_ILI9341_Puts ⇒ TM_ILI9341_Putc ⇒ TM_ILI9341_DrawPixel ⇒ TM_ILI9341_SetCursorPosition ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> TM_ILI9341_Putc
  [Called By]
  - >> TM_RTC_RequestHandler
  - >> main

  TM_ILI9341_GetStringSize (Thumb, 28 bytes, Stack size 16 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)

  TM_ILI9341_DrawLine (Thumb, 230 bytes, Stack size 48 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)
  [Calls]

  - >> TM_ILI9341_DrawPixel
  [Called By]
  - >> TM_ILI9341_DrawFilledCircle
  - >> TM_ILI9341_DrawFilledRectangle
  - >> TM_ILI9341_DrawRectangle

  TM_ILI9341_DrawRectangle (Thumb, 74 bytes, Stack size 32 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)
  [Calls]

  - >> TM_ILI9341_DrawLine

  TM_ILI9341_DrawFilledRectangle (Thumb, 46 bytes, Stack size 32 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)
  [Calls]

  - >> TM_ILI9341_DrawLine

  TM_ILI9341_DrawCircle (Thumb, 260 bytes, Stack size 56 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)
  [Calls]

  - >> TM_ILI9341_DrawPixel

  TM_ILI9341_DrawFilledCircle (Thumb, 350 bytes, Stack size 48 bytes, tm_stm32f4_ili9341.o(.text), UNUSED)
  [Calls]

  - >> TM_ILI9341_DrawLine
  - >> TM_ILI9341_DrawPixel

  TM_RTC_SetDateTime (Thumb, 512 bytes, Stack size 32 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = TM_RTC_SetDateTime ⇒ RTC_SetDate ⇒ RTC_EnterInitMode
  [Calls]
  - >> RTC_WriteBackupRegister
  - >> RTC_SetDate
  - >> RTC_SetTime
  - >> RTC_Init
  [Called By]
  - >> main
  - >> TM_RTC_SetDateTimeString
  - >> TM_RTC_Init

  TM_RTC_Config (Thumb, 86 bytes, Stack size 8 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TM_RTC_Config ⇒ RTC_WriteBackupRegister
  [Calls]
  - >> RTC_WriteBackupRegister
  - >> RTC_WaitForSynchro
  - >> RCC_RTCCLKCmd
  - >> RCC_RTCCLKConfig
  - >> RCC_LSICmd
  - >> RCC_LSEConfig
  - >> RCC_GetFlagStatus
  [Called By]
  - >> TM_RTC_Init

  TM_RTC_GetUnixTimeStamp (Thumb, 216 bytes, Stack size 20 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TM_RTC_GetUnixTimeStamp
  [Called By]
  - >> TM_RTC_GetDateTime

  TM_RTC_GetDateTime (Thumb, 106 bytes, Stack size 16 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TM_RTC_GetDateTime ⇒ TM_RTC_GetUnixTimeStamp
  [Calls]
  - >> RTC_GetDate
  - >> RTC_GetTime
  - >> TM_RTC_GetUnixTimeStamp
  [Called By]
  - >> TM_RTC_RequestHandler
  - >> TM_RTC_Init

  TM_RTC_Init (Thumb, 204 bytes, Stack size 32 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = TM_RTC_Init ⇒ TM_RTC_SetDateTime ⇒ RTC_SetDate ⇒ RTC_EnterInitMode
  [Calls]
  - >> PWR_BackupAccessCmd
  - >> EXTI_ClearITPendingBit
  - >> RTC_ClearITPendingBit
  - >> RTC_ReadBackupRegister
  - >> RTC_WaitForSynchro
  - >> RCC_APB1PeriphClockCmd
  - >> TM_RTC_GetDateTime
  - >> TM_RTC_Config
  - >> TM_RTC_SetDateTime
  [Called By]
  - >> main

  TM_RTC_SetDateTimeString (Thumb, 398 bytes, Stack size 32 bytes, tm_stm32f4_rtc.o(.text), UNUSED)
  [Calls]

  - >> TM_RTC_SetDateTime

  TM_RTC_GetDaysInMonth (Thumb, 86 bytes, Stack size 12 bytes, tm_stm32f4_rtc.o(.text), UNUSED)

  TM_RTC_GetDaysInYear (Thumb, 68 bytes, Stack size 8 bytes, tm_stm32f4_rtc.o(.text), UNUSED)

  TM_RTC_Interrupts (Thumb, 232 bytes, Stack size 16 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = TM_RTC_Interrupts ⇒ NVIC_Init
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_Init
  - >> RTC_ITConfig
  - >> RTC_WakeUpCmd
  - >> RTC_SetWakeUpCounter
  - >> RTC_WakeUpClockConfig
  - >> NVIC_Init
  [Called By]
  - >> main

  TM_RTC_GetDateTimeFromUnix (Thumb, 276 bytes, Stack size 12 bytes, tm_stm32f4_rtc.o(.text), UNUSED)

  TM_RTC_DisableAlarm (Thumb, 134 bytes, Stack size 8 bytes, tm_stm32f4_rtc.o(.text), UNUSED)
  [Calls]

  - >> EXTI_ClearITPendingBit
  - >> EXTI_Init
  - >> RTC_ClearFlag
  - >> RTC_ITConfig
  - >> RTC_AlarmCmd
  - >> NVIC_Init
  [Called By]
  - >> TM_RTC_SetAlarm

  TM_RTC_SetAlarm (Thumb, 208 bytes, Stack size 32 bytes, tm_stm32f4_rtc.o(.text), UNUSED)
  [Calls]

  - >> RTC_ClearFlag
  - >> RTC_ITConfig
  - >> RTC_AlarmCmd
  - >> RTC_SetAlarm
  - >> TM_RTC_DisableAlarm

  TM_RTC_WriteBackupRegister (Thumb, 18 bytes, Stack size 0 bytes, tm_stm32f4_rtc.o(.text), UNUSED)

  TM_RTC_ReadBackupRegister (Thumb, 20 bytes, Stack size 0 bytes, tm_stm32f4_rtc.o(.text), UNUSED)

  TM_RTC_AlarmAHandler (Thumb, 2 bytes, Stack size 0 bytes, tm_stm32f4_rtc.o(.text))
  [Called By]

  - >> RTC_Alarm_IRQHandler

  TM_RTC_AlarmBHandler (Thumb, 2 bytes, Stack size 0 bytes, tm_stm32f4_rtc.o(.text))
  [Called By]

  - >> RTC_Alarm_IRQHandler

  RTC_WKUP_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 168
  - Call Chain = RTC_WKUP_IRQHandler ⇒ TM_RTC_RequestHandler ⇒ TM_ILI9341_Puts ⇒ TM_ILI9341_Putc ⇒ TM_ILI9341_DrawPixel ⇒ TM_ILI9341_SetCursorPosition ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> RTC_ClearITPendingBit
  - >> RTC_GetITStatus
  - >> TM_RTC_RequestHandler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 56 bytes, Stack size 8 bytes, tm_stm32f4_rtc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = RTC_Alarm_IRQHandler ⇒ RTC_GetITStatus
  [Calls]
  - >> RTC_ClearITPendingBit
  - >> RTC_GetITStatus
  - >> TM_RTC_AlarmBHandler
  - >> TM_RTC_AlarmAHandler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  InitLedky (Thumb, 176 bytes, Stack size 16 bytes, read_inputs.o(.text), UNUSED)
  [Calls]

  - >> GPIO_SetBits
  - >> GPIO_Init
  - >> GPIO_DeInit
  - >> RCC_AHB1PeriphClockCmd

  Read_Digital_Inputs (Thumb, 242 bytes, Stack size 16 bytes, read_inputs.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Read_Digital_Inputs ⇒ GPIO_Init
  [Calls]
  - >> GPIO_ReadInputDataBit
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> TM_RTC_RequestHandler

  main (Thumb, 124 bytes, Stack size 16 bytes, main.o(.text))
  [Stack]

  - Max Depth = 188
  - Call Chain = main ⇒ TM_ILI9341_Init ⇒ TM_SPI_Init ⇒ TM_SPIx_Init ⇒ TM_SPI1_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> SystemInit
  - >> TM_RTC_Interrupts
  - >> TM_RTC_Init
  - >> TM_RTC_SetDateTime
  - >> TM_ILI9341_Puts
  - >> TM_ILI9341_Rotate
  - >> TM_ILI9341_Init
  - >> TM_ILI9341_Fill
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  TM_RTC_RequestHandler (Thumb, 158 bytes, Stack size 32 bytes, main.o(.text))
  [Stack]

  - Max Depth = 160
  - Call Chain = TM_RTC_RequestHandler ⇒ TM_ILI9341_Puts ⇒ TM_ILI9341_Putc ⇒ TM_ILI9341_DrawPixel ⇒ TM_ILI9341_SetCursorPosition ⇒ TM_ILI9341_SendCommand
  [Calls]
  - >> Read_Digital_Inputs
  - >> TM_RTC_GetDateTime
  - >> TM_ILI9341_Puts
  - >> __2sprintf
  [Called By]
  - >> RTC_WKUP_IRQHandler

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ TimingDelay_Decrement
  [Calls]
  - >> TimingDelay_Decrement
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  SystemInit (Thumb, 88 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(.text)

  SystemCoreClockUpdate (Thumb, 174 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __0sprintf$6 (Thumb, 34 bytes, Stack size 24 bytes, printf6.o(i.__0sprintf$6), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$6 (Thumb, 0 bytes, Stack size 24 bytes, printf6.o(i.__0sprintf$6), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf6.o(i.__0sprintf$6))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> TM_RTC_RequestHandler

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  RTC_ByteToBcd2 (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text))
  [Called By]

  - >> RTC_SetAlarm
  - >> RTC_SetDate
  - >> RTC_SetTime

  RTC_Bcd2ToByte (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_rtc.o(.text))
  [Called By]

  - >> RTC_GetTimeStamp
  - >> RTC_GetAlarm
  - >> RTC_SetAlarm
  - >> RTC_GetDate
  - >> RTC_SetDate
  - >> RTC_GetTime
  - >> RTC_SetTime

  TM_SPIx_Init (Thumb, 332 bytes, Stack size 48 bytes, tm_stm32f4_spi.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = TM_SPIx_Init ⇒ TM_SPI1_INT_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> SPI_StructInit
  - >> SPI_Init
  - >> TM_SPI1_INT_InitPins
  - >> TM_SPI2_INT_InitPins
  - >> TM_SPI3_INT_InitPins
  - >> TM_SPI4_INT_InitPins
  - >> TM_SPI5_INT_InitPins
  - >> TM_SPI6_INT_InitPins
  [Called By]
  - >> TM_SPI_InitFull
  - >> TM_SPI_InitWithMode
  - >> TM_SPI_Init

  SetSysClock (Thumb, 272 bytes, Stack size 12 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  _printf_core (Thumb, 748 bytes, Stack size 96 bytes, printf6.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  [Called By]
  - >> __0sprintf$6

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printf6.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printf6.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf6.o(i._sputc))
  [Called By]

  - >> __0sprintf$6
  [Address Reference Count : 1]
  - printf6.o(i.__0sprintf$6)

  ### Undefined Global Symbols