intosc |

2018.01.20.23:59:22 | Datasheet

Overview

Memory Map

## int_osc_0

altera_int_osc v17.0

## Parameters
INFORMATION | The output frequency for 10M02, 10M04, 10M08, 10M16, and 10M25 devices is 55~116MHz <br>The output frequency for 10M40, and 10M50 devices is 35~77MHz <br>
DEVICE_FAMILY | MAX10FPGA
PART_NAME | 10M08SAE144C8GES
DEVICE_ID | 08
CLOCK_FREQUENCY_1 | 116
CLOCK_FREQUENCY_2 | 77
CLOCK_FREQUENCY | 116
CBX_AUTO_BLACKBOX | ALL
deviceFamily | UNKNOWN
generateLegacySim | false

## Software Assignments (none)

generation took 0,01 seconds | rendering took 0,12 seconds