All Implementation Messages | po 16. 4 22:36:30 2012

Program |  | All Implementation Messages - Errors, Warnings, and Infos | New
xst | WARNING | Xst:647 - Input <en_zp> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:1305 - Output <ct_d> is never assigned. Tied to value 0. |
xst | WARNING | Xst:647 - Input <control> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <bclk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <data_zp> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <ready> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <en_zp> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:1305 - Output <ct_c> is never assigned. Tied to value 0. |
xst | WARNING | Xst:647 - Input <control> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:1305 - Output <en_z> is never assigned. Tied to value 0. |
xst | WARNING | Xst:647 - Input <bclk> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <data_zp> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <ready> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:1305 - Output <zpoz_c> is never assigned. Tied to value 000. |
xst | WARNING | Xst:1305 - Output <en_zp> is never assigned. Tied to value 0. |
xst | WARNING | Xst:1305 - Output <data_zp> is never assigned. Tied to value 00000000000000000000. |
xst | WARNING | Xst:647 - Input <ready> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <zpoz_c> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:647 - Input <zpoz_d> is never used. This port will be preserved and left unconnected if it belongs to a top-level block or it belongs to a sub-block and the hierarchy of this sub-block is preserved. |
xst | WARNING | Xst:1780 - Signal <wkey> is never used or assigned. This unconnected signal will be trimmed during the optimization process. |
xst | WARNING | Xst:1780 - Signal <rkey> is never used or assigned. This unconnected signal will be trimmed during the optimization process. |
xst | WARNING | Xst:646 - Signal <data_zppom2> is assigned but never used. This unconnected signal will be trimmed during the optimization process. |
xst | WARNING | Xst:646 - Signal <data_zppom1> is assigned but never used. This unconnected signal will be trimmed during the optimization process. |
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<0>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<10>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<1>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<11>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<2>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<12>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<3>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<13>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<4>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<14>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<5>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<15>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<6>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<7>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<8>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtridata_data_out<9>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<9>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<8>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<7>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<6>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<15>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<5>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<14>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<4>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<13>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<3>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<12>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<2>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<11>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<1>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<10>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:736 - Found 1-bit latch for signal <Mtrien_data_out<0>> created at line 116. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. | New
xst | WARNING | Xst:737 - Found 18-bit latch for signal <n>. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. |
xst | WARNING | Xst:737 - Found 18-bit latch for signal <i>. Latches may be generated from incomplete case or if statements. We do not recommend the use of latches in FPGA/CPLD designs, as they may lead to timing problems. |
xst | WARNING | Xst:653 - Signal <ready1> is used but never assigned. This sourceless signal will be automatically connected to value 0. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<1>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<0>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<2>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<3>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<4>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<5>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<6>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<7>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<8>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<9>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<10>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<11>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<12>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<13>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<14>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<15>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<16>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<17>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<18>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<19>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1293 - FF/Latch <FFd3> has a constant value of 0 in block <FSM>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <data_zz_0> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_1> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_2> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_3> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_4> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_5> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_6> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_7> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_8> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_9> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_10> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_11> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_12> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_13> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_14> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_15> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_16> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_17> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_18> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <data_zz_19> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <dout> (without init value) has a constant value of 0 in block <Inst_dat>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <en2> (without init value) has a constant value of 0 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<19>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <0>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <1>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <2>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <3>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <4>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <5>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <6>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <7>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <8>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <9>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <10>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <11>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <12>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <13>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <14>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <15>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <16>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <0> (without init value) has a constant value of 0 in block <17>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<1>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<0>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<2>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<3>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<4>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<5>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<6>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<7>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<8>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<9>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<10>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<11>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<12>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<13>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<14>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<15>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<16>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<17>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<18>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<0>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<10>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<1>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<11>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<2>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<12>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<3>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<13>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<4>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<14>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<5>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<15>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<6>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<7>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<8>>. | New
xst | WARNING | Xst:1294 - Latch <0> is equivalent to a wire in block <Mtridata_data_out<9>>. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<19>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<18>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<17>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<16>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<15>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<14>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<13>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<12>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<11>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<10>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<9>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<8>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<7>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<6>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<5>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<4>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<3>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<2>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<0>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<1>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<19>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<18>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<17>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<16>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<15>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<14>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<13>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<12>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<11>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<10>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<9>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<8>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<7>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<6>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<5>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<4>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<3>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<2>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<0>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<1>> (without init value) has a constant value of 1 in block <Inst_zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_z2<19>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<18>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<17>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<16>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<15>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<14>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<13>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<12>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<11>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<10>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<9>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<8>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<7>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<6>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<5>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<4>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<3>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<2>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<0>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <Mtrien_data_z2<1>> (without init value) has a constant value of 1 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1895 - Due to other FF/Latch trimming, FF/Latch <en2> (without init value) has a constant value of 0 in block <zero>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<1> and Mtrien_data_z2<0> Mtrien_data_z2<0> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<2> Mtrien_data_z2<2> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<3> Mtrien_data_z2<3> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<4> Mtrien_data_z2<4> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<5> Mtrien_data_z2<5> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<6> Mtrien_data_z2<6> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<7> Mtrien_data_z2<7> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<8> Mtrien_data_z2<8> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<9> Mtrien_data_z2<9> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<10> Mtrien_data_z2<10> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<11> Mtrien_data_z2<11> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<12> Mtrien_data_z2<12> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<13> Mtrien_data_z2<13> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<14> Mtrien_data_z2<14> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<15> Mtrien_data_z2<15> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<16> Mtrien_data_z2<16> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<17> Mtrien_data_z2<17> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<18> Mtrien_data_z2<18> signal will be lost. |
xst | WARNING | Xst:638 - in unit zero Conflict on KEEP property on signal Mtrien_data_z2<0> and Mtrien_data_z2<19> Mtrien_data_z2<19> signal will be lost. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<1>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<0>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<2>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<3>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<4>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<5>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<6>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<7>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<8>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<9>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<10>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<11>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<12>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<13>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<14>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<15>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<16>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<17>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<18>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:2677 - Node <Mtrien_data_z2<19>> of sequential type is unconnected in block <zero>. |
xst | WARNING | Xst:1710 - FF/Latch <n_17> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_16> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_15> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_14> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_13> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_12> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_11> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_10> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_9> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_8> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_7> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_6> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_5> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_4> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_3> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_2> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_1> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <n_0> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1896 - Due to other FF/Latch trimming, FF/Latch <p_s_FSM_FFd3> has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<9>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<8>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<7>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<6>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<15>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<5>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<14>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<4>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<13>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<3>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<12>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<2>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<11>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<1>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<10>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1294 - Latch <Mtridata_data_out<0>> is equivalent to a wire in block <zprac_adr>. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<0>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<10>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<1>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<11>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<2>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<12>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<3>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<13>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<4>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<14>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<5>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<15>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<6>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<7>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<8>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:1710 - FF/Latch <Mtrien_data_out<9>> (without init value) has a constant value of 0 in block <zprac_adr>. This FF/Latch will be trimmed during the optimization process. | New
xst | WARNING | Xst:2042 - Unit zero: 40 internal tristates are replaced by logic (pull-up yes): |
xst | WARNING | Xst:2042 - Unit dat: 20 internal tristates are replaced by logic (pull-up yes): |
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<0>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<10>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<1>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<11>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<2>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<12>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<3>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<13>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<4>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<14>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<5>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<15>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<6>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<7>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<8>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:2677 - Node <Mtrien_data_out<9>> of sequential type is unconnected in block <zprac_adr>. | New
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_0> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_1> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_2> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_3> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_4> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_5> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_6> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_7> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_8> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_9> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_10> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_11> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_12> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_13> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_14> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_15> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_16> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_17> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_18> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:1710 - FF/Latch <Inst_data/Inst_dat/data_zz_19> (without init value) has a constant value of 1 in block <top>. This FF/Latch will be trimmed during the optimization process. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_15> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_14> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_13> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_12> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_11> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_10> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_9> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_8> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_7> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_6> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_5> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_4> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_3> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_2> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_1> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_sram/din_reg_0> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom2_3> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom2_2> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom2_1> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom2_0> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_15> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_14> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_13> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_12> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_11> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_10> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_9> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_8> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_7> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_6> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_5> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_4> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_3> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_2> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_1> of sequential type is unconnected in block <top>. |
xst | WARNING | Xst:2677 - Node <Inst_memory/Inst_zprac_adr/data_pom1_0> of sequential type is unconnected in block <top>. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:2371 - HDL ADVISOR - Logic functions respectively driving the data and gate enable inputs of this latch share common terms. This situation will potentially lead to setup/hold violations and, as a result, to simulation problems. This situation may come from an incomplete case statement (all selector values are not covered). You should carefully review if it was in your intentions to describe such a latch. |
xst | INFO | Xst:1767 - HDL ADVISOR - Resource sharing has identified that some arithmetic operations in this design can share the same physical resources for reduced device utilization. For improved clock frequency you may try to disable resource sharing. |
xst | INFO | Xst:3034 - In order to maximize performance and save block RAM resources, the small ROM <Mrom_control_mux0000> will be implemented on LUT. If you want to force its implementation on block, use option/constraint rom_style. |
xst | INFO | Xst:2169 - HDL ADVISOR - Some clock signals were not automatically buffered by XST with BUFG/BUFR resources. Please use the buffer_type constraint in order to insert these buffers to the clock signals to help prevent skew problems. |