(export (version D)
  (design
    (source C:\Users\NXF47030\Documents\KiCad\PWR-mkl27z\PWR-mkl27z.sch)
    (date "4/22/2020 1:39:07 PM")
    (tool "Eeschema (5.1.2)-2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source PWR-mkl27z.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J2)
      (value Conn_ARM_JTAG_SWD_10)
      (footprint Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical)
      (datasheet http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf)
      (libsource (lib Connector) (part Conn_ARM_JTAG_SWD_10) (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5C3138))
    (comp (ref J1)
      (value USB_B_Micro)
      (footprint Connector_USB:USB_Micro-B_Molex_47346-0001)
      (datasheet ~)
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5C6237))
    (comp (ref R5)
      (value 33)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5CE78F))
    (comp (ref R4)
      (value 33)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5CEE3D))
    (comp (ref D1)
      (value B130-E3)
      (footprint Diode_SMD:D_SMA_Handsoldering)
      (datasheet http://www.vishay.com/docs/88946/b120.pdf)
      (libsource (lib Diode) (part B130-E3) (description "30V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5D70B1))
    (comp (ref C1)
      (value 2.2uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5DA9DD))
    (comp (ref C6)
      (value "0.1uF DNP")
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5E6743))
    (comp (ref C5)
      (value 2.2uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5E5951))
    (comp (ref FB3)
      (value "Ferrite_Bead_Small 330OHM")
      (footprint Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5E402A))
    (comp (ref C8)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5FB806))
    (comp (ref C11)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5FBCA5))
    (comp (ref C13)
      (value 1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5FC575))
    (comp (ref C14)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5FCA11))
    (comp (ref C9)
      (value 1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5FCDC8))
    (comp (ref C7)
      (value 1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5FD2B6))
    (comp (ref C10)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D607F62))
    (comp (ref C12)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D61078B))
    (comp (ref C2)
      (value 2.2uF)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D64BF34))
    (comp (ref R2)
      (value 10)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D669609))
    (comp (ref JP1)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D66A70A))
    (comp (ref porRegSelect1)
      (value DNC)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper_NC_Dual) (description "Dual jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5EFBA9))
    (comp (ref D4)
      (value B130-E3)
      (footprint Diode_SMD:D_SMA_Handsoldering)
      (datasheet http://www.vishay.com/docs/88946/b120.pdf)
      (libsource (lib Diode) (part B130-E3) (description "30V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6135BB))
    (comp (ref JP2)
      (value Jumper)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Device) (part Jumper) (description "Jumper, normally closed"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6243D9))
    (comp (ref FB1)
      (value "Ferrite_Bead_Small 330OHM")
      (footprint Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5C8403))
    (comp (ref FB2)
      (value "Ferrite_Bead_Small 330OHM")
      (footprint Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5C7718))
    (comp (ref X1)
      (value "XTAL 32kHz")
      (footprint keebs:xtal_4.9x1.8mm)
      (libsource (lib keyboard_parts) (part XTAL) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D641279))
    (comp (ref C4)
      (value 12p)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D642385))
    (comp (ref C3)
      (value 12p)
      (footprint Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part CP) (description "Polarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D642D56))
    (comp (ref R6)
      (value 10M)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D665461))
    (comp (ref D2)
      (value D_TVS)
      (footprint Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6AE16E))
    (comp (ref R3)
      (value 10)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D62DE11))
    (comp (ref D3)
      (value D_TVS)
      (footprint Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D69E2AF))
    (comp (ref D5)
      (value D_TVS)
      (footprint Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6A823F))
    (comp (ref J5)
      (value Conn_02x12_Counter_Clockwise)
      (footprint keebs:PinSocket_2x12_P2.54mm_Horizontal_Counter_Clockwise)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x12_Counter_Clockwise) (description "Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D74770D))
    (comp (ref J4)
      (value Conn_02x08_Counter_Clockwise)
      (footprint keebs:PinSocket_2x08_P2.54mm_Horizontal_Counter_Clockwise)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise) (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D85ACA8))
    (comp (ref J3)
      (value Conn_02x08_Counter_Clockwise)
      (footprint keebs:PinSocket_2x08_P2.54mm_Horizontal_Counter_Clockwise)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise) (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D8D4968))
    (comp (ref U2)
      (value MKL27Z32VLH4)
      (footprint Package_QFP:LQFP-64_10x10mm_P0.5mm)
      (datasheet http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf)
      (libsource (lib MCU_NXP_Kinetis) (part MKL27Z32VLH4) (description "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, USB FS Device (xtal-less)/OTG, LQFP-64"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D5C10F4))
    (comp (ref IC1)
      (value MCP1812BT-033_TT)
      (footprint SamacSys_Parts:SOT95P237X112-3N)
      (datasheet https://componentsearchengine.com/Datasheets/1/MCP1812BT-033_TT.pdf)
      (fields
        (field (name Description) "LDO Voltage Regulators Ultra Low Iq LDO")
        (field (name Height) 1.12)
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) MCP1812BT-033/TT)
        (field (name "Mouser Part Number") 579-MCP1812BT-033/TT)
        (field (name "Mouser Price/Stock") https://www.mouser.com/Search/Refine.aspx?Keyword=579-MCP1812BT-033%2FTT))
      (libsource (lib SamacSys_Parts) (part MCP1812BT-033_TT) (description "LDO Voltage Regulators Ultra Low Iq LDO"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D68DAE8))
    (comp (ref H4)
      (value MountingHole)
      (footprint MountingHole:MountingHole_4mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6F8F1C))
    (comp (ref H2)
      (value MountingHole)
      (footprint MountingHole:MountingHole_4mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6F9DC7))
    (comp (ref H1)
      (value MountingHole)
      (footprint MountingHole:MountingHole_4mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6FB296))
    (comp (ref H3)
      (value MountingHole)
      (footprint MountingHole:MountingHole_4mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole) (description "Mounting Hole without connection"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5D6FBDB6)))
  (libparts
    (libpart (lib Connector) (part Conn_ARM_JTAG_SWD_10)
      (description "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface")
      (docs http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf)
      (footprints
        (fp PinHeader?2x05?P1.27mm*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_ARM_JTAG_SWD_10))
      (pins
        (pin (num 1) (name VTref) (type power_in))
        (pin (num 2) (name SWDIO/TMS) (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name SWDCLK/TCK) (type output))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name SWO/TDO) (type input))
        (pin (num 7) (name KEY) (type NotConnected))
        (pin (num 8) (name NC/TDI) (type output))
        (pin (num 9) (name GNDDetect) (type passive))
        (pin (num 10) (name ~RESET~) (type openCol))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x08_Counter_Clockwise)
      (description "Generic connector, double row, 02x08, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x08_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_02x12_Counter_Clockwise)
      (description "Generic connector, double row, 02x12, counter clockwise pin numbering scheme (similar to DIP packge numbering), script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_2x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_02x12_Counter_Clockwise))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))
        (pin (num 10) (name Pin_10) (type passive))
        (pin (num 11) (name Pin_11) (type passive))
        (pin (num 12) (name Pin_12) (type passive))
        (pin (num 13) (name Pin_13) (type passive))
        (pin (num 14) (name Pin_14) (type passive))
        (pin (num 15) (name Pin_15) (type passive))
        (pin (num 16) (name Pin_16) (type passive))
        (pin (num 17) (name Pin_17) (type passive))
        (pin (num 18) (name Pin_18) (type passive))
        (pin (num 19) (name Pin_19) (type passive))
        (pin (num 20) (name Pin_20) (type passive))
        (pin (num 21) (name Pin_21) (type passive))
        (pin (num 22) (name Pin_22) (type passive))
        (pin (num 23) (name Pin_23) (type passive))
        (pin (num 24) (name Pin_24) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarized capacitor")
      (docs ~)
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_TVS)
      (description "Bidirectional transient-voltage-suppression diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_TVS))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A2) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead_Small)
      (description "Ferrite bead, small symbol")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Jumper)
      (description "Jumper, normally closed")
      (docs ~)
      (footprints
        (fp SolderJumper*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part Jumper_NC_Dual)
      (description "Dual jumper, normally closed")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged*))
      (fields
        (field (name Reference) JP)
        (field (name Value) Jumper_NC_Dual))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Diode) (part B120-E3)
      (aliases
        (alias B130-E3)
        (alias B140-E3)
        (alias B150-E3)
        (alias B160-E3))
      (description "20V 1A Schottky Barrier Rectifier Diode, SMA(DO-214AC)")
      (docs http://www.vishay.com/docs/88946/b120.pdf)
      (footprints
        (fp D*SMA*))
      (fields
        (field (name Reference) D)
        (field (name Value) B120-E3)
        (field (name Footprint) Diode_SMD:D_SMA))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib MCU_NXP_Kinetis) (part MKL27Z64VLH4)
      (aliases
        (alias MKL27Z32VLH4))
      (description "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, USB FS Device (xtal-less)/OTG, LQFP-64")
      (docs http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf)
      (footprints
        (fp LQFP*10x10mm*P0.5mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MKL27Z64VLH4)
        (field (name Footprint) Package_QFP:LQFP-64_10x10mm_P0.5mm))
      (pins
        (pin (num 1) (name PTE0) (type BiDi))
        (pin (num 2) (name PTE1) (type BiDi))
        (pin (num 3) (name VDD) (type power_in))
        (pin (num 4) (name VSS) (type power_in))
        (pin (num 5) (name USB0_DP) (type BiDi))
        (pin (num 6) (name USB0_DM) (type BiDi))
        (pin (num 7) (name USB_VDD) (type power_in))
        (pin (num 8) (name PTE16) (type BiDi))
        (pin (num 9) (name PTE20) (type BiDi))
        (pin (num 10) (name PTE21) (type BiDi))
        (pin (num 11) (name PTE22) (type BiDi))
        (pin (num 12) (name PTE23) (type BiDi))
        (pin (num 13) (name VDDA) (type power_in))
        (pin (num 14) (name VREFH/VREFO) (type power_in))
        (pin (num 15) (name VREFL) (type power_in))
        (pin (num 16) (name VSSA) (type power_in))
        (pin (num 17) (name PTE29) (type BiDi))
        (pin (num 18) (name PTE30) (type BiDi))
        (pin (num 19) (name PTE31) (type BiDi))
        (pin (num 20) (name PTE24) (type BiDi))
        (pin (num 21) (name PTE25) (type BiDi))
        (pin (num 22) (name PTA0) (type BiDi))
        (pin (num 23) (name PTA1) (type BiDi))
        (pin (num 24) (name PTA2) (type BiDi))
        (pin (num 25) (name PTA3) (type BiDi))
        (pin (num 26) (name PTA4) (type BiDi))
        (pin (num 27) (name PTA5) (type BiDi))
        (pin (num 28) (name PTA12) (type BiDi))
        (pin (num 29) (name PTA13) (type BiDi))
        (pin (num 30) (name VDD) (type passive))
        (pin (num 31) (name VSS) (type passive))
        (pin (num 32) (name PTA18) (type BiDi))
        (pin (num 33) (name PTA19) (type BiDi))
        (pin (num 34) (name PTA20) (type BiDi))
        (pin (num 35) (name PTB0/LLWU_P5) (type BiDi))
        (pin (num 36) (name PTB1) (type BiDi))
        (pin (num 37) (name PTB2) (type BiDi))
        (pin (num 38) (name PTB3) (type BiDi))
        (pin (num 39) (name PTB16) (type BiDi))
        (pin (num 40) (name PTB17) (type BiDi))
        (pin (num 41) (name PTB18) (type BiDi))
        (pin (num 42) (name PTB19) (type BiDi))
        (pin (num 43) (name PTC0) (type BiDi))
        (pin (num 44) (name PTC1/LLWU_P6/RTC_CLKIN) (type BiDi))
        (pin (num 45) (name PTC2) (type BiDi))
        (pin (num 46) (name PTC3/LLWU_P7) (type BiDi))
        (pin (num 47) (name VSS) (type passive))
        (pin (num 48) (name VDD) (type passive))
        (pin (num 49) (name PTC4/LLWU_P8) (type BiDi))
        (pin (num 50) (name PTC5/LLWU_P9) (type BiDi))
        (pin (num 51) (name PTC6/LLWU_P10) (type BiDi))
        (pin (num 52) (name PTC7) (type BiDi))
        (pin (num 53) (name PTC8) (type BiDi))
        (pin (num 54) (name PTC9) (type BiDi))
        (pin (num 55) (name PTC10) (type BiDi))
        (pin (num 56) (name PTC11) (type BiDi))
        (pin (num 57) (name PTD0) (type BiDi))
        (pin (num 58) (name PTD1) (type BiDi))
        (pin (num 59) (name PTD2) (type BiDi))
        (pin (num 60) (name PTD3) (type BiDi))
        (pin (num 61) (name PTD4/LLWU_P14) (type BiDi))
        (pin (num 62) (name PTD5) (type BiDi))
        (pin (num 63) (name PTD6/LLWU_P15) (type BiDi))
        (pin (num 64) (name PTD7) (type BiDi))))
    (libpart (lib Mechanical) (part MountingHole)
      (description "Mounting Hole without connection")
      (docs ~)
      (footprints
        (fp MountingHole*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole)))
    (libpart (lib SamacSys_Parts) (part MCP1812BT-033_TT)
      (description "LDO Voltage Regulators Ultra Low Iq LDO")
      (docs https://componentsearchengine.com/Datasheets/1/MCP1812BT-033_TT.pdf)
      (fields
        (field (name Reference) IC)
        (field (name Value) MCP1812BT-033_TT)
        (field (name Footprint) SOT95P237X112-3N)
        (field (name Datasheet) https://componentsearchengine.com/Datasheets/1/MCP1812BT-033_TT.pdf)
        (field (name Description) "LDO Voltage Regulators Ultra Low Iq LDO")
        (field (name Height) 1.12)
        (field (name "Mouser Part Number") 579-MCP1812BT-033/TT)
        (field (name "Mouser Price/Stock") https://www.mouser.com/Search/Refine.aspx?Keyword=579-MCP1812BT-033%2FTT)
        (field (name Manufacturer_Name) Microchip)
        (field (name Manufacturer_Part_Number) MCP1812BT-033/TT))
      (pins
        (pin (num 1) (name VOUT) (type BiDi))
        (pin (num 2) (name VIN) (type BiDi))
        (pin (num 3) (name GND) (type BiDi))))
    (libpart (lib keyboard_parts) (part XTAL)
      (fields
        (field (name Reference) X)
        (field (name Value) XTAL))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Connector_Generic)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector_Generic.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical Diode)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Diode.lib"))
    (library (logical MCU_NXP_Kinetis)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/MCU_NXP_Kinetis.lib"))
    (library (logical Mechanical)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Mechanical.lib"))
    (library (logical SamacSys_Parts)
      (uri C:/Users/NXF47030/AppData/Roaming/kicad/SamacSys_Parts.lib))
    (library (logical keyboard_parts)
      (uri C:/KiCad/kicad_lib_tmk-master/keyboard_parts.lib)))
  (nets
    (net (code 1) (name "Net-(J4-Pad10)")
      (node (ref J4) (pin 10)))
    (net (code 2) (name "Net-(J4-Pad11)")
      (node (ref J4) (pin 11)))
    (net (code 3) (name /PTE31)
      (node (ref U2) (pin 19))
      (node (ref J5) (pin 12)))
    (net (code 4) (name /PTE24)
      (node (ref J5) (pin 8))
      (node (ref U2) (pin 20)))
    (net (code 5) (name /PTE25)
      (node (ref J5) (pin 9))
      (node (ref U2) (pin 21)))
    (net (code 6) (name /PTE29)
      (node (ref U2) (pin 17))
      (node (ref J5) (pin 10)))
    (net (code 7) (name /PTE30)
      (node (ref U2) (pin 18))
      (node (ref J5) (pin 11)))
    (net (code 8) (name "Net-(J4-Pad13)")
      (node (ref J4) (pin 13)))
    (net (code 9) (name GNDA)
      (node (ref J4) (pin 16))
      (node (ref C10) (pin 2))
      (node (ref U2) (pin 16)))
    (net (code 10) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1)))
    (net (code 11) (name /PTB17)
      (node (ref U2) (pin 40))
      (node (ref J3) (pin 11)))
    (net (code 12) (name "Net-(J3-Pad6)")
      (node (ref J3) (pin 6)))
    (net (code 13) (name "Net-(J4-Pad14)")
      (node (ref J4) (pin 14)))
    (net (code 14) (name "Net-(J4-Pad15)")
      (node (ref J4) (pin 15)))
    (net (code 15) (name GND)
      (node (ref C6) (pin 2))
      (node (ref U2) (pin 31))
      (node (ref U2) (pin 4))
      (node (ref IC1) (pin 3))
      (node (ref FB1) (pin 1))
      (node (ref U2) (pin 47))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref J4) (pin 12))
      (node (ref C8) (pin 2))
      (node (ref J2) (pin 5))
      (node (ref J4) (pin 9))
      (node (ref J1) (pin 5))
      (node (ref J2) (pin 3))
      (node (ref C5) (pin 2)))
    (net (code 16) (name "Net-(FB2-Pad1)")
      (node (ref JP2) (pin 2))
      (node (ref FB2) (pin 1))
      (node (ref R3) (pin 2)))
    (net (code 17) (name /PTE1)
      (node (ref J5) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 18) (name "Net-(J5-Pad3)")
      (node (ref J5) (pin 3)))
    (net (code 19) (name /PTE20)
      (node (ref U2) (pin 9))
      (node (ref J5) (pin 4)))
    (net (code 20) (name /PTE21)
      (node (ref U2) (pin 10))
      (node (ref J5) (pin 5)))
    (net (code 21) (name /PTE22)
      (node (ref J5) (pin 6))
      (node (ref U2) (pin 11)))
    (net (code 22) (name /PTE23)
      (node (ref J5) (pin 7))
      (node (ref U2) (pin 12)))
    (net (code 23) (name /PTE0)
      (node (ref U2) (pin 1))
      (node (ref J5) (pin 1)))
    (net (code 24) (name /MD+)
      (node (ref R5) (pin 2))
      (node (ref U2) (pin 5)))
    (net (code 25) (name /MD-)
      (node (ref U2) (pin 6))
      (node (ref R4) (pin 1)))
    (net (code 26) (name "Net-(J2-Pad10)")
      (node (ref J2) (pin 10))
      (node (ref U2) (pin 34)))
    (net (code 27) (name /D+)
      (node (ref J1) (pin 3))
      (node (ref R5) (pin 1))
      (node (ref D3) (pin 1)))
    (net (code 28) (name "Net-(C12-Pad1)")
      (node (ref U2) (pin 14))
      (node (ref C12) (pin 1)))
    (net (code 29) (name /PTB18)
      (node (ref J3) (pin 10))
      (node (ref U2) (pin 41)))
    (net (code 30) (name /PTB19)
      (node (ref U2) (pin 42))
      (node (ref J3) (pin 9)))
    (net (code 31) (name /PTB16)
      (node (ref U2) (pin 39))
      (node (ref J3) (pin 12)))
    (net (code 32) (name /PTA1)
      (node (ref U2) (pin 23))
      (node (ref J3) (pin 8)))
    (net (code 33) (name /PTA2)
      (node (ref U2) (pin 24))
      (node (ref J3) (pin 7)))
    (net (code 34) (name /PTA4)
      (node (ref J3) (pin 5))
      (node (ref U2) (pin 26)))
    (net (code 35) (name /PTA5)
      (node (ref U2) (pin 27))
      (node (ref J3) (pin 4)))
    (net (code 36) (name /PTA12)
      (node (ref U2) (pin 28))
      (node (ref J3) (pin 3)))
    (net (code 37) (name /PTB0)
      (node (ref U2) (pin 35))
      (node (ref J3) (pin 16)))
    (net (code 38) (name /PTB1)
      (node (ref U2) (pin 36))
      (node (ref J3) (pin 15)))
    (net (code 39) (name /PTB2)
      (node (ref J3) (pin 14))
      (node (ref U2) (pin 37)))
    (net (code 40) (name /PTB3)
      (node (ref J3) (pin 13))
      (node (ref U2) (pin 38)))
    (net (code 41) (name +3.3VA)
      (node (ref C13) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U2) (pin 30))
      (node (ref U2) (pin 48))
      (node (ref U2) (pin 13))
      (node (ref J2) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref FB3) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref C14) (pin 1)))
    (net (code 42) (name "Net-(J2-Pad6)")
      (node (ref J2) (pin 6)))
    (net (code 43) (name /PTA13)
      (node (ref U2) (pin 29))
      (node (ref J3) (pin 2)))
    (net (code 44) (name "Net-(J2-Pad8)")
      (node (ref J2) (pin 8)))
    (net (code 45) (name "Net-(J2-Pad9)")
      (node (ref J2) (pin 9)))
    (net (code 46) (name +5V)
      (node (ref D1) (pin 2))
      (node (ref FB2) (pin 2))
      (node (ref porRegSelect1) (pin 1))
      (node (ref porRegSelect1) (pin 2)))
    (net (code 47) (name "Net-(C4-Pad1)")
      (node (ref U2) (pin 33))
      (node (ref X1) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref R6) (pin 2)))
    (net (code 48) (name "Net-(C3-Pad1)")
      (node (ref U2) (pin 32))
      (node (ref R6) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref X1) (pin 1)))
    (net (code 49) (name "Net-(D2-Pad1)")
      (node (ref JP2) (pin 1))
      (node (ref D2) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref R3) (pin 1)))
    (net (code 50) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref FB1) (pin 2))
      (node (ref D3) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref J1) (pin 6)))
    (net (code 51) (name "Net-(D4-Pad2)")
      (node (ref R2) (pin 2))
      (node (ref JP1) (pin 2))
      (node (ref D4) (pin 2)))
    (net (code 52) (name "Net-(C2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref IC1) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref JP1) (pin 1)))
    (net (code 54) (name "Net-(U2-Pad8)")
      (node (ref porRegSelect1) (pin 3))
      (node (ref U2) (pin 8)))
    (net (code 55) (name /PTD6)
      (node (ref J4) (pin 7))
      (node (ref U2) (pin 63)))
    (net (code 56) (name /PTC9)
      (node (ref U2) (pin 54))
      (node (ref J5) (pin 15)))
    (net (code 57) (name /PTC10)
      (node (ref U2) (pin 55))
      (node (ref J5) (pin 14)))
    (net (code 58) (name /PTC11)
      (node (ref U2) (pin 56))
      (node (ref J5) (pin 13)))
    (net (code 59) (name /PTD0)
      (node (ref J4) (pin 1))
      (node (ref U2) (pin 57)))
    (net (code 60) (name /PTD1)
      (node (ref J4) (pin 2))
      (node (ref U2) (pin 58)))
    (net (code 61) (name /PTD2)
      (node (ref J4) (pin 3))
      (node (ref U2) (pin 59)))
    (net (code 62) (name /PTD3)
      (node (ref J4) (pin 4))
      (node (ref U2) (pin 60)))
    (net (code 63) (name /PTD4)
      (node (ref U2) (pin 61))
      (node (ref J4) (pin 5)))
    (net (code 64) (name /PTD5)
      (node (ref J4) (pin 6))
      (node (ref U2) (pin 62)))
    (net (code 65) (name /PTC8)
      (node (ref J5) (pin 16))
      (node (ref U2) (pin 53)))
    (net (code 66) (name /PTD7)
      (node (ref U2) (pin 64))
      (node (ref J4) (pin 8)))
    (net (code 67) (name /PTC0)
      (node (ref U2) (pin 43))
      (node (ref J5) (pin 24)))
    (net (code 68) (name /PTC1)
      (node (ref U2) (pin 44))
      (node (ref J5) (pin 23)))
    (net (code 69) (name /PTC2)
      (node (ref U2) (pin 45))
      (node (ref J5) (pin 22)))
    (net (code 70) (name /PTC3)
      (node (ref J5) (pin 21))
      (node (ref U2) (pin 46)))
    (net (code 71) (name /PTC4)
      (node (ref J5) (pin 20))
      (node (ref U2) (pin 49)))
    (net (code 72) (name /PTC5)
      (node (ref J5) (pin 19))
      (node (ref U2) (pin 50)))
    (net (code 73) (name /PTC6)
      (node (ref J5) (pin 18))
      (node (ref U2) (pin 51)))
    (net (code 74) (name /PTC7)
      (node (ref U2) (pin 52))
      (node (ref J5) (pin 17)))
    (net (code 75) (name "Net-(C1-Pad1)")
      (node (ref IC1) (pin 2))
      (node (ref D1) (pin 1))
      (node (ref C1) (pin 1)))
    (net (code 76) (name "Net-(C5-Pad1)")
      (node (ref U2) (pin 7))
      (node (ref C5) (pin 1))
      (node (ref FB3) (pin 2))
      (node (ref C6) (pin 1)))
    (net (code 77) (name "Net-(J2-Pad7)")
      (node (ref J2) (pin 7)))
    (net (code 78) (name /D-)
      (node (ref D5) (pin 1))
      (node (ref J1) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 79) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 80) (name GNDREF)
      (node (ref U2) (pin 15))
      (node (ref C12) (pin 2)))
    (net (code 81) (name "Net-(J2-Pad4)")
      (node (ref U2) (pin 22))
      (node (ref J2) (pin 4)))
    (net (code 82) (name /PTA3)
      (node (ref U2) (pin 25))
      (node (ref J2) (pin 2)))))