Source:	C:\Users\NXF47030\Documents\KiCad\PWR-mkl27z\PWR-mkl27z.sch
Date:	8/29/2019 1:08:23 PM
Tool:	Eeschema (5.1.2)-2
Generator:	C:\Program Files\KiCad\bin\scripting\plugins/bom_csv_grouped_by_value.py
Component Count:	40

Individual Components:

Item	Qty	Reference(s)	Value	LibPart	Footprint	Datasheet
		C1	10uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C2	10uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C3	12p	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C4	12p	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C5	2.2uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C6	0.1uF DNP	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C7	1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C8	0.1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C9	1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C10	0.1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C11	0.1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C12	0.1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C13	1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		C14	0.1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		D1	B130-E3	Diode:B130-E3	Diode_SMD:D_SMA_Handsoldering	http://www.vishay.com/docs/88946/b120.pdf
		D2	D_TVS	Device:D_TVS	Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		D3	D_TVS	Device:D_TVS	Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		D4	B130-E3	Diode:B130-E3	Diode_SMD:D_SMA_Handsoldering	http://www.vishay.com/docs/88946/b120.pdf
		D5	D_TVS	Device:D_TVS	Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		D6	SP0502BAHT DNP	Power_Protection:SP0502BAHT	Diode_SMD:Littelfuse_PolyZen-LS	http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf
		FB1	Ferrite_Bead_Small 330OHM	Device:Ferrite_Bead_Small	Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		FB2	Ferrite_Bead_Small 330OHM	Device:Ferrite_Bead_Small	Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		FB3	Ferrite_Bead_Small 330OHM	Device:Ferrite_Bead_Small	Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		J1	USB_B_Micro	Connector:USB_B_Micro	keyboard_parts:USB_microB	~
		J2	Conn_ARM_JTAG_SWD_10	Connector:Conn_ARM_JTAG_SWD_10	Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical	http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf
		J3	Conn_02x08_Counter_Clockwise	Connector_Generic:Conn_02x08_Counter_Clockwise	keebs:PinSocket_2x08_P2.54mm_Horizontal_Counter_Clockwise	~
		J4	Conn_02x08_Counter_Clockwise	Connector_Generic:Conn_02x08_Counter_Clockwise	keebs:PinSocket_2x08_P2.54mm_Horizontal_Counter_Clockwise	~
		J5	Conn_02x12_Counter_Clockwise	Connector_Generic:Conn_02x12_Counter_Clockwise	keebs:PinSocket_2x12_P2.54mm_Horizontal_Counter_Clockwise	~
		JP1	Jumper	Device:Jumper	Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical	~
		JP2	Jumper	Device:Jumper	Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical	~
		R1	77	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		R2	10	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		R3	10	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		R4	33	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		R5	33	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		R6	10M	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
		U1	NCP1117-3.3_SOT223	Regulator_Linear:NCP1117-3.3_SOT223	Package_TO_SOT_SMD:SOT-223-3_TabPin2	http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF
		U2	MKL27Z32VLH4	MCU_NXP_Kinetis:MKL27Z32VLH4	Package_QFP:LQFP-64_10x10mm_P0.5mm	http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf
		X1	XTAL 32kHz	keyboard_parts:XTAL	keebs:xtal_4.9x1.8mm	
		porRegSelect1	Jumper_NC_Dual	Device:Jumper_NC_Dual	Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical	~



Collated Components:

Item	Qty	Reference(s)	Value	LibPart	Footprint	Datasheet
1	2	C1, C2	10uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
2	2	C3, C4	12p	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
3	1	C5	2.2uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
4	1	C6	0.1uF DNP	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
5	3	C7, C9, C13	1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
6	5	C8, C10, C11, C12, C14	0.1uF	Device:CP	Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
7	2	D1, D4	B130-E3	Diode:B130-E3	Diode_SMD:D_SMA_Handsoldering	http://www.vishay.com/docs/88946/b120.pdf
8	3	D2, D3, D5	D_TVS	Device:D_TVS	Diode_SMD:D_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
9	1	D6	SP0502BAHT DNP	Power_Protection:SP0502BAHT	Diode_SMD:Littelfuse_PolyZen-LS	http://www.littelfuse.com/~/media/files/littelfuse/technical%20resources/documents/data%20sheets/sp05xxba.pdf
10	3	FB1, FB2, FB3	Ferrite_Bead_Small 330OHM	Device:Ferrite_Bead_Small	Inductor_SMD:L_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
11	1	J1	USB_B_Micro	Connector:USB_B_Micro	keyboard_parts:USB_microB	~
12	1	J2	Conn_ARM_JTAG_SWD_10	Connector:Conn_ARM_JTAG_SWD_10	Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical	http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf
13	2	J3, J4	Conn_02x08_Counter_Clockwise	Connector_Generic:Conn_02x08_Counter_Clockwise	keebs:PinSocket_2x08_P2.54mm_Horizontal_Counter_Clockwise	~
14	1	J5	Conn_02x12_Counter_Clockwise	Connector_Generic:Conn_02x12_Counter_Clockwise	keebs:PinSocket_2x12_P2.54mm_Horizontal_Counter_Clockwise	~
15	2	JP1, JP2	Jumper	Device:Jumper	Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical	~
16	1	R1	77	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
17	2	R2, R3	10	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
18	2	R4, R5	33	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
19	1	R6	10M	Device:R	Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder	~
20	1	U1	NCP1117-3.3_SOT223	Regulator_Linear:NCP1117-3.3_SOT223	Package_TO_SOT_SMD:SOT-223-3_TabPin2	http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF
21	1	U2	MKL27Z32VLH4	MCU_NXP_Kinetis:MKL27Z32VLH4	Package_QFP:LQFP-64_10x10mm_P0.5mm	http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf
22	1	X1	XTAL 32kHz	keyboard_parts:XTAL	keebs:xtal_4.9x1.8mm	
23	1	porRegSelect1	Jumper_NC_Dual	Device:Jumper_NC_Dual	Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical	~
