VUT Brno®

# Power Stage

Model of Power stage for Space Vector modulation

## Library

Electromechanical Drives

## Description

Simple model of three-phase topology of a power stage with six power switches.

## Data Type Support

The block of SRM accepts any numeric data type supported by Simulink software. Input control signal abc defined ON and OFF power switches. Output is three-phase voltage.

## Parameters and Dialog Box

Source DC voltage

  Enter the value of parameters or mark checkbox, if you want created new input insted of parameter.

## See Also

`Space Vector Modulation`