!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R2
!
boot-start-marker
boot-end-marker
!
!
vrf definition Mgmt-intf
 !
 address-family ipv4
 exit-address-family
 !
 address-family ipv6
 exit-address-family
!
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip domain name CCNPv8.CoPP.Lab
ip cef
login on-success log
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$/sQNIJgKslA4m1$MRILt1.KNTGBIEnojKUAyQJWdmxwKyRvpgoc19V9wIk
!
redundancy
!
!
ip tftp source-interface Ethernet2/1
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 ip address 172.16.12.2 255.255.255.252
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 no ip address
 shutdown
!
!
router eigrp 123
 network 172.16.12.0 0.0.0.3
 eigrp router-id 0.0.0.2
!
ip forward-protocol nd
!
!
no ip http server
ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^CR2: Lab Trouble Ticket 2^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
 stopbits 1
line aux 0
 stopbits 1
line vty 0 4
 login
 transport input telnet ssh
!
!
end
