!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$ng4e$UlUAq944rXIk50b.b/Qcc1
!
no aaa new-model
!
!
!
bsd-client server url https://cloudsso.cisco.com/as/token.oauth2
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
cts logging verbose
!
!
username admin privilege 15 secret 9 $9$xjzN6FL5t540E1$RS4/JK2ywx.sOmnE2/Bot1LtHJKOVeVOSRDR6mmYem6
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 no ip address
 ipv6 address FE80::1:4 link-local
 ipv6 address 2001:DB8:ACAD:226::1/64
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 ipv6 address FE80::1:1 link-local
 ipv6 address 2001:DB8:ACAD:192::1/64
 ospfv3 1 ipv6 area 0
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Serial2/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial2/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial3/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial4/1
 no ip address
 ipv6 address FE80::1:3 link-local
 ipv6 address 2001:DB8:ACAD:2001::1/64
 ipv6 traffic-filter BOGON-MARTIAN in
 serial restart-delay 0
!
interface Serial4/2
 no ip address
 ipv6 address FE80::1:2 link-local
 ipv6 address 2001:DB8:ACAD:2000::1/64
 ipv6 traffic-filter BOGON-MARTIAN in
 serial restart-delay 0
!
interface Serial4/3
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/0
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/1
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/2
 no ip address
 shutdown
 serial restart-delay 0
!
interface Serial5/3
 no ip address
 shutdown
 serial restart-delay 0
!
router ospfv3 1
 router-id 1.1.1.1
 !
 address-family ipv6 unicast
  default-information originate always
 exit-address-family
!
router bgp 15
 bgp router-id 1.1.1.1
 bgp log-neighbor-changes
 neighbor 2001:DB8:ACAD:227::1 remote-as 41
 neighbor 2001:DB8:ACAD:227::1 ebgp-multihop 3
 neighbor 2001:DB8:ACAD:227::1 update-source Loopback0
 !
 address-family ipv4
  no neighbor 2001:DB8:ACAD:227::1 activate
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:ACAD:192::/64
  network 2001:DB8:ACAD:224::/64
  network 2001:DB8:ACAD:225::/64
  neighbor 2001:DB8:ACAD:227::1 activate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
ipv6 route 2001:DB8:ACAD:227::/64 Serial4/1 2001:DB8:ACAD:2001::2
ipv6 route 2001:DB8:ACAD:227::/64 Serial4/2 2001:DB8:ACAD:2000::2
!
!
!
ipv6 access-list BOGON-MARTIAN
 permit ipv6 2001:DB8:ACAD:227::/64 any
 permit ipv6 2001:DB8:ACAD:16::/64 any
 permit ipv6 2001:DB8:ACAD:27::/64 any
 deny ipv6 2001:DB8:ACAD::/48 any
 permit ipv6 any any
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R1, Trouble Ticket 21.1.3.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 exec-timeout 5 0
 login local
 transport input telnet
!
!
end

