!
version 15.6
no service pad
service timestamps debug datetime msec
service timestamps log uptime
!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$Db3z$2bWPwxLptqxYr8pKj4zr91
!
aaa new-model
!
!
aaa authentication login default local
!
!
!
!
!
aaa session-id common
!
!
!
clock timezone EET 2 0
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

ip domain name ccnplab.local
ip cef
no ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$JwN3TAGsR3uuPW$3uaQ7g/cs0uS0d8JK6sZ5duHtp9TSSb3jWLZYdltTsQ
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback0
 no ip address
!
interface Ethernet0/0
 switchport
 switchport access vlan 10
 switchport mode access
 duplex auto
!
interface Ethernet0/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/1
 switchport
 switchport access vlan 10
 switchport mode access
 duplex auto
!
interface Ethernet1/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet1/3
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/1
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet2/3
 no ip address
 shutdown
 duplex auto
!
interface Vlan10
 ip address 10.10.10.2 255.255.255.0
!
ip default-gateway 10.10.10.1
ip forward-protocol nd
!
!
ip http server
ip http secure-server
!
ip access-list standard SNMP_ACL
 permit 10.10.10.10
!
!
snmp-server community ciscolab RO SNMP_ACL
snmp-server location snmp_manager
snmp-server contact ciscolab_admin
snmp-server enable traps snmp authentication linkdown linkup coldstart warmstart
snmp-server enable traps tty
snmp-server enable traps config-copy
snmp-server enable traps config
snmp-server enable traps config-ctid
snmp-server enable traps bridge newroot topologychange
snmp-server enable traps stpx inconsistency root-inconsistency loop-inconsistency
snmp-server enable traps syslog
snmp-server enable traps vtp
snmp-server enable traps vlancreate
snmp-server enable traps vlandelete
snmp-server host 10.10.10.11 version 2c ciscolab
!
!
!
!
control-plane
!
banner motd ^C This is D1, Trouble Ticket 23.1.3.1 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 transport input ssh
!
end

