!
version 15.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R2
!
boot-start-marker
boot-end-marker
!
!
enable secret 9 $9$dHNj02jhRWvMCK$xqxzQHD/KUBYeJ9W/7jL7apK7.h2.YYRH0JldVmJMjQ
!
no aaa new-model
clock timezone AFT 4 30
mmi polling-interval 60
no mmi auto-configure
no mmi pvc
mmi snmp-timeout 180
!
!
!
!
!
!
!
!


!
!
!
!
no ip domain lookup
ip domain name ENCOR.23
ip cef
ipv6 unicast-routing
ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
username admin privilege 15 secret 9 $9$WB.kVAuWm0MW54$FCx.xepQt1wu/1wjY1V4zrMOFoKnxfmpQEhuzWlvXAY
!
redundancy
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.224.1 255.255.255.255
 ipv6 address FE80::2:3 link-local
 ipv6 address 2001:DB8:224::1/64
!
interface Ethernet0/0
 no ip address
 shutdown
!
interface Ethernet0/1
 no ip address
 shutdown
!
interface Ethernet0/2
 no ip address
 shutdown
!
interface Ethernet0/3
 no ip address
 shutdown
!
interface Ethernet1/0
 no ip address
 shutdown
!
interface Ethernet1/1
 no ip address
 shutdown
!
interface Ethernet1/2
 no ip address
 shutdown
!
interface Ethernet1/3
 no ip address
 shutdown
!
interface Ethernet2/0
 no ip address
 shutdown
!
interface Ethernet2/1
 ip address 209.165.200.2 255.255.255.0
 ipv6 address FE80::2:1 link-local
 ipv6 address 2001:DB8:200::2/64
!
interface Ethernet2/2
 no ip address
 shutdown
!
interface Ethernet2/3
 ip address 209.165.201.2 255.255.255.0
 ipv6 address FE80::2:1 link-local
 ipv6 address 2001:DB8:201::2/64
!
interface Ethernet3/0
 no ip address
 shutdown
!
interface Ethernet3/1
 no ip address
 shutdown
!
interface Ethernet3/2
 no ip address
 shutdown
!
interface Ethernet3/3
 no ip address
 shutdown
!
router bgp 77
 bgp router-id 4.6.77.2
 bgp log-neighbor-changes
 no bgp default ipv4-unicast
 neighbor 2001:DB8:200::1 remote-as 138
 neighbor 2001:DB8:201::1 remote-as 138
 neighbor 209.165.200.1 remote-as 138
 neighbor 209.165.201.1 remote-as 138
 !
 address-family ipv4
  network 209.165.224.1 mask 255.255.255.255
  neighbor 209.165.200.1 activate
  neighbor 209.165.201.1 activate
 exit-address-family
 !
 address-family ipv6
  network 2001:DB8:224::/64
  neighbor 2001:DB8:200::1 activate
  neighbor 2001:DB8:201::1 activate
 exit-address-family
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
!
!
!
!
!
!
banner motd ^C This is R2, Trouble Ticket 23.1.4.3 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
 login local
line aux 0
line vty 0 4
 exec-timeout 0 0
 login local
 transport input telnet
!
!
end
