!
hostname D1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$MSuC$/ELyuYnPv.9Q6Lzeed57P1
!
no aaa new-model
!
!
!
clock timezone AFT 4 30
!
!
!
!
!
!
!
!
!
!
!


!
!
!
ip audit notify log
ip audit po max-events 100

no ip domain lookup
ip cef
no ipv6 cef
!
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
username admin privilege 15 secret 9 $9$V7sOpv1/VZd/p8$V8xpntTjE1kqckSbK2Fz0hv//bK0d1BHscnsMP3bCK6
!
vlan internal allocation policy ascending
!
!
!
!
!
interface Loopback0
 ip address 198.51.100.1 255.255.255.128
!
interface Ethernet0/0
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/1
 ip address 10.1.10.2 255.255.255.0
!
interface Ethernet0/2
 no ip address
 shutdown
 duplex auto
!
interface Ethernet0/3
 no ip address
 shutdown
 duplex auto
!
router ospf 1
 router-id 11.11.11.11
 redistribute connected subnets tag 110
 network 10.1.10.0 0.0.0.255 area 10
!
ip forward-protocol nd
!
!
no ip http server
no ip http secure-server
!
!
!
!
control-plane
!
banner motd ^C This is D1, Trouble Ticket 17.1.2.1 ^C
!
line con 0
 exec-timeout 0 0
 logging synchronous
line aux 0
line vty 0 4
 login
!
end
