RP/0/0/CPU0:ios#show running-config
Sat May 15 09:51:23.243 UTC
Building configuration...
!! IOS XR Configuration 6.0.1
!! Last configuration change at Thu May 13 17:41:51 2021 by cisco
!
interface MgmtEth0/0/CPU0/0
 shutdown
!
interface GigabitEthernet0/0/0/0
 ipv6 address 2001:db8:2284::22/64
 ipv6 enable
!
interface GigabitEthernet0/0/0/1
 ipv6 address 2001:db8:2234::2/64
 ipv6 enable
!
interface GigabitEthernet0/0/0/2
 ipv6 address 2001:db8:2222:123::1/64
 ipv6 enable
!
interface GigabitEthernet0/0/0/3
 shutdown
!
interface GigabitEthernet0/0/0/4
 shutdown
!
interface GigabitEthernet0/0/0/5
 shutdown
!
interface GigabitEthernet0/0/0/6
 shutdown
!
interface GigabitEthernet0/0/0/7
 shutdown
!
router ospfv3 1
 bfd multiplier 7
 bfd fast-detect
 bfd minimum-interval 6500
 router-id 2.2.2.2
 default-information originate always
 area 0
 !
 area 1
  interface GigabitEthernet0/0/0/1
  !
 !
 area 2
  interface GigabitEthernet0/0/0/2
  !
 !
 area 9.9.9.9
  interface GigabitEthernet0/0/0/0
   bfd fast-detect
  !
 !
 address-family ipv6 unicast
!
end