Run Main.mat

Main starts the GUI, which includes following functions:


alternat.mat - the alternating minimization algorithm
bluring.mat - the blurring function
noiseadd.mat - the noise adding function
sh_quality.mat - the sharpness evaluating function
cst_quality.mat - the contrast evaluating function

The real data and the test data are attached.




The real data description (aberrations meaning):

Data are divided in three folders according acquisition dwell time [us]
Image title consist of:

kx - magnification (275kx = 275 000x magnification)
ss - spot size (ss11 = the smallest spot size)
50um - aperture (50um = 50 um aperture width)
fine_tuning - describes system adjustment
last number is just serial number of image with given parameters