"Symbol";"Value";"Unit";
"TraceParts.PartNumber";"10-11072012-065358";"";
"TraceParts.ClassPath";"SCHNEIDER_ELECTRIC:/ROOT/C29/10-11072012-065358";"";
"TraceParts.InstanceId";"10-11072012-0653588TKLJWVV8B659XU7U1FL70VSJ";"";
"REFERENCE";"BMH1001P01A2A";"";
"TRACEPARTS";"TRACEPARTS";"";
"SUPPLIER";"Schneider Electric";"";
"DESIGN";"Lexium servo motor BMH with rotatable right-angled connectors, flange 100, peak IP54 untapped, without holding break and compatible with LXM32.D18N4";"";
"TraceParts.PartLanguage";"en";"";
"TraceParts.PartStatus";"Published";"";
"TraceParts.PartTitle";"Lexium servo motor BMH100 rotatable";"";
"TraceParts.PartVersion";"1.0.3";"";
