upgrade fpd auto
version 12.4
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname R3
!
boot-start-marker
boot-end-marker
!
security authentication failure rate 2 log
logging message-counter syslog
enable secret 5 $1$qq25$VbXGlYNz5IdZlEfD9DlhC1
!
aaa new-model
!
!
aaa authentication login default group tacacs+
aaa authentication login SSH-LOGIN group tacacs+
aaa authentication login CONSOLE line local
!
!
aaa session-id common
ip source-route
ip cef
!
!
!
!
no ip domain lookup
ip domain name lab.local
login block-for 300 attempts 2 within 120
no ipv6 cef
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
username admin privilege 15 secret 5 $1$ObG2$Ja2vj2X/HPUFZ7fWeB/n41
archive
 log config
  hidekeys
!
!
!
!
!
ip ssh maxstartups 3
ip ssh time-out 60
ip ssh authentication-retries 5
ip ssh version 2
!
!
!
!
interface FastEthernet0/0
 ip address 10.0.1.2 255.255.255.252
 duplex auto
 speed auto
!
interface FastEthernet0/1
 no ip address
 shutdown
 duplex auto
 speed auto
!
interface FastEthernet1/0
 ip address 32.10.0.65 255.255.255.252
 ip ospf authentication message-digest
 duplex auto
 speed auto
!
interface FastEthernet1/1
 ip address 10.112.63.130 255.255.255.252
 ip ospf authentication message-digest
 duplex auto
 speed auto
!
router ospf 1
 router-id 10.112.63.128
 log-adjacency-changes
 passive-interface FastEthernet0/0
 network 10.0.1.0 0.0.0.3 area 0
 network 10.112.63.128 0.0.0.3 area 0
 network 32.10.0.64 0.0.0.3 area 0
!
ip forward-protocol nd
ip route 0.0.0.0 0.0.0.0 10.112.63.129
ip route 0.0.0.0 0.0.0.0 32.10.0.66 2
no ip http server
no ip http secure-server
!
!
!
!
logging trap notifications
logging 192.168.11.10
no cdp run

!
!
!
!
!
tacacs-server host 192.168.11.10
!
control-plane
!
!
!
!
!
!
!
gatekeeper
 shutdown
!
!
line con 0
 exec-timeout 30 0
 logging synchronous
 login authentication CONSOLE
 stopbits 1
line aux 0
 no exec
 stopbits 1
line vty 0 4
 exec-timeout 30 0
 logging synchronous
 login authentication SSH-LOGIN
 transport input ssh
!
end
