<!DOCTYPE html
  PUBLIC "-//W3C//DTD HTML 4.01 Transitional//EN" "http://www.w3.org/TR/1999/REC-html401-19991224/loose.dtd">
<html lang="en"><head>
      <meta http-equiv="Content-Type" content="text/html; charset=utf-8">
   <title>SWEPEXDCM :: Blocks (Simulink&reg;)</title>
  <meta http-equiv="Content-Script-Type" content="text/javascript"><script language="JavaScript" src="docscripts.js"></script></head>
<body><a name="top_of_page"></a>
  <b>VUT Brno<sup>&reg;</sup></b>
  <h1 class="reftitle">SWDCM</h1>
    <p>Model of Series-wound DC Motor</p>
    
  <h2>Library</h2>
    <p>Electromechanical Drives</p>
    
  <h2>Description <span class="inlinemediaobject"></span></h2>
    <img src="PMDCM_Blocks.png" alt="">
    <p>Model of Series-wound DC Motor is in the five variants, created by </p>
    <ul type="disc">
        <li><p>Simulink blocks (SEPEX DC Motor Block)</p></li>
        <li><p>S-function Lvel-2 in language C as continous (SEPEX DC Motor continous)</p></li>
        <li><p>S-function Lvel-2 in language C as discrete (SEPEX DC Motor discrete)</p></li>
        <li><p>S-function Lvel-2 in language M as continous (SEPEX DC Motor continous)</p></li>
        <li><p>S-function Lvel-2 in language M as discrete (SEPEX DC Motor discrete)</p></li>
    </ul>
    
  <h2>Data Type Support</h2>
    <p> The block of SEPEX DC Motor accepts only one dimension input signals and any numeric data type supported by Simulink software.</p>
  
  <h2>Parameters and Dialog Box</h2>
    <p><img src="SEPEXDCM_Main.png" alt=""></p>
    <dl>
        <dt><span class="term"><b>Input parameters</b></span></dt>
            <dd><p>Enter the value of parameters or mark checkbox, if you want created new input insted of parameter.</p></dd>
        <dt><span class="term"><b>Sample time (Only in discrete type of model)</b></span></dt>
            <dd><p>Enter the time interval between sample time hits. Model use Euler method.</p></dd>
        <dt><span class="term"><b>Buttons <i>Field winding inductance</i> and <i>Magnetic Flux</i></b></span></dt>
            <dd><p>This button is define functionality this parameters in new window. Parameter can be define by</p></dd>
             <ul type="disc">
                <dd><li><p>Table from workspace or from Mat-file. </p></li></dd>
                <dd><li><p>Constant value</p></li></dd>
                <dd><li><p>New input</p></li></dd>
             </ul>
            <dd><img src="SEPEXDCM_Buttons.png"  alt=""></dd>
            <dd><p>Table describes parameter as function of field winding current. Table can be defined by rows or columns. First row or column contains data of field winding current. Second row or column contains functions value of field winding current. If table is loaded from Mat-file, then Mat-file must be in the current directory. Linear interpolation is used for estimation actual values.</p></dd>
        <dt><span class="term"><b>Non zeros initial conditions</b></span></dt>
            <dd><p>After this button is clicked, new window is opened. Enter the value of initial state variables. Default values of initial conditions are set to zero.</p></dd>
            <dd><img src="SEPEXDCM_IC.png"  alt=""></dd>
        <dt><span class="term"><b>Output paramters</b></span></dt>
            <dd><p>You may add another outputs to block.</p></dd>
    </dl>
    
  <h2>Table of model parameters</h2>
    <img src="SEPEXDCM_Table.png" alt="">
        
  <h2>Mathematical model</h2>
    <img src="SEPEXDCM_eq.bmp" alt="">
     
  <h2>See Also</h2>
    <p><a href="PMDCM_Help.html"><tt>PMDCM</tt></a>, <a href="SWDCM_Help.html"><tt>Series-wound DC Motor</tt></a>, <a href="PMSM_Help.html"><tt>PMSM</tt></a></p>
   
</body></html>
  <!-- Last updated: 20 May 2010 -->