EMMA Coverage Report (generated Tue Dec 18 20:38:46 CET 2007)
[all classes][cz.vutbr.feec.packets.rtp]

## COVERAGE SUMMARY FOR SOURCE FILE [PayloadConstants.java]

name | class, % | method, % | block, % | line, %
--- | --- | --- | --- | ---
PayloadConstants.java | 0% (0/1) | 0% (0/1) | 0% (0/3) | 0% (0/1)

### COVERAGE BREAKDOWN BY CLASS AND METHOD

name | class, % | method, % | block, % | line, %
--- | --- | --- | --- | ---
class PayloadConstants | 0% (0/1) | 0% (0/1) | 0% (0/3) | 0% (0/1)
PayloadConstants (): void |  | 0% (0/1) | 0% (0/3) | 0% (0/1)

1 | package cz.vutbr.feec.packets.rtp;
2 |
3 | /**
4 | * This class provides constants associated with RTCP Packets -similar to those defined
5 | * in rtp.h
6 | */
7 |
8 | public class PayloadConstants extends Object
9 | {
10 | /*
11 | * RTP PACKET CONSTANTS
12 | */
13 | /** Version =2. */
14 | public static final byte VERSION = 2;
15 |
16 | /** Padding =0. */
17 | public static final byte PADDING = 0;
18 |
19 | /** Marker =0. */
20 | public static final byte MARKER = 0;
21 |
22 | /** EXTENSION =0. */
23 | public static final byte EXTENSION = 0;
24 |
25 | /** payload types =0. */
26 | public static final byte RTP_PAYLOAD_PCMU = 0;
27 |
28 | /** The Constant RTP_PAYLOAD_1016. */
29 | public static final byte RTP_PAYLOAD_1016 = 1;
30 |
31 | /** The Constant RTP_PAYLOAD_G721. */
32 | public static final byte RTP_PAYLOAD_G721 = 2;
33 |
34 | /** The Constant RTP_PAYLOAD_GSM. */
35 | public static final byte RTP_PAYLOAD_GSM = 3;
36 |
37 | /** The Constant RTP_PAYLOAD_G723. */
38 | public static final byte RTP_PAYLOAD_G723 = 4;
39 |
40 | /** The Constant RTP_PAYLOAD_DVI4_8k. */
41 | public static final byte RTP_PAYLOAD_DVI4_8k = 5;
42 |
43 | /** The Constant RTP_PAYLOAD_DVI4_16k. */
44 | public static final byte RTP_PAYLOAD_DVI4_16k= 6;
45 |
46 | /** The Constant RTP_PAYLOAD_LPC. */
47 | public static final byte RTP_PAYLOAD_LPC = 7;
48 |
49 | /** The Constant RTP_PAYLOAD_PCMA. */
50 | public static final byte RTP_PAYLOAD_PCMA = 8;
51 |
52 | /** The Constant RTP_PAYLOAD_H263. */
53 | public static final byte RTP_PAYLOAD_H263 = 34;
54 |
55 |
56 | /*
57 | * RTCP TYPES
58 | */
59 | /** RTCP Sender Report Packet (SR) = 200. */
60 | public static final int RTCP_SR = (int) 200;
61 |
62 | /** RTCP Receiver Report Packet (RR) = 201. */
63 | public static final int RTCP_RR = (int) 201;
64 |
65 | /** RTCP Source Description Packet (SDES) = 202. */
66 | public static final int RTCP_SDES = (int) 202;
67 |
68 | /** RTCP BYE Packet = 203. */
69 | public static final int RTCP_BYE = (int) 203;
70 |
71 | /** RTCP APP Packet = 204. */
72 | public static final int RTCP_APP = (int) 204;
73 |
74 | /** RTCP RSI Packet = 204. */
75 | public static final int RTCP_RSI = (int) 208;
76 |
77 |
78 | /** The Constant RTP_DATA. */
79 | public static final int RTP_DATA = (int) 0;
80 |
81 | /*
82 | * SDES TYPES
83 | */
84 |
85 | /** End SDES Item =0. */
86 | public static final byte RTCP_SDES_END = (byte) 0;
87 |
88 | /** Canonical end - point identifier SDES Item =1. */
89 | public static final byte RTCP_SDES_CNAME = (byte) 1;
90 |
91 | /** User Name SDES Item = 2. */
92 | public static final byte RTCP_SDES_NAME = (byte) 2;
93 |
94 | /** Electronic mail address SDES Item =3. */
95 | public static final byte RTCP_SDES_EMAIL = (byte) 3;
96 |
97 | /** Phone number SDES Item = 4. */
98 | public static final byte RTCP_SDES_PHONE = (byte) 4;
99 |
100 | /** Geographic user location SDES Item = 5. */
101 | public static final byte RTCP_SDES_LOC = (byte) 5;
102 |
103 | /** Application or tool name SDES Item = 6. */
104 | public static final byte RTCP_SDES_TOOL = (byte) 6;
105 |
106 | /** Notice or status SDES Item = 7. */
107 | public static final byte RTCP_SDES_NOTE = (byte) 7;
108 |
109 | /** Private extensions SDES Item = 8. */
110 | public static final byte RTCP_SDES_PRIV = (byte) 8;
111 |
112 | }

[all classes][cz.vutbr.feec.packets.rtp]
EMMA 2.0.5312 EclEmma Fix 1 (C) Vladimir Roubtsov