Sonochan II 0.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
S_usb_endpoint_audio_descriptor_1 Struct Reference

Usb Audio Endpoint Descriptor. More...

`#include <usb_descriptors.h>`

## Data Fields
U8 | bLength
| Size of this descriptor in bytes. More...
U8 | bDescriptorType
| ENDPOINT descriptor type. More...
U8 | bEndpointAddress
| Address of the endpoint. More...
U8 | bmAttributes
| Endpoint's attributes. More...
U16 | wMaxPacketSize
| Maximum packet size for this EP. More...
U8 | bInterval
| Interval for polling EP in ms. More...
U8 | bRefresh
U8 | bSynAddress

## Detailed Description

Usb Audio Endpoint Descriptor.

## Field Documentation

U8 S_usb_endpoint_audio_descriptor_1::bDescriptorType

ENDPOINT descriptor type.

U8 S_usb_endpoint_audio_descriptor_1::bEndpointAddress

Address of the endpoint.

U8 S_usb_endpoint_audio_descriptor_1::bInterval

Interval for polling EP in ms.

U8 S_usb_endpoint_audio_descriptor_1::bLength

Size of this descriptor in bytes.

U8 S_usb_endpoint_audio_descriptor_1::bmAttributes

Endpoint's attributes.

U8 S_usb_endpoint_audio_descriptor_1::bRefresh

U8 S_usb_endpoint_audio_descriptor_1::bSynAddress

U16 S_usb_endpoint_audio_descriptor_1::wMaxPacketSize

Maximum packet size for this EP.

The documentation for this struct was generated from the following file:

- /mnt/data/GENTOO_FILES/home/k1ll3r/Dokumenty/Diplomka/Sonochan_II/FW_sdr_widget/sdr-widget/src/usb_descriptors.h