# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/FAIR_RARE.ppg"
;****************************************************************
;
; Copyright (c) 2002
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; All Rights Reserved
;
; a RARE imaging experiment
;
;****************************************************************
;
;
; d0 - TR padding
; d1, d2  - TE padding
; d3 = PVM_GradDelayTime
; d4 = PVM_RampTime
; d8 = CONFIG_amplifier_enable

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/MRI.include" 1
;****************************************************************
;
; $Source: /pv/CvsTree/pv/gen/src/prg/methManag/PPG/MRI.include,v $
;
; Copyright (c) 2006
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; All Rights Reserved
;
;;****************************************************************
;MRI.include

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/Avance.incl" 1
;Avance3.incl
;   for AVi
;
;avance-version (07/01/22)
;
;$CLASS=HighRes Incl
;$COMMENT=












































































































































;$Id: Avance3.incl,v 1.3.2.4 2007/08/20 07:14:40 pfre Exp $
# 14 "/opt/PV5.1/exp/stan/nmr/lists/pp/MRI.include" 2


define delay aqq
define delay deparx
define delay derxadc
define delay rdepa

"aqq=dw*td"
"rdepa=de-depa"
"deparx=depa-derx"
"derxadc=derx-deadc"











































# 86 "/opt/PV5.1/exp/stan/nmr/lists/pp/MRI.include"






# 20 "/opt/PV5.1/exp/stan/nmr/lists/pp/FAIR_RARE.ppg" 2

preset off

define delay d3enab
"d3enab = d3 - de"

define loopcounter lc1
"lc1 = ds"

define list<delay> vd1 = {$VdList1}
define list<delay> vd2 = {$VdList2}

define list<frequency> fq2list = {$ACQ_O2_list}

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 1
;****************************************************************
;
; Copyright (c) 2003-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: PrepModulesHead.mod,v 1.14.2.1 2007/07/02 13:05:36 mawi Exp $
;
; All Rights Reserved
;
; Declaration of pulseprogram parameters and subroutines for 
; preparation  modules
;
;****************************************************************

;**** Fat Suppression Module ****

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/FatSupDef.mod" 1
;****************************************************************
;
; Copyright (c) 2002-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: FatSupDef.mod,v 1.1.2.2 2007/07/02 14:26:25 mawi Exp $
;
; All Rights Reserved
;
; FatSupDef.mod : Declaration of Fat Suppression Subroutine
;
;****************************************************************

if(PVM_FatSupOnOff)
{
define list<frequency> modlis6 = {$PVM_FatSupFL}
define delay FsD0 = {$PVM_FsD0}
define delay FsD1 = {$PVM_FsD1}
define delay FsD2 = {$PVM_FsD2}

define pulse FsP0 = {$PVM_FsP0}
}

















# 18 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2


;**** Flow Saturation Module ****

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/FlowSatDef.mod" 1
;****************************************************************
;
; Copyright (c) 2005-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: FlowSatDef.mod,v 1.1.4.2 2007/07/02 13:26:58 mawi Exp $
;
; All Rights Reserved
;
; FlowSatDef.mod: Declaration of subroutines for Flow Saturation 
; call
; subr FlowSat()
; subr FlowSatInit()
; subr FlowSatInc()
; 
;****************************************************************

if(PVM_InFlowSatOnOff == 1)
   {
define list<frequency> modlis4 = {$PVM_InFlowSatFL}
define delay SfD0 = {$PVM_SfD0}
define delay SfD1 = {$PVM_SfD1}
define delay SfD2 = {$PVM_SfD2}

define pulse SfP0 = {$PVM_SfP0}

define loopcounter SfLp0 = {$PVM_SfLp0}
   }










































# 22 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2


;**** Inversion Pulse Module ****
# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/InvPulseDef.mod" 1
;****************************************************************
;
; Copyright (c) 2002-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: InvPulseDef.mod,v 1.1.2.2 2007/07/02 14:26:25 mawi Exp $
;
; All Rights Reserved
;
; InvPulseDef.mod : Declaration of Inversion Pulse subroutine
;
; call
; subr InvPulse()
;
;****************************************************************
;   
;       PVM_InvRFPulseArr      :  
;     
;       sp22            TPQQ[14].name : PVM_InvRFPulsePropertyArr[0].Filename
;
;       PVM_IpP0                      :  PVM_InvRFPulseArr[0].PulseLength
;
;       PVM_IpD2                      :  PVM_InvPulseDelay[0]
;       PVM_IpD3                      :  PVM_InvPulseSpoilTime[0]
;       PVM_IpD1                      :  CONFIG_amplifier _enable
;       PVM_IpD0                      :  PVM_RampTime
;

if(PVM_InvPulseOnOff == 1)
{
define list<frequency>  modlis2= {$PVM_InvPulseOffsetHz}
define delay IpD0 = {$PVM_IpD0}
define delay IpD1 = {$PVM_IpD1}
define delay IpD2 = {$PVM_IpD2}
define delay IpD3 = {$PVM_IpD3}

define pulse IpP0 = {$PVM_IpP0}
}




















# 25 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2


;**** Magnetisation Transfer Module ****

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/MagTransDef.mod" 1
;****************************************************************
; $Source: /pv/CvsTree/pv/gen/src/prg/methManag/PPG/MagTransDef.mod,v $
;
; Copyright (c) 2005-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; All Rights Reserved
;
; MagTransDef.mod: Declaration of subroutine for Magnetization 
;                  transfer 
; call
; subr MagTrans()
;
; $Id: MagTransDef.mod,v 1.1.2.3 2008/06/05 17:10:28 mawi Exp $
;****************************************************************
;**** Magnetisation Transfer Module ****


if(PVM_MagTransOnOff)
{
define list<frequency> modlis3 = {$PVM_MagTransFL} 
define delay MtD0 = {$PVM_MtD0}
define delay MtD1 = {$PVM_MtD1}
define delay MtD2 = {$PVM_MtD2}
define delay MtD3 = {$PVM_MtD3}

define pulse MtP0 = {$PVM_MtP0}

define loopcounter MtLp0 = {$PVM_MtLp0}
}


















# 29 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2



;**** Saturation Pulse Module ****

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/SatPulseDef.mod" 1
;****************************************************************
;
; Copyright (c) 2002-2003
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: SatPulseDef.mod,v 1.1.2.3 2009/02/25 09:35:00 fhen Exp $
;
; All Rights Reserved
;
; SatPulseDef.mod : Declaration of Saturation Pulse subroutines
; call 
; subr SatPulse()
;
;****************************************************************
;   
;    PVM_SatRFPulseArr      :  
;     
;       sp28            DPQQ[12].name : PVM_SatRFPulsePropertyArr[0].Filename
;       sp29            DPQQ[13].name : PVM_SatRFPulsePropertyArr[1].Filename
;       sp30            DPQQ[14].name : PVM_SatRFPulsePropertyArr[2].Filename
;       sp31            DPQQ[15].name : PVM_SatRFPulsePropertyArr[3].Filename
;
;       PVM_SpP0                     :  PVM_SatRFPulseArr[0].PulseLength
;       PVM_SpP1                     :  PVM_SatRFPulseArr[1].PulseLength
;       PVM_SpP2                     :  PVM_SatRFPulseArr[2].PulseLength
;       PVM_SpP3                     :  PVM_SatRFPulseArr[3].PulseLength
;
;       PVM_SpD2                     :  PVM_SatPulseDelay1[0]
;       PVM_SpD6                     :  PVM_SatPulseSpoilTime[0]
;       PVM_SpD10                    :  PVM_SatPulseDelay2[0]
;       PVM_SpD3                     :  PVM_SatPulseSpoilTime[1]
;       PVM_SpD7                     :  PVM_SatPulseDelay1[1]
;       PVM_SpD11                    :  PVM_SatPulseDelay2[1]
;       PVM_SpD4                     :  PVM_SatPulseDelay1[2]
;       PVM_SpD8                     :  PVM_SatPulseSpoilTime[2]
;       PVM_SpD12                    :  PVM_SatPulseDelay2[2]
;       PVM_SpD5                     :  PVM_SatPulseDelay1[3]
;       PVM_SpD9                     :  PVM_SatPulseSpoilTime[3]
;       PVM_SpD13                    :  PVM_SatPulseDelay2[3]
;

if(PVM_SatPulseOnOff == 1)
   {
define list<frequency> modlis7 = {$PVM_SatPulseOffsetHz}

define delay SpD0 = {$PVM_SpD0}
define delay SpD1 = {$PVM_SpD1}
define delay SpD2 = {$PVM_SpD2}
define delay SpD3 = {$PVM_SpD3}
define delay SpD4 = {$PVM_SpD4}
define delay SpD5 = {$PVM_SpD5}
define delay SpD6 = {$PVM_SpD6}
define delay SpD7 = {$PVM_SpD7}
define delay SpD8 = {$PVM_SpD8}
define delay SpD9 = {$PVM_SpD9}
define delay SpD10 = {$PVM_SpD10}
define delay SpD11 = {$PVM_SpD11}
define delay SpD12 = {$PVM_SpD12}
define delay SpD13 = {$PVM_SpD13}
define pulse SpP0 = {$PVM_SpP0}
define pulse SpP1 = {$PVM_SpP1}
define pulse SpP2 = {$PVM_SpP2}
define pulse SpP3 = {$PVM_SpP3}

   }




























































# 34 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2



;*** Saturation Slices Module ***

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/SatSliceDef.mod" 1
;****************************************************************
;
; Copyright (c) 2002-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: SatSliceDef.mod,v 1.2.2.1 2007/07/02 13:01:13 mawi Exp $
;
; All Rights Reserved
;
; SatSlices.mod : Declaration of Saturation Slice subroutine
; call
; subr SatSlices()
;
;****************************************************************
;
; SaturationSlicesPulse :
;
;        sp25              DPQQ[9].name : PVM_SatSlicesPulse.Filename
;        PVM_SatP0                     : PVM_SatSlicesPulse.Length
;
;        
;        PVM_SatD1                     : CONFIG_amplifier_enable
;        PVM_SatD0                     : PVM_RampTime
;        PVM_SatD2                     : PVM_FovSatSpoilTime
;        PVM_SatLp0                    : PVM_FovSatNSlices 
;
;**** Saturation Slice Module ****
if(PVM_FovSatOnOff == 1)
{
define list<frequency> modlis5 = {$PVM_FovSatFL}
define delay SatD0 = {$PVM_SatD0}
define delay SatD1 = {$PVM_SatD1}
define delay SatD2 = {$PVM_SatD2}

define pulse SatP0 = {$PVM_SatP0}

define loopcounter SatLp0 = {$PVM_SatLp0}
}























 
# 39 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2



;**** Black Blood Module ****
# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/BlBloodDef.mod" 1
;****************************************************************
;
; Copyright (c) 2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: BlBloodDef.mod,v 1.1.2.2 2007/07/02 14:26:25 mawi Exp $
;
; All Rights Reserved
;
; BlBloodDef.mod : Declaration of Black blood  subroutine
;
; call
; subr BlBlood(ph0) : Black blood preparation with RF phaselist
;                     ph0
;
;****************************************************************

if(PVM_BlBloodOnOff)
  {
define list<frequency> modlis8 = {$PVM_BlBloodFL}
define delay BlbD0 = {$PVM_BlbD0}
define delay BlbD1 = {$PVM_BlbD1}
define delay BlbD2 = {$PVM_BlbD2}
define delay BlbD3 = {$PVM_BlbD3}

define pulse BlbP0 = {$PVM_BlbP0}
  }
























# 43 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2



;**** Trigger Module ****
define delay TrigD0 = {$PVM_TrigD0}
;**** Trigger Out Module ****
define delay TrigOutD0 = {$PVM_TrigOutD0}

;**** OuterVolumeSuppression **** Solvent Suppression Module ****

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/WsOvsDef.mod" 1
;****************************************************************
;
; Copyright (c) 2005-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: WsOvsDef.mod,v 1.1.2.3 2008/03/19 14:25:28 sako Exp $
;
; All Rights Reserved
;
; WsOvsDef.mod: Declaration of water suppression and Outer 
;               volume suppression subroutines
;
; call 
; subr Ovs(ph0) ;  execution of OVS with ph0 phaselist
;
; subr WsOvs(ph0,ph1) : execution of OVS with ph0 and WS with ph1
;                       phaselist
;****************************************************************

;**** OuterVolumeSuppression ****

if(PVM_OvsOnOff == 1)
{
define list<frequency> Ovslist={$PVM_OvsFrequencyList}
define delay OvsD0 = {$PVM_OvsD0}
define delay OvsD1 = {$PVM_OvsD1}
define pulse OvsP0 = {$PVM_OvsP0}
}





























;*** WaterSuppression Module with OVS ****

if (PVM_WsMode)
{

define list<frequency> Wslist={$PVM_WsOffsetHz}
define pulse WsP0 = {$PVM_WsP0}
define pulse WsP1 = {$PVM_WsP1}
define pulse WsP2 = {$PVM_WsP2}
define delay WsNp0 
"WsNp0 = WsP0"
define delay WsNp1 
"WsNp1 = WsP1"
define delay WsNp2 
"WsNp2 = WsP2"
define list<delay> ChD1={$PVM_ChppgD1}
define list<delay> ChD2={$PVM_ChppgD2}
define list<delay> VpD1={$PVM_VpppgD1}
define list<delay> VpD2={$PVM_VpppgD2}

}
















































































































































































# 53 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2


;**** Solvent Suppression module and FOV Saturation module ******

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/WsSatDef.mod" 1
;******************************************************************
;
; Copyright (c) 2002-2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: WsSatDef.mod,v 1.1.2.2 2007/07/02 14:26:26 mawi Exp $ 
;
; All Rights Reserved
;
; WsSatDef.mod - Declaration of water suppression and FOV saturation 
;                subroutines
; call
; subr WsSat(ph0) : execution of WS with ph0 phaselist and 
;                   FOV saturation (as passed as argument)    
;      
;*******************************************************************



















































































































































































# 57 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2


;*********** selective inversion recovery **********

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/SelSliceIrDef.mod" 1
;****************************************************************
;
; Copyright (c) 2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: SelSliceIrDef.mod,v 1.1.2.2 2007/07/02 14:26:25 mawi Exp $
;
; All Rights Reserved
;
; SelSliceIrDef.mod : declaration of slice Selective Inversion 
;                     Recovery subroutine
; call SliceSelIr()
; 
;
;****************************************************************


if(PVM_SelIrOnOff)
  {
define list<frequency> IrFL = {$PVM_SelIrFL} 
define delay IrD0 = {$PVM_SelIrD0}
define delay IrD1 = {$PVM_SelIrD1}
define delay IrD2 = {$PVM_SelIrD2}
define delay IrD3 = {$PVM_SelIrD3}
define delay IrD4 = {$PVM_SelIrD4}

define pulse IrP0 = {$PVM_SelIrP0}

define loopcounter IrL0 = {$PVM_SelIrL0}
  }



















# 61 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2


;***********Tagging*****************

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/TagDef.mod" 1
;****************************************************************
;
; Copyright (c) 2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: TagDef.mod,v 1.1.2.4 2008/06/05 17:09:32 mawi Exp $
;
; All Rights Reserved
;
; TagDef.mod : Declaration of tagging subroutine
; call
; subr Tagging()
;
;****************************************************************

if(PVM_TaggingOnOff)
{
define list<frequency> taggfreq={$PVM_TaggingFL}

define delay TaggD0 = {$PVM_TaggingD0}
define delay TaggD1 = {$PVM_TaggingD1}
define delay TaggD2 = {$PVM_TaggingD2}
define delay TaggD3 = {$PVM_TaggingD3}
define delay TaggD4 = {$PVM_TaggingD4}
define delay TaggD5 = {$PVM_TaggingD5}

define pulse TaggP0 = {$PVM_TaggingP0}
define loopcounter TaggL0 = {$PVM_TaggingLp0}
}


























































# 65 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2


;*********** Noe *******************

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/NoeDef.mod" 1
;****************************************************************
;
; Copyright (c) 2007
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; $Id: NoeDef.mod,v 1.1.2.2 2007/07/02 14:26:26 mawi Exp $
;
; All Rights Reserved
;
; NoeDef.mod: Declaration of Nuclear Overhouser Enhancement 
;             subroutine
; call
; subr Noe()
;
;****************************************************************

if(PVM_NoeOnOff == On)
{
define delay NoeD0 = {$PVM_NoeD0}
define delay NoeD1 = {$PVM_NoeD1}
}





















# 69 "/opt/PV5.1/exp/stan/nmr/lists/pp/PrepModulesHead.mod" 2




define loopcounter EvolLp0 = {$PVM_EvolLp0}
define list<delay> EvolD0 = {$PVM_EvolD0}


# 34 "/opt/PV5.1/exp/stan/nmr/lists/pp/FAIR_RARE.ppg" 2

fq1b receive				     	     \n if (CONFIG_instrument_type != Avance_I)           \n {                                                 \n dccorr                                         \n }                         \n if (CONFIG_preemp_type == GREAT_60)               \n {                                                 \n if (CONFIG_instrument_type != Avance_III)      \n {                                              \n 500m setnmr0|34|33|32                          \n }                                              \n else                                           \n {                                              \n 200u setnmr0|34|33|32                          \n }                                              \n }                                                 \n if (CONFIG_preemp_type == DPP_with_SW_Blanking)   \n {                                                 \n 10u ctrlgrad 0                                 \n 10u grad{(0)|(0)|(0) }			     \n 200u setnmr0|34|33|32                          \n }


if( ACQ_dim >=2 )
{
  lgrad r2d<2d> = ACQ_size[1]
  zgrad r2d
}
if( ACQ_dim >= 3)
{
  lgrad r3d<3d> = ACQ_size[2]
  zgrad r3d
}

lgrad slice = NSLICES
zslice
zgrad r2d

;pre-setting the r2d counter for the dummy scans:
decr,   dgrad r2d
        lo to decr times l1	;DS*ACQ_rare_factor
        dgrad r2d		; because igrad is done before gc_control

start,  10u	sgrad r2d
	d0	

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/TriggerPerPhaseStep.mod" 1
;****************************************************************
;
; Copyright (c) 1998-2003
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; All Rights Reserved
;
; TriggerPerPhaseStep.mod - Trigger Module
;
;****************************************************************
;
;      PVM_TrigD0               --> PVM_EcgTriggerModuleTime = ACQ_trigger_delay
;
if (PVM_TriggerMode == per_PhaseStep)
{
if (ACQ_trigger_enable == 1)
{
  10u   setnmr3|6
if (CONFIG_instrument_type == Avance_III)
{
  10u   trignl1
  10u   trigpe3
}
else
{
  10u   trigpl1
}
  10u   setnmr3^6
  TrigD0
}
}
# 61 "/opt/PV5.1/exp/stan/nmr/lists/pp/FAIR_RARE.ppg" 2


	d4     grad{(0)|(0)|PVM_ppgGradAmpArray1(100)} fq2list:f1 ; variable inv slab sel gradient
	d3                                       
	d3                  
	d8     gatepulse 1
	p2:sp2 ph0
	d11    grad{(0)|(0)|(t5)} ; spoiler
	vd1    groff              ; ir delay

slice,  10u	fq8b:f1

# 1 "/opt/PV5.1/exp/stan/nmr/lists/pp/TriggerPerSlice.mod" 1
;****************************************************************
;
; Copyright (c) 1998-2003
; Bruker BioSpin MRI GmbH
; D-76275 Ettlingen, Germany
;
; All Rights Reserved
;
; TriggerPerSlice.mod - Trigger Module
;
;****************************************************************
;
;     PVM_TrigD0               --> PVM_EcgTriggerModuleTime = ACQ_trigger_delay
;
if (PVM_TriggerMode == per_Slice)
{
if (ACQ_trigger_enable == 1)
{
  10u   setnmr3|6
if (CONFIG_instrument_type == Avance_III)
{
  10u   trignl1
  10u   trigpe3
}
else
{
  10u   trigpl1
}
  10u   setnmr3^6 
  TrigD0
}
}
# 73 "/opt/PV5.1/exp/stan/nmr/lists/pp/FAIR_RARE.ppg" 2


;----------------------------------preparation modules -------------
;EXEC_begin SatSlices line 1565 (76) SatSlices()
 
if(PVM_FovSatOnOff == 1)  
{
lgrad PVM_FovSatGrad = PVM_FovSatNSlices
lgrad PVM_FovSatSpoiler = 1
zgrad PVM_FovSatGrad
zgrad PVM_FovSatSpoiler

        50u     modlis5.res

fov9,    SatD0 	modlis5:f1   	grad{PVM_FovSatGrad(100,,direct_scale)|(0)|(0)}
        SatD1   gatepulse 1
        SatP0:sp25          
        SatD2   modlis5.inc	grad{(0)|(0)|PVM_FovSatSpoiler(100,,no_scale)}
        igrad PVM_FovSatGrad
       lo to fov9 times SatLp0
        SatD0	        	grad{(0)|(0)|(0)}
        20u
}
   
;EXEC_end   SatSlices line 1565 (76) SatSlices()
;EXEC_begin MagTrans line 1566 (77) MagTrans()
 

  if(PVM_MagTransOnOff)
  {
 
      50u  modlis3.res
      MtD1 gatepulse 1
mtc10,MtD2 modlis3:f1
      MtP0:sp27 
      lo to mtc10 times MtLp0
      MtD3  		grad{(0)|(0)|PVM_MagTransSpoiler(100,,no_scale)}
      MtD0       	groff
      100u
  }
 
;EXEC_end   MagTrans line 1566 (77) MagTrans()
;EXEC_begin FatSup line 1567 (78) FatSup()
 
if(PVM_FatSupOnOff)
{
lgrad PVM_FatSupSpoiler = 1
10u zgrad PVM_FatSupSpoiler

40u       modlis6:f1
1m        gatepulse 1
FsP0:sp26    
FsD2     grad{(0)|(0)|PVM_FatSupSpoiler(100,,no_scale)}
FsD0      groff
50u
}

 
;EXEC_end   FatSup line 1567 (78) FatSup()
 
        10u     fq1:f1
        d1	grad {(0)|(0)|(t4)}  ; spoiler
        d4      grad {(0)|(0)|(t0)}  ; slice grad
        d8	gatepulse 1          ; grad stabilizing (min=CFG_TransmitterEnable())
	p0:sp0 	ph0
        d2      grad {(t2)|(0)|(t1)} ; dephasing
        d14     grad {(0) |(0)|(t3)} ; slice grad
echo1,  0u      rgrad r2d
echo,   d8      gatepulse 1
        p1:sp1 	ph1
        d8  igrad r2d
        d3  gc_control
        {       ;shapes cover one period between rf pulses
                 d10 grad{ReadShape(100,ShapeSize)|PhaseShape(100,ShapeSize)*r2d(100)|SliceShape(100,ShapeSize)}
                 grad{(0)|(0)|(t3)}
        }
	d3enab   
        rdepa						 \n deparx     adc ph0  syrec	          \n derxadc     ph1:r  			  \n deadc        
	d6	 cpdngs30:f1
	d7       eoscnp
lo to echo times NECHOES/PVM_NEchoImages
lo to echo1 times PVM_NEchoImages
        2m
	d4       groff 
;----------------------------------slice loop-----------------------
	0u islice
	10u
	lo to slice times NSLICES  
	2.5u	ipp0
        vd2
;----------------------------------averaging loop-------------------
	lo to start times NA
	10u	rpp0
;----------------------------------2d loop--------------------------
if( ACQ_dim >= 2 )
{
	"lc1 = lc1 - 1"		; this makes
	if "lc1>=0" goto start	; dummy scans 

	lo to start times l2	;ACQ_size[1]/ACQ_rare_factor
}
        lo to start times NAE
        0u igrad PVM_ppgGradAmpArray1 vd1.inc vd2.inc fq2list.inc
        lo to start times NR
if (ACQ_scan_type != Scan_Experiment) \n{ \n goto start \n}

exit

ph0 = 0 2
ph1 = 1


