https://www.youtube.com/watch?v=zXj37jAeer8


conf t
hostname Router1
ip domain name xzbori22.vutbr.cz
crypto key generate rsa general-keys modulus 1024

aaa new-model

line vty 0 4
transport input ssh
login local
username tzboril privilege 15 secret cisco
ip ssh ver 2


Verif commands:
ssh -l tzboril {IP_address}
Password:
who
show ssh
show control-plan host open-ports
show tcp
