Building configuration...

Current configuration : 12902 bytes
!
! Last configuration change at 18:46:33 UTC Fri May 20 2022 by tzboril
!
version 16.12
service timestamps debug datetime msec
service timestamps log datetime msec
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
platform console serial
!
hostname R4
!
boot-start-marker
boot-end-marker
!
!
!
aaa new-model
!
!
aaa authentication login default local
aaa authorization exec default local
!
!
!
!
!
aaa session-id common
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
  no destination transport-method email
!
!
!
!
!
!
!
no ip domain lookup
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
!
!
!
!
!
!
multilink bundle-name authenticated
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
crypto pki trustpoint TP-self-signed-1293816562
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1293816562
 revocation-check none
 rsakeypair TP-self-signed-1293816562
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-1293816562
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31323933 38313635 3632301E 170D3232 30343231 31363337
  34315A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 32393338
  31363536 32308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100A625 55F94CE5 0F94BBD9 FDEA303B 49BF8972 92BE4C55 03FF592C
  026890EF A5161FC1 90C000CE 462B74B7 8909FD1F 6224FC10 6F418FB9 3C2F0D3F
  25876C67 A2ED6D22 04874B1B 2E73C35F 2C3B73B3 39DA0874 95E05375 3CA65433
  173D9245 DC0CF687 FDC0A71D F8502B8A 7C642CAE B8C9E311 3AADC5DC C6563F94
  4C75E87B AD5B25D4 3B422684 D1C01637 424B43A0 36AFFE2D 475D5A05 D477ECE3
  3A9A1EE8 98BA5BE4 C825D2FF 8A947F14 718134D6 6917A2EC 2E6211EC 60A17C05
  89B067E9 D17708C9 35087E91 2C932B38 4516D8FE 16F0D327 60DE4F86 4BEDBBFC
  9D132712 9FFDD348 22AB982E 526515D1 D8483FAF 729B7421 CA7F903D 6F885533
  5E79E4EB 022D0203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14F0E52A 610D3E75 3B05A429 1AF72DF1 57C1806F
  9F301D06 03551D0E 04160414 F0E52A61 0D3E753B 05A4291A F72DF157 C1806F9F
  300D0609 2A864886 F70D0101 05050003 82010100 39434B24 4F3F861E CE43370E
  168E2B63 BB358F13 92EE5B15 E470783B 578A0D5E 4BD17B9D A2DA7D90 CBAEA606
  DC1A72A4 27C1626E EDE8C1A8 87C1C26E 91055E1D ED5A971F 252A1CC1 AC212084
  D1B9633C 67CA1EB1 F4D9B197 7DBAA84B 66AA1A12 31AA2868 06E9A881 983DC26D
  00A4A82A 79688EDE 3CE8C885 1AE49E78 E6A05308 39AF3610 A76A5B3B 693F5802
  6DA5A550 BB062463 F78AD139 9DBAEC56 95DC1ED2 D53DAC90 C8C5A441 238BAB11
  AF9AC5B9 D2E57FDD 3EE3874C 8D215F75 2FDD5334 7CC3D3D5 A1D71EBD D04480F4
  2F858979 9E519B04 7143E325 E55C66B9 D2F0A95D DDFEFAF0 FFEFDCAE 13E1423B
  C3B8D273 ABF6B637 878B0688 D3763651 1034E2B2
  	quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
  	quit
!
license udi pid CSR1000V sn 9EPVWQE8NC1
diagnostic bootup level minimal
memory free low-watermark processor 72329
!
!
spanning-tree extend system-id
!
username tzboril privilege 15 secret 9 $9$YMm8ijPt1TAWW.$p9H9L5X78ccoL/4yp42Qwb.64.IcoMS/ktREDsp6NMw
!
redundancy
!
!
!
!
!
cdp run
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
!
interface GigabitEthernet1
 ip address 172.30.0.2 255.255.255.252
 negotiation auto
 cdp enable
 no mop enabled
 no mop sysid
!
interface GigabitEthernet2
 ip address 172.16.2.1 255.255.255.0
 negotiation auto
 cdp enable
 no mop enabled
 no mop sysid
!
interface GigabitEthernet3
 ip address 172.16.8.1 255.255.255.0
 negotiation auto
 cdp enable
 no mop enabled
 no mop sysid
!
interface GigabitEthernet4
 ip address 172.16.9.1 255.255.255.0
 negotiation auto
 cdp enable
 no mop enabled
 no mop sysid
!
interface GigabitEthernet5
 ip address 172.16.5.1 255.255.255.0
 negotiation auto
 no mop enabled
 no mop sysid
!
interface GigabitEthernet6
 ip address 10.255.255.4 255.255.255.0
 negotiation auto
 no mop enabled
 no mop sysid
!
router ospf 109
 router-id 5.5.5.5
 network 172.16.3.1 0.0.0.0 area 3
 network 172.16.4.1 0.0.0.0 area 3
 network 172.16.0.0 0.0.7.255 area 3
 network 172.30.0.2 0.0.0.0 area 3
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
ip route 192.168.122.0 255.255.255.0 GigabitEthernet6
ip ssh version 2
ip scp server enable
!
!
!
!
snmp-server group group_1 v3 priv
snmp-server community cisco RO
snmp-server enable traps snmp authentication linkdown linkup coldstart warmstart
snmp-server enable traps vrrp
snmp-server enable traps pfr
snmp-server enable traps flowmon
snmp-server enable traps ds1
snmp-server enable traps entity-perf throughput-notif
snmp-server enable traps call-home message-send-fail server-fail
snmp-server enable traps tty
snmp-server enable traps casa
snmp-server enable traps ospf state-change
snmp-server enable traps ospf errors
snmp-server enable traps ospf retransmit
snmp-server enable traps ospf lsa
snmp-server enable traps ospf cisco-specific state-change nssa-trans-change
snmp-server enable traps ospf cisco-specific state-change shamlink interface
snmp-server enable traps ospf cisco-specific state-change shamlink neighbor
snmp-server enable traps ospf cisco-specific errors
snmp-server enable traps ospf cisco-specific retransmit
snmp-server enable traps ospf cisco-specific lsa
snmp-server enable traps eigrp
snmp-server enable traps adslline
snmp-server enable traps vdsl2line
snmp-server enable traps license
snmp-server enable traps smart-license
snmp-server enable traps ethernet evc status create delete
snmp-server enable traps ether-oam
snmp-server enable traps ethernet cfm cc mep-up mep-down cross-connect loop config
snmp-server enable traps ethernet cfm crosscheck mep-missing mep-unknown service-up
snmp-server enable traps entity-qfp mem-res-thresh throughput-notif
snmp-server enable traps entity-state
snmp-server enable traps diameter
snmp-server enable traps bgp cbgp2
snmp-server enable traps dlsw
snmp-server enable traps entity-sensor
snmp-server enable traps resource-policy
snmp-server enable traps flash insertion removal lowspace
snmp-server enable traps nhrp nhs
snmp-server enable traps nhrp nhc
snmp-server enable traps nhrp nhp
snmp-server enable traps nhrp quota-exceeded
snmp-server enable traps ipsla
snmp-server enable traps cnpd
snmp-server enable traps entity-diag boot-up-fail hm-test-recover hm-thresh-reached scheduled-test-fail
snmp-server enable traps auth-framework sec-violation
snmp-server enable traps bfd
snmp-server enable traps cef resource-failure peer-state-change peer-fib-state-change inconsistency
snmp-server enable traps memory bufferpeak
snmp-server enable traps config-copy
snmp-server enable traps config
snmp-server enable traps config-ctid
snmp-server enable traps dhcp
snmp-server enable traps fru-ctrl
snmp-server enable traps entity
snmp-server enable traps event-manager
snmp-server enable traps frame-relay
snmp-server enable traps frame-relay subif
snmp-server enable traps hsrp
snmp-server enable traps pimstdmib neighbor-loss invalid-register invalid-join-prune rp-mapping-change interface-election
snmp-server enable traps ipmulticast
snmp-server enable traps isis
snmp-server enable traps ip local pool
snmp-server enable traps msdp
snmp-server enable traps mvpn
snmp-server enable traps ospfv3 state-change
snmp-server enable traps ospfv3 errors
snmp-server enable traps pim neighbor-change rp-mapping-change invalid-pim-message
snmp-server enable traps pppoe
snmp-server enable traps cpu threshold
snmp-server enable traps rsvp
snmp-server enable traps l2tun session
snmp-server enable traps l2tun pseudowire status
snmp-server enable traps aaa_server
snmp-server enable traps atm subif
snmp-server enable traps pki
snmp-server enable traps ike policy add
snmp-server enable traps ike policy delete
snmp-server enable traps ike tunnel start
snmp-server enable traps ike tunnel stop
snmp-server enable traps ipsec cryptomap add
snmp-server enable traps ipsec cryptomap delete
snmp-server enable traps ipsec cryptomap attach
snmp-server enable traps ipsec cryptomap detach
snmp-server enable traps ipsec tunnel start
snmp-server enable traps ipsec tunnel stop
snmp-server enable traps ipsec too-many-sas
snmp-server enable traps gdoi gm-start-registration
snmp-server enable traps gdoi gm-registration-complete
snmp-server enable traps gdoi gm-re-register
snmp-server enable traps gdoi gm-rekey-rcvd
snmp-server enable traps gdoi gm-rekey-fail
snmp-server enable traps gdoi ks-rekey-pushed
snmp-server enable traps gdoi gm-incomplete-cfg
snmp-server enable traps gdoi ks-no-rsa-keys
snmp-server enable traps gdoi ks-new-registration
snmp-server enable traps gdoi ks-reg-complete
snmp-server enable traps gdoi ks-role-change
snmp-server enable traps gdoi ks-gm-deleted
snmp-server enable traps gdoi ks-peer-reachable
snmp-server enable traps gdoi ks-peer-unreachable
snmp-server enable traps firewall serverstatus
snmp-server enable traps dsp card-status
snmp-server enable traps dsp oper-state
snmp-server enable traps dsp video-usage
snmp-server enable traps dsp video-out-of-resource
snmp-server enable traps frame-relay multilink bundle-mismatch
snmp-server enable traps syslog
snmp-server enable traps mpls rfc ldp
snmp-server enable traps mpls ldp
snmp-server enable traps mpls rfc traffic-eng
snmp-server enable traps mpls traffic-eng
snmp-server enable traps mpls fast-reroute protected
snmp-server enable traps otn
snmp-server enable traps pw vc
snmp-server enable traps lisp
snmp-server enable traps dial
snmp-server enable traps sbc adj-status
snmp-server enable traps sbc blacklist
snmp-server enable traps sbc congestion-alarm
snmp-server enable traps sbc h248-ctrlr-status
snmp-server enable traps sbc media-source
snmp-server enable traps sbc radius-conn-status
snmp-server enable traps sbc sla-violation
snmp-server enable traps sbc sla-violation-rev1
snmp-server enable traps sbc svc-state
snmp-server enable traps sbc qos-statistics
snmp-server enable traps ethernet cfm alarm
snmp-server enable traps alarms informational
snmp-server enable traps rf
snmp-server enable traps transceiver all
snmp-server enable traps bulkstat collection transfer
snmp-server enable traps vrfmib vrf-up vrf-down vnet-trunk-up vnet-trunk-down
snmp-server enable traps mpls vpn
snmp-server enable traps mpls rfc vpn
snmp-server enable traps voice
snmp-server enable traps ccme
snmp-server enable traps srst
!
!
!
!
!
control-plane
!
!
!
!
!
!
line con 0
 stopbits 1
line vty 0 4
 transport input ssh
!
!
!
!
!
!
end