(export (version D)
  (design
    (source "D:\\zaloha\\Google Drive\\Documents\\_škola\\bakalarka\\_vyvoj\\sekvencer\\HW\\sekvencer_v0.01 HW\\sekvencer_v0.01.sch")
    (date "5.4.2018 12:50:41")
    (tool "Eeschema (5.0.0-rc2-dev-366-ga2f118d2f)")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source sekvencer_v0.01.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value ATmega328P-AU)
      (footprint Package_QFP:TQFP-32_7x7mm_P0.8mm)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8271-8-bit-avr-microcontroller-atmega48a-48pa-88a-88pa-168a-168pa-328-328p_datasheet.pdf)
      (libsource (lib MCU_Microchip_ATmega) (part ATmega328P-AU))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6A867))
    (comp (ref L3)
      (value 10u)
      (footprint Inductor_SMD:L_0805_2012Metric)
      (libsource (lib Device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6F6A4))
    (comp (ref C18)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6F851))
    (comp (ref C3)
      (value 47u)
      (footprint Capacitor_THT:CP_Radial_D5.0mm_P2.50mm)
      (libsource (lib Device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6FB98))
    (comp (ref C7)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6FD7F))
    (comp (ref C9)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6FDD4))
    (comp (ref C13)
      (value 1n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6FDFA))
    (comp (ref C14)
      (value 100p)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB6FE2E))
    (comp (ref C15)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB70F3D))
    (comp (ref C17)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB72059))
    (comp (ref C16)
      (value 1n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB7220F))
    (comp (ref R2)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB73295))
    (comp (ref J5)
      (value LCD)
      (footprint Connector_JST:JST_EH_B09B-EH-A_1x09_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x09))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB77302))
    (comp (ref R6)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB792F7))
    (comp (ref Q3)
      (value BSS138)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.tme.eu/cz/Document/8b54c0c306d8a0230addbe9ac657cf6d/BSS138LT1G.PDF)
      (libsource (lib Device) (part Q_NMOS_GSD))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB81ADC))
    (comp (ref R11)
      (value 100k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB83224))
    (comp (ref J7)
      (value TX_REL)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8677C))
    (comp (ref R10)
      (value 100k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB89B9F))
    (comp (ref J6)
      (value RX_REL)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB89BB2))
    (comp (ref D4)
      (value D)
      (footprint Diode_SMD:D_MELF)
      (libsource (lib Device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8A727))
    (comp (ref Q4)
      (value IRLML0030TRPBF)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.infineon.com/dgdl/irlml0030pbf.pdf?fileId=5546d462533600a401535664773825df)
      (libsource (lib Device) (part Q_NMOS_GSD))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8E958))
    (comp (ref R12)
      (value 100k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8E96A))
    (comp (ref J8)
      (value FAN)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8E97D))
    (comp (ref D5)
      (value D)
      (footprint Diode_SMD:D_MELF)
      (libsource (lib Device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8FAF3))
    (comp (ref C1)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB9112D))
    (comp (ref L1)
      (value 560n)
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB91270))
    (comp (ref C4)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB913F6))
    (comp (ref J3)
      (value SWR)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB997C7))
    (comp (ref RV1)
      (value 10k)
      (footprint Potentiometer_SMD:Potentiometer_Bourns_3214J_Horizontal)
      (libsource (lib Device) (part POT_TRIM))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB85AE2))
    (comp (ref C11)
      (value 47n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB85B6A))
    (comp (ref C2)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8C1C0))
    (comp (ref L2)
      (value 560n)
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.50mm_HandSolder)
      (libsource (lib Device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8C1C6))
    (comp (ref C5)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8C1CC))
    (comp (ref J4)
      (value POWER)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8C1DF))
    (comp (ref RV2)
      (value 10k)
      (footprint Potentiometer_SMD:Potentiometer_Bourns_3214J_Horizontal)
      (libsource (lib Device) (part POT_TRIM))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8C1F2))
    (comp (ref C12)
      (value 47n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB8C1F8))
    (comp (ref J2)
      (value PTT)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB92F88))
    (comp (ref D2)
      (value D)
      (footprint Diode_SMD:D_SOD-123)
      (libsource (lib Device) (part D))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB930C2))
    (comp (ref Q1)
      (value BC857)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (libsource (lib Device) (part Q_PNP_BEC))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB80EFF))
    (comp (ref R1)
      (value 4k7)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB85339))
    (comp (ref C10)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB924BC))
    (comp (ref C8)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB925DC))
    (comp (ref C6)
      (value 1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB92662))
    (comp (ref R3)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABA240D))
    (comp (ref R8)
      (value 4k7)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABA64C2))
    (comp (ref R15)
      (value 270k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABD7300))
    (comp (ref R16)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABD7399))
    (comp (ref R7)
      (value 4k7)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AB99214))
    (comp (ref R20)
      (value 0R005)
      (footprint KLALIB_Resistors_Shunt:OAR5R010FLF)
      (datasheet https://www.tme.eu/cz/Document/9a11044aeb9919912b385f857afa61b7/oar.pdf)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACD9495))
    (comp (ref R19)
      (value 0R005)
      (footprint KLALIB_Resistors_Shunt:OAR5R010FLF)
      (datasheet https://www.tme.eu/cz/Document/9a11044aeb9919912b385f857afa61b7/oar.pdf)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACD95D8))
    (comp (ref R22)
      (value 4k7)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD1AE5A))
    (comp (ref Q5)
      (value BBS3002-TL-1E)
      (footprint Package_TO_SOT_SMD:TO-263-2)
      (datasheet http://www.farnell.com/datasheets/2337918.pdf?_ga=2.37639200.12383568.1522753699-1027071704.1516743165&_gac=1.79549798.1522167148.Cj0KCQjw1-fVBRC3ARIsAIifYOPkZdOLWuJG89v_8Q1mJPJjDJGU3LWCKZpCUy6__Npd1mdZPKpMYl8aAjQHEALw_wcB)
      (libsource (lib Device) (part Q_PMOS_GDS))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD20097))
    (comp (ref J10)
      (value 50V_OUT)
      (footprint KLALIB_PCB_Screw_Terminal:TerminalBlock_KEYS7808)
      (libsource (lib Connector_Specialized) (part Screw_Terminal_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD5D878))
    (comp (ref C24)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE0BED3))
    (comp (ref C23)
      (value 1u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE0C07F))
    (comp (ref C27)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABCB0C3))
    (comp (ref R5)
      (value 22k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABFFD4A))
    (comp (ref R4)
      (value 22k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC0A087))
    (comp (ref Q2)
      (value Q_NMOS_DGS)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.tme.eu/cz/Document/6c7ba86a4db59a0411a4966dbe2bd1aa/BSS123-7-F.pdf)
      (libsource (lib Device) (part Q_NMOS_GSD))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC15CD8))
    (comp (ref R18)
      (value 100k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC15CE4))
    (comp (ref J1)
      (value AVR_ISP_01X06)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical)
      (libsource (lib KLIB_Con_Prog) (part AVR_ISP_01X06))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABE5D81))
    (comp (ref U4)
      (value LTC6101AHS5)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (datasheet http://cds.linear.com/docs/en/datasheet/6101fh.pdf)
      (libsource (lib KLALIB_Amplifiers) (part LTC6101AHS5))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC56CF2))
    (comp (ref R14)
      (value 10k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC581C8))
    (comp (ref R13)
      (value 499R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACB7FAF))
    (comp (ref R21)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ADAFCD8))
    (comp (ref D_STAT1)
      (value "LH R974-LP-1")
      (footprint LED_SMD:LED_0805_2012Metric)
      (libsource (lib Device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ADBDF74))
    (comp (ref U3)
      (value LM2576HVS-12)
      (footprint Package_TO_SOT_SMD:TO-263-5_TabPin3)
      (datasheet http://www.ti.com/lit/ds/symlink/lm2576.pdf)
      (libsource (lib Regulator_Switching) (part LM2576HVS-12))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ADCE47B))
    (comp (ref C21)
      (value 100u)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P5.00mm)
      (libsource (lib Device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ADCE5C1))
    (comp (ref C20)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ADCE68F))
    (comp (ref D6)
      (value STPS3L60U)
      (footprint Diode_SMD:D_SMB)
      (datasheet https://www.tme.eu/cz/Document/52d57fe80dbff7a95e6e84e0ea32277a/STPS3L60U.pdf)
      (libsource (lib Device) (part D_Schottky))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE00C93))
    (comp (ref L4)
      (value DE1209-230u)
      (footprint Inductor_SMD:L_12x12mm_H8mm)
      (datasheet https://www.tme.eu/cz/Document/d1f8b47d020ebf11f3b92c6891638dfa/de.pdf)
      (libsource (lib Device) (part L))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE105B7))
    (comp (ref C26)
      (value 470u)
      (footprint Capacitor_THT:CP_Radial_D10.0mm_P5.00mm)
      (libsource (lib Device) (part CP))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE1819E))
    (comp (ref U2)
      (value LP2950-5.0_TO252)
      (footprint Package_TO_SOT_SMD:TO-252-2)
      (datasheet http://www.ti.com/lit/ds/symlink/lp2950-n.pdf)
      (libsource (lib Regulator_Linear) (part LP2950-5.0_TO252))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE4F073))
    (comp (ref C22)
      (value 4u7)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE6F627))
    (comp (ref C25)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE6F7A3))
    (comp (ref C19)
      (value 1n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AEF5BD3))
    (comp (ref R9)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AF608F2))
    (comp (ref D_5V1)
      (value "LH R974-LP-1")
      (footprint LED_SMD:LED_0805_2012Metric)
      (libsource (lib Device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AF60900))
    (comp (ref Q6)
      (value BSS138)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet https://www.tme.eu/cz/Document/8b54c0c306d8a0230addbe9ac657cf6d/BSS138LT1G.PDF)
      (libsource (lib Device) (part Q_NMOS_GSD))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFD3729))
    (comp (ref L5)
      (value BLM31PG500SN1L)
      (footprint Capacitor_SMD:C_1206_3216Metric)
      (datasheet https://www.tme.eu/cz/Document/1ccbd33732eb07f42b8bfd60a02eaa88/blm31pg500sn1l.pdf)
      (libsource (lib Device) (part Ferrite_Bead))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFE6D53))
    (comp (ref C28)
      (value NFM21CC223R1H3D)
      (footprint EMI_Suppression_Filters_Cap_Type:NFM21C_Series)
      (datasheet https://www.tme.eu/cz/Document/6569e59e184cc065c1b380e8778a791e/MURATA-NFM21C-series.pdf)
      (libsource (lib Device) (part EMI_Filter_C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AFE6FF8))
    (comp (ref C29)
      (value NFM21CC223R1H3D)
      (footprint EMI_Suppression_Filters_Cap_Type:NFM21C_Series)
      (datasheet https://www.tme.eu/cz/Document/6569e59e184cc065c1b380e8778a791e/MURATA-NFM21C-series.pdf)
      (libsource (lib Device) (part EMI_Filter_C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABF209F))
    (comp (ref R23)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC16DC5))
    (comp (ref C30)
      (value NFM21CC223R1H3D)
      (footprint EMI_Suppression_Filters_Cap_Type:NFM21C_Series)
      (datasheet https://www.tme.eu/cz/Document/6569e59e184cc065c1b380e8778a791e/MURATA-NFM21C-series.pdf)
      (libsource (lib Device) (part EMI_Filter_C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC33038))
    (comp (ref R24)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC3303E))
    (comp (ref J11)
      (value BIAS)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC02834))
    (comp (ref J9)
      (value 50V_IN)
      (footprint KLALIB_PCB_Screw_Terminal:TerminalBlock_KEYS7808)
      (libsource (lib Connector_Specialized) (part Screw_Terminal_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABF2CC7))
    (comp (ref J12)
      (value 50V_GND)
      (footprint MountingHole:MountingHole_4mm_Pad_Via)
      (libsource (lib Connector_Specialized) (part Screw_Terminal_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ABF2E7D))
    (comp (ref C31)
      (value 22p)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC6AE1D))
    (comp (ref C32)
      (value 22p)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (libsource (lib Device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC7ED6F))
    (comp (ref Y1)
      (value 16MHz)
      (footprint Crystal:Crystal_SMD_2520-4Pin_2.5x2.0mm)
      (libsource (lib Device) (part Crystal_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC7EFBB))
    (comp (ref D3)
      (value LM4040DBZ-2.5)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.ti.com/lit/ds/symlink/lm4040-n.pdf)
      (libsource (lib Reference_Voltage) (part LM4040DBZ-2.5))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC4155B))
    (comp (ref J13)
      (value TERMISTOR)
      (footprint Connector_JST:JST_XH_B02B-XH-A_1x02_P2.50mm_Vertical)
      (libsource (lib Connector_Generic) (part Conn_01x02))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC4226B))
    (comp (ref R25)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC6CFF2))
    (comp (ref J14)
      (value 50V_GND)
      (footprint MountingHole:MountingHole_4mm_Pad_Via)
      (libsource (lib Connector_Specialized) (part Screw_Terminal_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACC1DC1))
    (comp (ref J15)
      (value 50V_GND)
      (footprint MountingHole:MountingHole_4mm_Pad_Via)
      (libsource (lib Connector_Specialized) (part Screw_Terminal_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACC1E9F))
    (comp (ref J16)
      (value 50V_GND)
      (footprint MountingHole:MountingHole_4mm_Pad_Via)
      (libsource (lib Connector_Specialized) (part Screw_Terminal_01x01))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACC1F79))
    (comp (ref C33)
      (value NFM21CC223R1H3D)
      (footprint EMI_Suppression_Filters_Cap_Type:NFM21C_Series)
      (datasheet https://www.tme.eu/cz/Document/6569e59e184cc065c1b380e8778a791e/MURATA-NFM21C-series.pdf)
      (libsource (lib Device) (part EMI_Filter_C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AC60BDD))
    (comp (ref R17)
      (value 22k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACA0366))
    (comp (ref C34)
      (value NFM21CC223R1H3D)
      (footprint EMI_Suppression_Filters_Cap_Type:NFM21C_Series)
      (datasheet https://www.tme.eu/cz/Document/6569e59e184cc065c1b380e8778a791e/MURATA-NFM21C-series.pdf)
      (libsource (lib Device) (part EMI_Filter_C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACAB533))
    (comp (ref RV3)
      (value 10k)
      (footprint Potentiometer_SMD:Potentiometer_Bourns_3214J_Horizontal)
      (libsource (lib Device) (part POT_TRIM))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ACF87E5))
    (comp (ref R29)
      (value 3k9)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD68C72))
    (comp (ref D_RX1)
      (value "LH R974-LP-1")
      (footprint LED_SMD:LED_0805_2012Metric)
      (libsource (lib Device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD68F42))
    (comp (ref R30)
      (value 3k9)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD804CA))
    (comp (ref D_TX1)
      (value "LH R974-LP-1")
      (footprint LED_SMD:LED_0805_2012Metric)
      (libsource (lib Device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD804D1))
    (comp (ref R31)
      (value 3k9)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD8C42F))
    (comp (ref D_FAN1)
      (value "LH R974-LP-1")
      (footprint LED_SMD:LED_0805_2012Metric)
      (libsource (lib Device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AD8C436))
    (comp (ref R28)
      (value 18k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE88125))
    (comp (ref D_50V1)
      (value "LH R974-LP-1")
      (footprint LED_SMD:LED_0805_2012Metric)
      (libsource (lib Device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5AE8812B))
    (comp (ref R27)
      (value 12k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B023AE9))
    (comp (ref R26)
      (value 1k)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (libsource (lib Device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B053F51))
    (comp (ref D_PTT1)
      (value "LH R974-LP-1")
      (footprint LED_SMD:LED_0805_2012Metric)
      (libsource (lib Device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B053F57)))
  (libparts
    (libpart (lib MCU_Microchip_ATmega) (part ATmega168A-AU)
      (aliases
        (alias ATmega48A-AU)
        (alias ATmega48PA-AU)
        (alias ATmega88A-AU)
        (alias ATmega88PA-AU)
        (alias ATmega168PA-AU)
        (alias ATmega328-AU)
        (alias ATmega328P-AU))
      (description "TQFP32, 16k Flash, 1kB SRAM, 512B EEPROM")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8271-8-bit-avr-microcontroller-atmega48a-48pa-88a-88pa-168a-168pa-328-328p_datasheet.pdf)
      (footprints
        (fp TQFP*7x7mm*P0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ATmega168A-AU)
        (field (name Footprint) Package_QFP:TQFP-32_7x7mm_P0.8mm))
      (pins
        (pin (num 1) (name PD3) (type BiDi))
        (pin (num 2) (name PD4) (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name VCC) (type power_in))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name VCC) (type passive))
        (pin (num 7) (name XTAL1/PB6) (type BiDi))
        (pin (num 8) (name XTAL2/PB7) (type BiDi))
        (pin (num 9) (name PD5) (type BiDi))
        (pin (num 10) (name PD6) (type BiDi))
        (pin (num 11) (name PD7) (type BiDi))
        (pin (num 12) (name PB0) (type BiDi))
        (pin (num 13) (name PB1) (type BiDi))
        (pin (num 14) (name PB2) (type BiDi))
        (pin (num 15) (name PB3) (type BiDi))
        (pin (num 16) (name PB4) (type BiDi))
        (pin (num 17) (name PB5) (type BiDi))
        (pin (num 18) (name AVCC) (type power_in))
        (pin (num 19) (name ADC6) (type input))
        (pin (num 20) (name AREF) (type input))
        (pin (num 21) (name GND) (type passive))
        (pin (num 22) (name ADC7) (type input))
        (pin (num 23) (name PC0) (type BiDi))
        (pin (num 24) (name PC1) (type BiDi))
        (pin (num 25) (name PC2) (type BiDi))
        (pin (num 26) (name PC3) (type BiDi))
        (pin (num 27) (name PC4) (type BiDi))
        (pin (num 28) (name PC5) (type BiDi))
        (pin (num 29) (name ~RESET~/PC6) (type BiDi))
        (pin (num 30) (name PD0) (type BiDi))
        (pin (num 31) (name PD1) (type BiDi))
        (pin (num 32) (name PD2) (type BiDi))))
    (libpart (lib KLIB_Con_Prog) (part AVR_ISP_01X06)
      (description "AVR, ISP, header, 01X06")
      (docs ~)
      (footprints
        (fp *Header*))
      (fields
        (field (name Reference) J)
        (field (name Value) AVR_ISP_01X06)
        (field (name Footprint) Socket_Strips:Socket_Strip_Straight_1x06_Pitch2.54mm))
      (pins
        (pin (num 1) (name VTG) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name SCK) (type output))
        (pin (num 4) (name ~RST) (type output))
        (pin (num 5) (name MISO) (type input))
        (pin (num 6) (name MOSI) (type output))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp *:C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part CP)
      (description "Polarised capacitor")
      (docs ~)
      (footprints
        (fp *:CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Feedthrough)
      (aliases
        (alias EMI_Filter_C))
      (description "feedthrough capacitor")
      (docs ~)
      (fields
        (field (name Reference) C)
        (field (name Value) C_Feedthrough))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp *:C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x09)
      (description "Generic connector, single row, 01x09, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x09))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))))
    (libpart (lib Device) (part Crystal_Small)
      (description "Two pin crystal, small symbol")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part D)
      (description Diode)
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp *:D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp *:D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead)
      (description "Ferrite bead")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp *:L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) L)
        (field (name Value) Ferrite_Bead))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part L)
      (description Inductor)
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp *:L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part LED)
      (description "LED generic")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Regulator_Switching) (part LM2576HVS-12)
      (aliases
        (alias LM2576HVS-3.3)
        (alias LM2576HVS-5)
        (alias LM2576HVS-15)
        (alias LM2576HVS-ADJ)
        (alias LM2576S-12)
        (alias LM2576S-3.3)
        (alias LM2576S-5)
        (alias LM2576S-15)
        (alias LM2576S-ADJ)
        (alias LM2575BU-ADJ)
        (alias LM2575-3.3BU)
        (alias LM2575-5.0BU)
        (alias LM2575-12BU)
        (alias GL2576-3.3TA5R)
        (alias GL2576-5.0TA5R)
        (alias GL2576-12TA5R)
        (alias GL2576-15TA5R)
        (alias GL2576-ATA5R))
      (description "12V, 3A SIMPLE SWITCHER® Step-Down Voltage Regulator, High Voltage Input, TO-263")
      (docs http://www.ti.com/lit/ds/symlink/lm2576.pdf)
      (footprints
        (fp TO?263*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM2576HVS-12)
        (field (name Footprint) Package_TO_SOT_SMD:TO-263-5_TabPin3))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name OUT) (type output))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name FB) (type input))
        (pin (num 5) (name ~ON~/OFF) (type input))))
    (libpart (lib Reference_Voltage) (part LM4040DBZ-2.0)
      (aliases
        (alias LM4040DBZ-2.5)
        (alias LM4040DBZ-3)
        (alias LM4040DBZ-4.1)
        (alias LM4040DBZ-5)
        (alias LM4040DBZ-8.2)
        (alias LM4040DBZ-10))
      (description "2.048V Precision Micropower Shunt Voltage Reference, SOT-23")
      (docs http://www.ti.com/lit/ds/symlink/lm4040-n.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) D)
        (field (name Value) LM4040DBZ-2.0)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Regulator_Linear) (part LM78M05_TO252)
      (aliases
        (alias MC78M05_TO252)
        (alias KA78M05_TO252)
        (alias LF15_TO252)
        (alias LF18_TO252)
        (alias LF25_TO252)
        (alias LF33_TO252)
        (alias LF50_TO252)
        (alias LF60_TO252)
        (alias LF80_TO252)
        (alias LF85_TO252)
        (alias LF120_TO252)
        (alias LP2950-3.0_TO252)
        (alias LP2950-3.3_TO252)
        (alias LP2950-5.0_TO252)
        (alias LF47_TO252)
        (alias LF90_TO252))
      (description "Positive 500mA 35V Linear Regulator, Fixed Output 5V, TO-252 (D-PAK)")
      (docs http://www.fairchildsemi.com/ds/LM/LM78M05.pdf)
      (footprints
        (fp TO?252*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM78M05_TO252)
        (field (name Footprint) Package_TO_SOT_SMD:TO-252-2))
      (pins
        (pin (num 1) (name VI) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name VO) (type power_out))))
    (libpart (lib KLALIB_Amplifiers) (part LTC6101AHS5)
      (fields
        (field (name Reference) U)
        (field (name Value) LTC6101AHS5)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5)
        (field (name Datasheet) http://cds.linear.com/docs/en/datasheet/6101fh.pdf))
      (pins
        (pin (num 1) (name OUT) (type output))
        (pin (num 2) (name V-) (type power_in))
        (pin (num 3) (name -) (type input))
        (pin (num 4) (name +) (type input))
        (pin (num 5) (name V+) (type power_in))))
    (libpart (lib Device) (part POT_TRIM)
      (description Trim-Potentiometer)
      (docs ~)
      (footprints
        (fp Potentiometer*))
      (fields
        (field (name Reference) RV)
        (field (name Value) POT_TRIM))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))))
    (libpart (lib Device) (part Q_NMOS_GSD)
      (description "Transistor N-MOSFETwith substrate diode (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib Device) (part Q_PMOS_GDS)
      (description "Transistor P-MOSFET with substrate diode (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PMOS_GDS))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib Device) (part Q_PNP_BEC)
      (description "Transistor PNP (general)")
      (docs ~)
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_PNP_BEC))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp *:R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Connector_Specialized) (part Screw_Terminal_01x01)
      (description "Generic screw terminal, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp TerminalBlock*:*))
      (fields
        (field (name Reference) J)
        (field (name Value) Screw_Terminal_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive)))))
  (libraries
    (library (logical Connector_Generic)
      (uri C:\kicad\library/Connector_Generic.lib))
    (library (logical Connector_Specialized)
      (uri C:\kicad\library/Connector_Specialized.lib))
    (library (logical Device)
      (uri C:\kicad\library/Device.lib))
    (library (logical KLALIB_Amplifiers)
      (uri C:/kicad/klalib/library/KLALIB_Amplifiers.lib))
    (library (logical KLIB_Con_Prog)
      (uri C:/kicad/wykys/klib/library/KLIB_Con_Prog.lib))
    (library (logical MCU_Microchip_ATmega)
      (uri C:\kicad\library/MCU_Microchip_ATmega.lib))
    (library (logical Reference_Voltage)
      (uri C:\kicad\library/Reference_Voltage.lib))
    (library (logical Regulator_Linear)
      (uri C:\kicad\library/Regulator_Linear.lib))
    (library (logical Regulator_Switching)
      (uri C:\kicad\library/Regulator_Switching.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref D_PTT1) (pin 1))
      (node (ref D_50V1) (pin 1))
      (node (ref C33) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref J15) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref R14) (pin 1))
      (node (ref C1) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref J14) (pin 1))
      (node (ref J16) (pin 1))
      (node (ref RV3) (pin 3))
      (node (ref RV1) (pin 3))
      (node (ref C11) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref J12) (pin 1))
      (node (ref J11) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref Q3) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref J13) (pin 2))
      (node (ref U1) (pin 21))
      (node (ref D3) (pin 2))
      (node (ref Q4) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref Q6) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref J5) (pin 3))
      (node (ref U1) (pin 3))
      (node (ref C17) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C29) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref D6) (pin 2))
      (node (ref C24) (pin 2))
      (node (ref C23) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref U2) (pin 2))
      (node (ref C21) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref C19) (pin 2))
      (node (ref Q2) (pin 2))
      (node (ref C25) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref C22) (pin 2))
      (node (ref D_STAT1) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref RV2) (pin 3))
      (node (ref U3) (pin 3))
      (node (ref U3) (pin 5))
      (node (ref C20) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref J4) (pin 1)))
    (net (code 2) (name "Net-(D6-Pad1)")
      (node (ref D6) (pin 1))
      (node (ref L4) (pin 1))
      (node (ref U3) (pin 2)))
    (net (code 3) (name +5V)
      (node (ref D_5V1) (pin 2))
      (node (ref C25) (pin 1))
      (node (ref J5) (pin 2))
      (node (ref C22) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref C16) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref L3) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref RV3) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 6)))
    (net (code 4) (name "Net-(D_STAT1-Pad2)")
      (node (ref D_STAT1) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 5) (name /STATUS_LED1)
      (node (ref R21) (pin 2))
      (node (ref U1) (pin 11)))
    (net (code 6) (name +12V)
      (node (ref C3) (pin 1))
      (node (ref J8) (pin 1))
      (node (ref J7) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref L4) (pin 2))
      (node (ref C26) (pin 1))
      (node (ref D4) (pin 1))
      (node (ref J6) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref D_RX1) (pin 2))
      (node (ref D_TX1) (pin 2))
      (node (ref D_FAN1) (pin 2))
      (node (ref D5) (pin 1))
      (node (ref C19) (pin 1))
      (node (ref U2) (pin 1)))
    (net (code 7) (name "Net-(Q2-Pad3)")
      (node (ref R27) (pin 1))
      (node (ref Q2) (pin 3)))
    (net (code 8) (name /MCU_SUPPLY)
      (node (ref Q2) (pin 1))
      (node (ref U1) (pin 9))
      (node (ref R18) (pin 1)))
    (net (code 9) (name "Net-(J10-Pad1)")
      (node (ref R28) (pin 2))
      (node (ref J10) (pin 1))
      (node (ref Q5) (pin 2)))
    (net (code 10) (name /RESET)
      (node (ref R6) (pin 2))
      (node (ref U1) (pin 29))
      (node (ref J1) (pin 3)))
    (net (code 11) (name /DB5)
      (node (ref J1) (pin 4))
      (node (ref J5) (pin 7))
      (node (ref U1) (pin 15)))
    (net (code 12) (name /DB6)
      (node (ref J5) (pin 8))
      (node (ref U1) (pin 16))
      (node (ref J1) (pin 5)))
    (net (code 13) (name /DB7)
      (node (ref U1) (pin 17))
      (node (ref J1) (pin 6))
      (node (ref J5) (pin 9)))
    (net (code 14) (name "Net-(R5-Pad2)")
      (node (ref R5) (pin 2))
      (node (ref RV2) (pin 2)))
    (net (code 15) (name "Net-(R4-Pad2)")
      (node (ref RV1) (pin 2))
      (node (ref R4) (pin 2)))
    (net (code 16) (name "Net-(R13-Pad1)")
      (node (ref R13) (pin 1))
      (node (ref U4) (pin 3)))
    (net (code 17) (name "Net-(J5-Pad1)")
      (node (ref RV3) (pin 2))
      (node (ref J5) (pin 1)))
    (net (code 18) (name "Net-(C34-Pad1)")
      (node (ref C34) (pin 1))
      (node (ref R17) (pin 1)))
    (net (code 19) (name "Net-(C13-Pad1)")
      (node (ref C13) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref R15) (pin 1))
      (node (ref C28) (pin 3))
      (node (ref C20) (pin 1))
      (node (ref C21) (pin 1))
      (node (ref U3) (pin 1)))
    (net (code 20) (name +50V)
      (node (ref J9) (pin 1))
      (node (ref C24) (pin 1))
      (node (ref L5) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref R19) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref C23) (pin 1)))
    (net (code 21) (name "Net-(D_RX1-Pad1)")
      (node (ref D_RX1) (pin 1))
      (node (ref R29) (pin 1)))
    (net (code 22) (name "Net-(J13-Pad1)")
      (node (ref R3) (pin 2))
      (node (ref J13) (pin 1))
      (node (ref R17) (pin 2)))
    (net (code 23) (name "Net-(J11-Pad1)")
      (node (ref R25) (pin 1))
      (node (ref J11) (pin 1)))
    (net (code 24) (name /MCU_BIAS)
      (node (ref R25) (pin 2))
      (node (ref U1) (pin 10)))
    (net (code 25) (name "Net-(C33-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref C33) (pin 1)))
    (net (code 26) (name "Net-(C33-Pad3)")
      (node (ref C33) (pin 3))
      (node (ref D2) (pin 1)))
    (net (code 27) (name "Net-(D_50V1-Pad2)")
      (node (ref D_50V1) (pin 2))
      (node (ref R28) (pin 1)))
    (net (code 28) (name "Net-(D_PTT1-Pad2)")
      (node (ref D_PTT1) (pin 2))
      (node (ref R26) (pin 1)))
    (net (code 29) (name "Net-(D_TX1-Pad1)")
      (node (ref R30) (pin 1))
      (node (ref D_TX1) (pin 1)))
    (net (code 30) (name "Net-(D_FAN1-Pad1)")
      (node (ref R31) (pin 1))
      (node (ref D_FAN1) (pin 1)))
    (net (code 31) (name "Net-(C2-Pad1)")
      (node (ref L2) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C30) (pin 3)))
    (net (code 32) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref C29) (pin 3))
      (node (ref L1) (pin 1)))
    (net (code 33) (name "Net-(C29-Pad1)")
      (node (ref C29) (pin 1))
      (node (ref R23) (pin 1)))
    (net (code 34) (name "Net-(J3-Pad2)")
      (node (ref R23) (pin 2))
      (node (ref J3) (pin 2)))
    (net (code 35) (name "Net-(C30-Pad1)")
      (node (ref C30) (pin 1))
      (node (ref R24) (pin 1)))
    (net (code 36) (name "Net-(J4-Pad2)")
      (node (ref R24) (pin 2))
      (node (ref J4) (pin 2)))
    (net (code 37) (name "Net-(C28-Pad1)")
      (node (ref L5) (pin 1))
      (node (ref C28) (pin 1)))
    (net (code 38) (name "Net-(D_5V1-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref D_5V1) (pin 1)))
    (net (code 39) (name "Net-(C31-Pad1)")
      (node (ref Y1) (pin 2))
      (node (ref C31) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 40) (name "Net-(U1-Pad26)")
      (node (ref U1) (pin 26)))
    (net (code 41) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 42) (name "Net-(U1-Pad31)")
      (node (ref U1) (pin 31)))
    (net (code 43) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))
    (net (code 44) (name /ADC_TEMP)
      (node (ref C34) (pin 3))
      (node (ref U1) (pin 23)))
    (net (code 45) (name /ADC_UCC)
      (node (ref C27) (pin 1))
      (node (ref R15) (pin 2))
      (node (ref R16) (pin 1))
      (node (ref U1) (pin 22)))
    (net (code 46) (name /ADC_ICC)
      (node (ref U4) (pin 1))
      (node (ref R14) (pin 2))
      (node (ref U1) (pin 19)))
    (net (code 47) (name /MCU_REL2)
      (node (ref U1) (pin 28))
      (node (ref Q3) (pin 1))
      (node (ref R11) (pin 1)))
    (net (code 48) (name /ADC_POWER)
      (node (ref R5) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref U1) (pin 25)))
    (net (code 49) (name /ADC_SWR)
      (node (ref U1) (pin 24))
      (node (ref R4) (pin 1))
      (node (ref C11) (pin 1)))
    (net (code 50) (name /RS)
      (node (ref J5) (pin 4))
      (node (ref U1) (pin 12)))
    (net (code 51) (name /E)
      (node (ref J5) (pin 5))
      (node (ref U1) (pin 13)))
    (net (code 52) (name /DB4)
      (node (ref U1) (pin 14))
      (node (ref J5) (pin 6)))
    (net (code 53) (name /MCU_FAN)
      (node (ref U1) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref Q4) (pin 1)))
    (net (code 54) (name "Net-(J8-Pad2)")
      (node (ref J8) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref Q4) (pin 3)))
    (net (code 55) (name /MCU_REL1)
      (node (ref R10) (pin 1))
      (node (ref U1) (pin 27))
      (node (ref Q6) (pin 1)))
    (net (code 56) (name "Net-(D4-Pad2)")
      (node (ref R29) (pin 2))
      (node (ref Q6) (pin 3))
      (node (ref J6) (pin 1))
      (node (ref D4) (pin 2)))
    (net (code 57) (name "Net-(C18-Pad1)")
      (node (ref U1) (pin 18))
      (node (ref C18) (pin 1))
      (node (ref L3) (pin 2)))
    (net (code 58) (name /MCU_PTT)
      (node (ref Q1) (pin 3))
      (node (ref R8) (pin 1))
      (node (ref R26) (pin 2))
      (node (ref U1) (pin 32)))
    (net (code 59) (name "Net-(C32-Pad1)")
      (node (ref C32) (pin 1))
      (node (ref Y1) (pin 1))
      (node (ref U1) (pin 8)))
    (net (code 60) (name +2V5)
      (node (ref R3) (pin 1))
      (node (ref U1) (pin 20))
      (node (ref D3) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 61) (name "Net-(C4-Pad1)")
      (node (ref C4) (pin 1))
      (node (ref L1) (pin 2))
      (node (ref RV1) (pin 1)))
    (net (code 62) (name "Net-(C5-Pad1)")
      (node (ref RV2) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref C5) (pin 1)))
    (net (code 63) (name "Net-(J2-Pad2)")
      (node (ref R7) (pin 2))
      (node (ref J2) (pin 2)))
    (net (code 64) (name "Net-(Q5-Pad1)")
      (node (ref R22) (pin 1))
      (node (ref Q5) (pin 1))
      (node (ref R27) (pin 2)))
    (net (code 65) (name "Net-(Q5-Pad3)")
      (node (ref Q5) (pin 3))
      (node (ref U4) (pin 4))
      (node (ref R22) (pin 2))
      (node (ref R20) (pin 1))
      (node (ref R19) (pin 1)))
    (net (code 66) (name "Net-(D5-Pad2)")
      (node (ref J7) (pin 2))
      (node (ref Q3) (pin 3))
      (node (ref D5) (pin 2))
      (node (ref R30) (pin 2)))
    (net (code 67) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref Q1) (pin 1))
      (node (ref R1) (pin 2)))))