Partlist exported from C:/Users/martin/AppData/Roaming/SPB_16.6/eagle/QuadBoard v1.1/Scheme_v1.1.sch at 9. 5. 2017 17:04

Qty | Value | Device | Package | Parts | Description | DESCRIPTION | MF | MPN | OC_FARNELL | OC_NEWARK | PACKAGE | SUPPLIER
12 |  | MA03-1 | MA03-1 | SV1, SV2, SV3, SV4, SV5, SV6, SV7, SV8, SV9, SV10, SV11, SV12 | PIN HEADER |  |  |  | unknown | unknown |  |
7 | 100n | C-EUC0805 | C0805 | C6, C8, C9, C10, C11, C12, C13 | CAPACITOR, European symbol |  |  |  |  |  |  |
3 | 10k | R-EU_R0805 | R0805 | R2, R4, R7 | RESISTOR, European symbol |  |  |  |  |  |  |
4 | 10u | C-EUC1206K | C1206K | C2, C3, C4, C5 | CAPACITOR, European symbol |  |  |  |  |  |  |
2 | 12k | R-EU_R0805 | R0805 | R8, R9 | RESISTOR, European symbol |  |  |  |  |  |  |
1 | 16MHz | XTAL/S | QS | Q1 | CRYSTAL |  |  |  |  |  |  |
1 | 1X1 | 1X1 | 1X1 | H2-SSPIN |  |  |  |  |  |  |  |
1 | 1X4 | 1X4 | 1X4 | H1 |  |  |  |  |  |  |  |
1 | 1u | C-EUC1206 | C1206 | C14 | CAPACITOR, European symbol |  |  |  |  |  |  |
3 | 22k | R-EU_R0805 | R0805 | R6, R10, R11 | RESISTOR, European symbol |  |  |  |  |  |  |
2 | 22p | C-EUC0805 | C0805 | C1, C7 | CAPACITOR, European symbol |  |  |  |  |  |  |
1 | 2X3 | 2X3 | 2X3 | H1-PROG/SPI |  |  |  |  |  |  |  |
2 | 2X4 | 2X4 | 2X4 | H2, H3 |  |  |  |  |  |  |  |
2 | 2k2 | R-EU_R0805 | R0805 | R1, R5 | RESISTOR, European symbol |  |  |  |  |  |  |
1 | 52k3 | R-EU_R0805 | R0805 | R3 | RESISTOR, European symbol |  |  |  |  |  |  |
1 | ATMEGA2560-16AU | ATMEGA2560-16AU | QFP50P1600X1600X120-100N | U1 | Microcontroller | Microcontroller |  | ATMEGA2560-16AU | 1288330 | 23M5051 | LQFP-100 | ATMEL
1 | DL16-22 | L-USL4532P | L4532P | L3 | INDUCTOR, American symbol |  |  |  |  |  |  |
1 | GY-86 | GY-86 | GY-86 | GY-86 |  |  |  |  |  |  |  |
1 | LD117AS33TR | LD117AS33TR | SOT223 | IC1 | Low drop fixed and adjustable positive voltage regulators 1 A |  |  |  |  |  |  |
1 | LL4148 | CGRM4007-G | SOD-123_MINI-SMA | D1 | Molded plasitc,JEDEC SOD-123/Mini SMA |  |  |  |  |  |  |
1 | MBRS140 | MBRS130LT3 | SMB | D4 | Schottky Power Rectifier |  |  |  |  |  |  |
1 | MCP16301/H | MCP16301/H | SOT23-6 | IC2 | High-Voltage Input Integrated Switch Step-Down Regulator |  |  |  |  |  |  |
1 | PWR+ | LSP10 | LSP10 | LSP1 | SOLDER PAD drill 1.0 mm, distributor Buerklin, 12H555 |  |  |  |  |  |  |
1 | PWR- | LSP10 | LSP10 | LSP2 | SOLDER PAD drill 1.0 mm, distributor Buerklin, 12H555 |  |  |  |  |  |  |