
[Shared parameters]
Parameter Name Compiler Comment Date Melt Type Melt Type Unit Standard Name Temperature Temperature Unit Type Of Measure Density Density Unit Specimen Name Specimen Treatment Test Procedure Specimen Quantity Specimen Quantity Unit Specimen Format Specimen Lot Specimen Supplier Die Diameter Die Diameter Unit Die Length Die Length Unit PreHeating Total PreHeating Total Unit PreHeating Load PreHeating Load Unit Max Test Time Max Test Time Unit Cut Auto Cut Step Cut Time Cut Time Unit Discard Type Discard Type Unit Discard Value Discard Value Unit Tollerance Tollerance Unit Measure Start Measure Start Unit Compacting Time Compacting Time Unit Compacting Force Compacting Force Unit Cicle Select Wait Time Wait Time Unit Test Start Expulsion Force Expulsion Force Unit Specimen Note Number of steps Reference Resting Height Resting Height Unit Expulsion Weight Expulsion Weight Unit Expulsion Height Expulsion Height Unit PreHeating without Load PreHeating without Load Unit Start Start Unit Compacting Height Compacting Height Unit End expulsion height End expulsion height Unit Weigths istallated Weigths istallated Unit Type of Step Weights sequence Die Swell Step Die Swell Step Unit 
PLA_210_2.16 CEAST Lab. Melt Flow Modular TEMPLATE parameters set 25.10.2019 9:22:24 1  Manual 210.000 °C 0 1.000 g/cm³ 15 672 None CUSTOM  P P P 0 g GRANULAT Lot ABC CEAST 2.095 mm 8.000 mm 240 s 240 s 0 s 0 0 0.000 s Manual  0.000  2.000 cm³/10min 46.00 mm 0.00 s ---- N Type 0 (Solvay) ---- s Position ---- N CEAST Sample 0 0 ---- mm 0.000 kg 0.00 mm 240 s 46.00 mm 0.00 mm 0.00 mm   2.16/5/21.6 INCREASE 0.000 mm 

[Step parameters]
Load Load Unit Pressure Pressure Unit MFR-MVR Expected Title TYPE MFR-MVR Expected MFR-MVR Expected Unit Step lenght Step lenght Unit Step Time Step Time Unit Interval Len Interval Len Unit IntervalTime IntervalTime Unit Number of measures Measure Measure Unit Step Step Unit Density Density Unit 
2.160 kg 0.000 Pa MVR 1.000 cm³/10min 30.000 mm 0.000 s 0.750 mm 0.000 s 40 30.00 mm 0 [Number] 0.000 g/cm³ 

[Shared data]
Test name Instrument Name Reference Specimen weight Specimen weight Unit Density Density Unit Test date Operator name Comment Reference Elab. Code Fix Value Percent Value Tollerance Discard Type Discard Value Number of steps Last Modified 
PLA-filament-2 MFT 0 0.000 g 1.000 g/cm³ 23.6.2020 14:02:03 MC  0 0 0 2.000 Manual 0.000 0  

[Step data]
Number Of Received Measures Number Of Valid Measures Total Time Total Time Unit MFR Mean MFR Mean Unit MFR Std. Deviation MFR Std. Deviation Unit MFR Sigma MFR Sigma Unit MFR Variance MVR Mean MVR Mean Unit MVR Std. Deviation MVR Std. Deviation Unit MVR Sigma MVR Sigma Unit MVR Variance Shear Rate Shear Rate Unit Shear Stress Shear Stress Unit Viscosity Viscosity Unit Velocity Velocity Unit Swell Swell Unit Stability Stability Unit Start Len Start Len Unit Start Time Start Time Unit Start Temperature Start Temperature Unit 
40 40 52.594 s 24.464 g/10min 1.943 g/10min 1.943 g/10min 3.774 24.464 cm³/10min 1.943 cm³/10min 1.943 cm³/10min 3.774 44.899 1/s 19360.289 Pa 431.239 Pa*s 0.574 mm/s 0.000 % -10.844 %/min 46.010 mm 318.000 s 209.900 °C 
[Data Step n.: 1]
N. Time [s] Measure [mm] MFR [g/10min] MVR [cm³/10min] ShearRate [1/s] Viscosity [Pa*s]
   1: 1.48 0.76 21.766 21.766 40.187 481.759
   2: 1.28 0.73 24.409 24.409 45.066 429.598
   3: 1.26 0.76 25.734 25.734 47.512 407.479
   4: 1.27 0.76 25.351 25.351 46.804 413.643
   5: 1.32 0.74 23.794 23.794 43.930 440.709
   6: 1.40 0.76 23.151 23.151 42.743 452.950
   7: 1.28 0.74 24.557 24.557 45.339 427.010
   8: 1.27 0.76 25.518 25.518 47.113 410.937
   9: 1.33 0.74 23.594 23.594 43.560 444.448
  10: 1.51 0.76 21.462 21.462 39.625 488.594
  11: 1.36 0.76 23.825 23.825 43.988 440.126
  12: 1.17 0.74 26.920 26.920 49.701 389.532
  13: 1.17 0.76 27.688 27.688 51.119 378.728
  14: 1.31 0.74 23.931 23.931 44.183 438.181
  15: 1.16 0.76 27.926 27.926 51.559 375.497
  16: 1.15 0.74 27.497 27.497 50.768 381.351
  17: 1.21 0.76 26.943 26.943 49.743 389.204
  18: 1.16 0.74 27.189 27.189 50.198 385.677
  19: 1.13 0.76 28.806 28.806 53.183 364.031
  20: 1.25 0.74 25.210 25.210 46.544 415.959
  21: 1.31 0.76 24.823 24.823 45.829 422.444
  22: 1.23 0.74 25.661 25.661 47.378 408.638
  23: 1.27 0.76 25.666 25.666 47.386 408.567
  24: 1.21 0.74 26.000 26.000 48.003 403.314
  25: 1.27 0.76 25.504 25.504 47.088 411.149
  26: 1.29 0.74 24.301 24.301 44.866 431.517
  27: 1.40 0.76 23.113 23.113 42.672 453.698
  28: 1.37 0.74 22.920 22.920 42.317 457.508
  29: 1.33 0.76 24.435 24.435 45.114 429.139
  30: 1.27 0.74 24.838 24.838 45.857 422.187
  31: 1.31 0.76 24.696 24.696 45.595 424.615
  32: 1.39 0.74 22.658 22.658 41.833 462.800
  33: 1.44 0.76 22.505 22.505 41.551 465.944
  34: 1.46 0.74 21.555 21.555 39.796 486.491
  35: 1.44 0.76 22.554 22.554 41.641 464.938
  36: 1.39 0.76 23.368 23.368 43.144 448.738
  37: 1.45 0.74 21.585 21.585 39.851 485.815
  38: 1.45 0.76 22.260 22.260 41.099 471.066
  39: 1.37 0.73 22.894 22.894 42.268 458.037
  40: 1.47 0.76 21.959 21.959 40.542 477.536

