
[Shared parameters]
Parameter Name Compiler Comment Date Melt Type Melt Type Unit Standard Name Temperature Temperature Unit Type Of Measure Density Density Unit Specimen Name Specimen Treatment Test Procedure Specimen Quantity Specimen Quantity Unit Specimen Format Specimen Lot Specimen Supplier Die Diameter Die Diameter Unit Die Length Die Length Unit PreHeating Total PreHeating Total Unit PreHeating Load PreHeating Load Unit Max Test Time Max Test Time Unit Cut Auto Cut Step Cut Time Cut Time Unit Discard Type Discard Type Unit Discard Value Discard Value Unit Tollerance Tollerance Unit Measure Start Measure Start Unit Compacting Time Compacting Time Unit Compacting Force Compacting Force Unit Cicle Select Wait Time Wait Time Unit Test Start Expulsion Force Expulsion Force Unit Specimen Note Number of steps Reference Resting Height Resting Height Unit Expulsion Weight Expulsion Weight Unit Expulsion Height Expulsion Height Unit PreHeating without Load PreHeating without Load Unit Start Start Unit Compacting Height Compacting Height Unit End expulsion height End expulsion height Unit Weigths istallated Weigths istallated Unit Type of Step Weights sequence Die Swell Step Die Swell Step Unit 
PLA_210_2.16 CEAST Lab. Melt Flow Modular TEMPLATE parameters set 25.10.2019 9:22:24 1  Manual 210.000 °C 0 1.000 g/cm³ 15 672 None CUSTOM  P P P 0 g GRANULAT Lot ABC CEAST 2.095 mm 8.000 mm 240 s 240 s 0 s 0 0 0.000 s Manual  0.000  2.000 cm³/10min 46.00 mm 0.00 s ---- N Type 0 (Solvay) ---- s Position ---- N CEAST Sample 0 0 ---- mm 0.000 kg 0.00 mm 240 s 46.00 mm 0.00 mm 0.00 mm   2.16/5/21.6 INCREASE 0.000 mm 

[Step parameters]
Load Load Unit Pressure Pressure Unit MFR-MVR Expected Title TYPE MFR-MVR Expected MFR-MVR Expected Unit Step lenght Step lenght Unit Step Time Step Time Unit Interval Len Interval Len Unit IntervalTime IntervalTime Unit Number of measures Measure Measure Unit Step Step Unit Density Density Unit 
2.160 kg 0.000 Pa MVR 1.000 cm³/10min 30.000 mm 0.000 s 0.750 mm 0.000 s 40 30.00 mm 0 [Number] 0.000 g/cm³ 

[Shared data]
Test name Instrument Name Reference Specimen weight Specimen weight Unit Density Density Unit Test date Operator name Comment Reference Elab. Code Fix Value Percent Value Tollerance Discard Type Discard Value Number of steps Last Modified 
PLA-drt-1 MFT 0 0.000 g 1.000 g/cm³ 23.6.2020 15:39:10 MC  0 0 0 2.000 Manual 0.000 0  

[Step data]
Number Of Received Measures Number Of Valid Measures Total Time Total Time Unit MFR Mean MFR Mean Unit MFR Std. Deviation MFR Std. Deviation Unit MFR Sigma MFR Sigma Unit MFR Variance MVR Mean MVR Mean Unit MVR Std. Deviation MVR Std. Deviation Unit MVR Sigma MVR Sigma Unit MVR Variance Shear Rate Shear Rate Unit Shear Stress Shear Stress Unit Viscosity Viscosity Unit Velocity Velocity Unit Swell Swell Unit Stability Stability Unit Start Len Start Len Unit Start Time Start Time Unit Start Temperature Start Temperature Unit 
40 40 9.560 s 512.896 g/10min 742.641 g/10min 742.641 g/10min 551516.375 512.896 cm³/10min 742.641 cm³/10min 742.641 cm³/10min 551516.375 247.020 1/s 19360.289 Pa 78.379 Pa*s 12.028 mm/s 0.000 % -832.457 %/min 45.920 mm 250.000 s 209.900 °C 
[Data Step n.: 1]
N. Time [s] Measure [mm] MFR [g/10min] MVR [cm³/10min] ShearRate [1/s] Viscosity [Pa*s]
   1: 0.02 0.78 1956.483 1956.483 3612.209 5.360
   2: 0.02 0.73 1958.835 1958.835 3616.551 5.353
   3: 0.02 0.76 1901.300 1901.300 3510.327 5.515
   4: 0.02 0.73 1958.835 1958.835 3616.551 5.353
   5: 0.02 0.74 1961.500 1961.500 3621.472 5.346
   6: 0.02 0.76 1903.809 1903.809 3514.958 5.508
   7: 0.02 0.76 1906.317 1906.317 3519.589 5.501
   8: 0.02 0.74 1745.924 1745.924 3223.460 6.006
   9: 0.02 0.74 1366.376 1366.376 2522.707 7.674
  10: 0.04 0.76 753.660 753.660 1391.465 13.914
  11: 0.19 0.76 169.011 169.011 312.040 62.044
  12: 0.28 0.74 110.419 110.419 203.863 94.967
  13: 0.31 0.76 103.674 103.674 191.411 101.145
  14: 0.31 0.74 100.221 100.221 185.035 104.630
  15: 0.33 0.76 99.540 99.540 183.778 105.346
  16: 0.32 0.74 98.475 98.475 181.812 106.485
  17: 0.33 0.76 98.165 98.165 181.240 106.821
  18: 0.32 0.74 98.475 98.475 181.812 106.485
  19: 0.33 0.76 99.671 99.671 184.020 105.208
  20: 0.31 0.74 102.980 102.980 190.130 101.827
  21: 0.33 0.76 98.165 98.165 181.240 106.821
  22: 0.32 0.74 98.783 98.783 182.382 106.153
  23: 0.33 0.76 99.977 99.977 184.586 104.885
  24: 0.32 0.74 99.094 99.094 182.955 105.820
  25: 0.33 0.76 99.366 99.366 183.457 105.530
  26: 0.32 0.74 99.586 99.586 183.864 105.297
  27: 0.32 0.76 100.776 100.776 186.061 104.053
  28: 0.31 0.74 100.863 100.863 186.221 103.964
  29: 0.32 0.76 101.090 101.090 186.641 103.730
  30: 0.31 0.74 101.514 101.514 187.423 103.298
  31: 0.32 0.76 102.044 102.044 188.402 102.761
  32: 0.31 0.74 101.704 101.704 187.774 103.104
  33: 0.32 0.76 102.232 102.232 188.748 102.572
  34: 0.31 0.74 102.035 102.035 188.384 102.770
  35: 0.32 0.76 102.097 102.097 188.499 102.707
  36: 0.32 0.76 102.420 102.420 189.096 102.383
  37: 0.31 0.74 102.562 102.562 189.358 102.242
  38: 0.31 0.76 102.937 102.937 190.050 101.870
  39: 0.30 0.73 102.759 102.759 189.721 102.046
  40: 0.32 0.76 102.150 102.150 188.598 102.654

