
[Shared parameters]
Parameter Name Compiler Comment Date Melt Type Melt Type Unit Standard Name Temperature Temperature Unit Type Of Measure Density Density Unit Specimen Name Specimen Treatment Test Procedure Specimen Quantity Specimen Quantity Unit Specimen Format Specimen Lot Specimen Supplier Die Diameter Die Diameter Unit Die Length Die Length Unit PreHeating Total PreHeating Total Unit PreHeating Load PreHeating Load Unit Max Test Time Max Test Time Unit Cut Auto Cut Step Cut Time Cut Time Unit Discard Type Discard Type Unit Discard Value Discard Value Unit Tollerance Tollerance Unit Measure Start Measure Start Unit Compacting Time Compacting Time Unit Compacting Force Compacting Force Unit Cicle Select Wait Time Wait Time Unit Test Start Expulsion Force Expulsion Force Unit Specimen Note Number of steps Reference Resting Height Resting Height Unit Expulsion Weight Expulsion Weight Unit Expulsion Height Expulsion Height Unit PreHeating without Load PreHeating without Load Unit Start Start Unit Compacting Height Compacting Height Unit End expulsion height End expulsion height Unit Weigths istallated Weigths istallated Unit Type of Step Weights sequence Die Swell Step Die Swell Step Unit 
PLA_210_2.16 CEAST Lab. Melt Flow Modular TEMPLATE parameters set 25.10.2019 9:22:24 1  Manual 210.000 °C 0 1.000 g/cm³ 15 672 None CUSTOM  P P P 0 g GRANULAT Lot ABC CEAST 2.095 mm 8.000 mm 240 s 240 s 0 s 0 0 0.000 s Manual  0.000  2.000 cm³/10min 46.00 mm 0.00 s ---- N Type 0 (Solvay) ---- s Position ---- N CEAST Sample 0 0 ---- mm 0.000 kg 0.00 mm 240 s 46.00 mm 0.00 mm 0.00 mm   2.16/5/21.6 INCREASE 0.000 mm 

[Step parameters]
Load Load Unit Pressure Pressure Unit MFR-MVR Expected Title TYPE MFR-MVR Expected MFR-MVR Expected Unit Step lenght Step lenght Unit Step Time Step Time Unit Interval Len Interval Len Unit IntervalTime IntervalTime Unit Number of measures Measure Measure Unit Step Step Unit Density Density Unit 
2.160 kg 0.000 Pa MVR 1.000 cm³/10min 30.000 mm 0.000 s 0.750 mm 0.000 s 40 30.00 mm 0 [Number] 0.000 g/cm³ 

[Shared data]
Test name Instrument Name Reference Specimen weight Specimen weight Unit Density Density Unit Test date Operator name Comment Reference Elab. Code Fix Value Percent Value Tollerance Discard Type Discard Value Number of steps Last Modified 
PLA-filament-1 MFT 0 0.000 g 1.000 g/cm³ 23.6.2020 12:32:10 MC  0 0 0 2.000 Manual 0.000 0  

[Step data]
Number Of Received Measures Number Of Valid Measures Total Time Total Time Unit MFR Mean MFR Mean Unit MFR Std. Deviation MFR Std. Deviation Unit MFR Sigma MFR Sigma Unit MFR Variance MVR Mean MVR Mean Unit MVR Std. Deviation MVR Std. Deviation Unit MVR Sigma MVR Sigma Unit MVR Variance Shear Rate Shear Rate Unit Shear Stress Shear Stress Unit Viscosity Viscosity Unit Velocity Velocity Unit Swell Swell Unit Stability Stability Unit Start Len Start Len Unit Start Time Start Time Unit Start Temperature Start Temperature Unit 
40 40 41.268 s 31.047 g/10min 1.300 g/10min 1.300 g/10min 1.691 31.047 cm³/10min 1.300 cm³/10min 1.300 cm³/10min 1.691 57.222 1/s 19360.289 Pa 338.332 Pa*s 0.728 mm/s 0.000 % 22.408 %/min 46.010 mm 298.000 s 210.000 °C 
[Data Step n.: 1]
N. Time [s] Measure [mm] MFR [g/10min] MVR [cm³/10min] ShearRate [1/s] Viscosity [Pa*s]
   1: 1.11 0.76 29.133 29.133 53.788 359.939
   2: 1.08 0.73 29.047 29.047 53.628 361.010
   3: 1.11 0.76 29.093 29.093 53.713 360.437
   4: 1.11 0.76 29.251 29.251 54.005 358.491
   5: 1.07 0.74 29.358 29.358 54.204 357.178
   6: 1.11 0.76 29.263 29.263 54.027 358.342
   7: 1.06 0.74 29.496 29.496 54.458 355.507
   8: 1.09 0.76 29.786 29.786 54.994 352.046
   9: 1.05 0.74 29.930 29.930 55.259 350.353
  10: 1.08 0.76 29.951 29.951 55.299 350.105
  11: 1.08 0.76 30.130 30.130 55.628 348.029
  12: 1.04 0.74 30.201 30.201 55.759 347.213
  13: 1.08 0.76 30.130 30.130 55.628 348.029
  14: 1.04 0.74 30.172 30.172 55.706 347.546
  15: 1.07 0.76 30.384 30.384 56.097 345.121
  16: 1.04 0.74 30.300 30.300 55.942 346.078
  17: 1.06 0.76 30.510 30.510 56.329 343.700
  18: 1.03 0.74 30.505 30.505 56.321 343.748
  19: 1.06 0.76 30.740 30.740 56.755 341.118
  20: 1.03 0.74 30.654 30.654 56.595 342.084
  21: 1.05 0.76 31.064 31.064 57.352 337.568
  22: 1.00 0.74 31.418 31.418 58.006 333.765
  23: 1.03 0.76 31.455 31.455 58.074 333.373
  24: 0.99 0.74 31.702 31.702 58.531 330.770
  25: 1.03 0.76 31.669 31.669 58.470 331.114
  26: 0.99 0.74 31.691 31.691 58.511 330.885
  27: 1.02 0.76 31.751 31.751 58.622 330.256
  28: 0.99 0.74 31.819 31.819 58.747 329.552
  29: 1.02 0.76 31.908 31.908 58.910 328.640
  30: 0.98 0.74 32.144 32.144 59.347 326.220
  31: 1.00 0.76 32.289 32.289 59.614 324.763
  32: 0.97 0.74 32.466 32.466 59.940 322.993
  33: 1.01 0.76 32.214 32.214 59.476 325.513
  34: 0.96 0.74 32.600 32.600 60.189 321.658
  35: 0.99 0.76 32.626 32.626 60.236 321.406
  36: 0.99 0.76 32.659 32.659 60.297 321.082
  37: 0.95 0.74 32.863 32.863 60.674 319.088
  38: 0.98 0.76 33.049 33.049 61.018 317.288
  39: 0.94 0.73 33.236 33.236 61.362 315.507
  40: 0.97 0.76 33.209 33.209 61.314 315.758

