
[Shared parameters]
Parameter Name Compiler Comment Date Melt Type Melt Type Unit Standard Name Temperature Temperature Unit Type Of Measure Density Density Unit Specimen Name Specimen Treatment Test Procedure Specimen Quantity Specimen Quantity Unit Specimen Format Specimen Lot Specimen Supplier Die Diameter Die Diameter Unit Die Length Die Length Unit PreHeating Total PreHeating Total Unit PreHeating Load PreHeating Load Unit Max Test Time Max Test Time Unit Cut Auto Cut Step Cut Time Cut Time Unit Discard Type Discard Type Unit Discard Value Discard Value Unit Tollerance Tollerance Unit Measure Start Measure Start Unit Compacting Time Compacting Time Unit Compacting Force Compacting Force Unit Cicle Select Wait Time Wait Time Unit Test Start Expulsion Force Expulsion Force Unit Specimen Note Number of steps Reference Resting Height Resting Height Unit Expulsion Weight Expulsion Weight Unit Expulsion Height Expulsion Height Unit PreHeating without Load PreHeating without Load Unit Start Start Unit Compacting Height Compacting Height Unit End expulsion height End expulsion height Unit Weigths istallated Weigths istallated Unit Type of Step Weights sequence Die Swell Step Die Swell Step Unit 
PLA_210_2.16 CEAST Lab. Melt Flow Modular TEMPLATE parameters set 25.10.2019 9:22:24 1  Manual 210.000 °C 0 1.000 g/cm³ 15 672 None CUSTOM  P P P 0 g GRANULAT Lot ABC CEAST 2.095 mm 8.000 mm 240 s 240 s 0 s 0 0 0.000 s Manual  0.000  2.000 cm³/10min 46.00 mm 0.00 s ---- N Type 0 (Solvay) ---- s Position ---- N CEAST Sample 0 0 ---- mm 0.000 kg 0.00 mm 240 s 46.00 mm 0.00 mm 0.00 mm   2.16/5/21.6 INCREASE 0.000 mm 

[Step parameters]
Load Load Unit Pressure Pressure Unit MFR-MVR Expected Title TYPE MFR-MVR Expected MFR-MVR Expected Unit Step lenght Step lenght Unit Step Time Step Time Unit Interval Len Interval Len Unit IntervalTime IntervalTime Unit Number of measures Measure Measure Unit Step Step Unit Density Density Unit 
2.160 kg 0.000 Pa MVR 1.000 cm³/10min 30.000 mm 0.000 s 0.750 mm 0.000 s 40 30.00 mm 0 [Number] 0.000 g/cm³ 

[Shared data]
Test name Instrument Name Reference Specimen weight Specimen weight Unit Density Density Unit Test date Operator name Comment Reference Elab. Code Fix Value Percent Value Tollerance Discard Type Discard Value Number of steps Last Modified 
PLA-drt-2 MFT 0 0.000 g 1.000 g/cm³ 23.6.2020 15:18:47 MC  0 0 0 2.000 Manual 0.000 0  

[Step data]
Number Of Received Measures Number Of Valid Measures Total Time Total Time Unit MFR Mean MFR Mean Unit MFR Std. Deviation MFR Std. Deviation Unit MFR Sigma MFR Sigma Unit MFR Variance MVR Mean MVR Mean Unit MVR Std. Deviation MVR Std. Deviation Unit MVR Sigma MVR Sigma Unit MVR Variance Shear Rate Shear Rate Unit Shear Stress Shear Stress Unit Viscosity Viscosity Unit Velocity Velocity Unit Swell Swell Unit Stability Stability Unit Start Len Start Len Unit Start Time Start Time Unit Start Temperature Start Temperature Unit 
40 40 33.473 s 38.948 g/10min 7.518 g/10min 7.518 g/10min 56.520 38.948 cm³/10min 7.518 cm³/10min 7.518 cm³/10min 56.520 70.547 1/s 19360.289 Pa 274.380 Pa*s 0.913 mm/s 0.000 % -25.896 %/min 46.010 mm 252.000 s 210.000 °C 
[Data Step n.: 1]
N. Time [s] Measure [mm] MFR [g/10min] MVR [cm³/10min] ShearRate [1/s] Viscosity [Pa*s]
   1: 0.63 0.76 51.482 51.482 95.051 203.684
   2: 0.76 0.73 41.402 41.402 76.440 253.275
   3: 0.85 0.76 38.071 38.071 70.289 275.438
   4: 0.86 0.76 37.367 37.367 68.989 280.628
   5: 0.85 0.74 36.922 36.922 68.169 284.005
   6: 0.88 0.76 36.862 36.862 68.057 284.471
   7: 0.83 0.74 37.812 37.812 69.811 277.322
   8: 0.78 0.76 41.655 41.655 76.906 251.739
   9: 0.38 0.74 82.702 82.702 152.690 126.795
  10: 0.87 0.76 37.207 37.207 68.695 281.831
  11: 0.89 0.76 36.502 36.502 67.392 287.278
  12: 0.86 0.74 36.720 36.720 67.796 285.568
  13: 0.89 0.76 36.543 36.543 67.468 286.954
  14: 0.86 0.74 36.423 36.423 67.247 287.900
  15: 0.84 0.76 38.402 38.402 70.901 273.059
  16: 0.87 0.74 36.262 36.262 66.950 289.174
  17: 0.90 0.76 36.305 36.305 67.028 288.837
  18: 0.87 0.74 36.262 36.262 66.950 289.174
  19: 0.89 0.76 36.468 36.468 67.329 287.546
  20: 0.86 0.74 36.557 36.557 67.494 286.845
  21: 0.89 0.76 36.673 36.673 67.709 285.932
  22: 0.86 0.74 36.813 36.813 67.967 284.848
  23: 0.88 0.76 36.923 36.923 68.171 283.996
  24: 0.85 0.74 37.029 37.029 68.366 283.185
  25: 0.88 0.76 37.008 37.008 68.326 283.351
  26: 0.85 0.74 37.110 37.110 68.515 282.569
  27: 0.87 0.76 37.171 37.171 68.627 282.107
  28: 0.84 0.74 37.286 37.286 68.840 281.236
  29: 0.87 0.76 37.342 37.342 68.943 280.815
  30: 0.84 0.74 37.419 37.419 69.086 280.236
  31: 0.86 0.76 37.645 37.645 69.503 278.553
  32: 0.84 0.74 37.592 37.592 69.405 278.948
  33: 0.86 0.76 37.596 37.596 69.412 278.919
  34: 0.83 0.74 37.818 37.818 69.822 277.280
  35: 0.86 0.76 37.809 37.809 69.806 277.343
  36: 0.85 0.76 37.942 37.942 70.052 276.371
  37: 0.82 0.74 38.041 38.041 70.235 275.652
  38: 0.85 0.76 38.206 38.206 70.538 274.464
  39: 0.82 0.73 38.268 38.268 70.653 274.019
  40: 0.84 0.76 38.291 38.291 70.696 273.852

