ClarkInv
Inverse Clark's transformation
Library
GMCLIB
Description
Performs an Inverse Clark's transformation on to 2-phase input signal according to the following equations:
An assumption for correct function is zero sum of the output 3-phase signal. If this assumption is violated, the previous equations don't hold anymore.
Inputs and outputs
Inputs:
alpha, beta - 2-phase output signal in stationary frame
Outputs:
a,b,c - 3-phase input signal in stationary frame
See also
Clarke, ClarkeUnbalanced, ClarkeInvUnbalanced, Park, ParkInv,