Park
Park's transformation
Library
GMCLIB
Description
Performs a Park's transformation on to 2-phase input signal according to the following equations:
.
Inputs and outputs
Inputs:
alpha, beta - 2-phase input signal in stationary frame
theta - angle between alpha-axis and d-axis [rad] (e.g. electrical motor position)
Outputs:
d, q - 2-phase output signal in synchronous frame
See also
Clarke, ClarkeInv, ClarkeUnbalanced, ClarkeInvUnbalanced, ParkInv,