ADC
A/D converter
Library
GMCLIB
Description
Performs an A/D converter with user-defined resolution, input range and sampling period.
Parameters and dialog box
The ADC block dialog box appears as follows:
The block constrains the input signal to n-bit resolution. The entered range is divided into 2^n equal levels. The input is converted at the beginning of sampling period Ts and the output holds its value for the rest the period.
Inputs and outputs
Inputs:
in - input signal
Outputs:
out - output signal
See also
3PH ADC