Trigonometric function
Standard trigonometric functions + atanYX and atanYXshifted
Library
GFLIB
Description
Computes sin, cos, tan, asin, acos, atan, atanYX or atanYXshifted specified in the dialog box.
Parameters and dialog box
The Trigonometric function block dialog box appears as follows:
For calculation atanYX and atanYXshifted two input signals are required. For atanYXshifted shifting parameters have to be specified.
Inputs and outputs
Inputs:
inY = general input, for atanYX and atanYXshifted input Y
inX = avilable only for atanYX and atanYXshifted as input X
Outputs:
out - output signal