Ramp
Ramp (rate limiter) function
Library
GFLIB
Description
Limits the rising and falling slew rate
Parameters and dialog box
The Ramp block dialog box appears as follows:
Limits the maximum rising slew rate to Up/Ts per 1s and maximum falling slew rate to Down/Ts per 1s.
For input square wave with amplitude=10 the Ramp function output with the parameters 10,10,0.5 (Up, Down, Ts respectively) will be:
Inputs and outputs
Inputs:
in - input signal
Outputs:
out - output signal