SVMsci
Space Vector Modulation with Sine Cap Injection
Library
GMCLIB
Description
Computes an appropriate duty cycle (range 0 - 1) for each phase and current sector from the input alpha-beta voltage scaled in range -1 - 1. The calculation technique is called Space Vector Modulation with Sine Cap Injection and it's output course is on the following picture:
Inputs:
alpha, beta - 2 phase input voltage (range -1 - 1) [V]
Outputs:
a, b, c - duty cycle for each phase [-]
sector - actual sector number (1-6) [-]
See also
PWMict, SVMstd, SVMalt,