Partlist exported from C:/Users/Radek/OneDrive/school/FEKT/S6/_BP/_SP/HW/PCB/ROwen_Power.sch at 22.5.2016 0:40:14

Qty | Value | Device | Package | Parts | Description | MF | MPN | OC_FARNELL | OC_NEWARK
1 |  | C-EU050-055X075 | C050-055X075 | C2 | CAPACITOR, European symbol |  |  |  |
1 |  | CPOL-EUE3.5-10 | E3,5-10 | C1 | POLARIZED CAPACITOR, European symbol |  |  |  |
2 |  | D_10 | DO41 | D2, D3 | Dioda - univerzální |  |  |  |
1 | 100mA | SH22,5A | SH22,5A | F1 | FUSE HOLDER grid 22,5mm, isolated cap OGN0031 8201, Schurter (Buerklin) |  | 0031.7701.11 | unknown | 04F1224
1 | 10A | SH22,5A | SH22,5A | F2 | FUSE HOLDER grid 22,5mm, isolated cap OGN0031 8201, Schurter (Buerklin) |  | 0031.7701.11 | unknown | 04F1224
4 | 220 | R-EU_0207/10 | 0207/10 | R7, R8, R9, R12 | RESISTOR, European symbol |  |  |  |
4 | 330 | R-EU_0207/10 | 0207/10 | R4, R5, R6, R11 | RESISTOR, European symbol |  |  |  |
4 | 360 | R-EU_0207/10 | 0207/10 | R1, R2, R3, R10 | RESISTOR, European symbol |  |  |  |
1 | 39 | R-EU_0309/12 | 0309/12 | R13 | RESISTOR, European symbol |  |  |  |
4 | BTA16 | BTA16 | TO220 | T1, T2, T3, T4 |  |  |  |  |
1 | D-MUSTEK_B380C1000DIL | D-MUSTEK_B380C1000DIL | DM_DB1 | M1 | Diodovy mustek - Graetz |  |  |  |
1 | MLW14_90° | MLW14_90° | MLW14A | CON1 | Konektory MLW - vidlice - 14x |  |  |  |
4 | MOC3041M | MOC3041M | DIL06 | OK1, OK2, OK3, OK4 | 6-Pin DIP Zero-Cross Optoisolators Triac Driver Output (250/400 Volt Peak) | FAIRCHILD SEMICONDUCTOR | MOC3041M | 1086677 | 78K6090
1 | TRHEI304-1 | TRHEI304-1 | TRHEI304 | TR1 | Transformator - do DPS - 2,6 VA |  |  |  |
11 | WAGO256 | WAGO256 | WAGO256 | CON2, CON3, CON4, CON5, CON6, CON7, CON8, CON9, CON10, CON11, CON12 | Konektor WAGO - RM 5,08mm - s packou |  |  |  |