#### File: D:\bobes\0 skola\_car4\my matlab\HIL - PID speed\firmware\Vejlupek_Car4_HIL_PIDSpeed_dspic\sources\rt_SATURATE.h
        1   /*
        2    * File: rt_SATURATE.h
        3    *
        4    * Real-Time Workshop code generated for Simulink model Vejlupek_Car4_HIL_PIDSpeed.
        5    *
        6    * Model version                        : 1.460
        7    * Real-Time Workshop file version      : 7.3  (R2009a)  15-Jan-2009
        8    * Real-Time Workshop file generated on : Fri Apr 30 16:12:44 2010
        9    * TLC version                          : 7.3 (Jan 18 2009)
       10    * C source code generated on           : Fri Apr 30 16:12:44 2010
       11    *--------------------------------------------------------------
       12    *   Embedded Coder for Microchip dsPIC family.                 |
       13    *   Generate .c and .h files from your Matlab/simulink model   |
       14    *   and compile the diagram to .hex and .coff file that can be |
       15    *   downloaded directly into the microcontroller               |
       16    *                                                              |
       17    * Licence Accorded to Ing. Robert Grepl, Ph.D.                 |
       18    *                     Technical University Brno                |
       19    *                                                              |
       20    *   Written by Lubin KERHUEL -  http://www.kerhuel.eu          |
       21    *  - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - |
       22    *   Version 3.1                               26-Nov-2009      |
       23    *   For Matlab 7.8             R2009a                          |
       24    *--------------------------------------------------------------
       25    */
       26
       27   #ifndef RTW_HEADER_rt_SATURATE_h_
       28   #define RTW_HEADER_rt_SATURATE_h_
       29   #define rt_SATURATE(sig,ll,ul)         (((sig) >= (ul)) ? (ul) : (((sig) <= (ll)) ? (ll) : (sig)) )
       30   #endif                                 /* RTW_HEADER_rt_SATURATE_h_ */
       31
       32   /* File trailer for Real-Time Workshop generated code.
       33    *
       34    * [EOF]
       35    */